### Navigation

- index
- modules |
- modules |
- FNSS 0.6.1 documentation »
- Module code »

# Source code for fnss.adapters.omnetpp

    """Omnet++ adapter

    This module contains the code for converting an FNSS topology object into a NED
    script to deploy such topology into Omnet++.
    """
    from warnings import warn

    from fnss.units import time_units, capacity_units

    __all__ = ['to_omnetpp']

    # Template text rendered by the template engine
    __TEMPLATE = r"""// Code generated by Fast Network Simulator Setup (FNSS)
    <%
    import re
    from fnss.units import time_units, capacity_units
    from fnss.netconfig.nodeconfig import get_stack, \
                                          get_application_names, \
                                          get_application_properties

    # Convert capacity in Mb
    if set_capacities:
        capacity_norm = capacity_units[topology.graph['capacity_unit']] / 1000000.0
    # Convert delay it in ms
    if set_delays:
        delay_norm = time_units[topology.graph['delay_unit']]

    # Get topology name
    name = topology.name
    name = "net" if name == "" else re.sub("[^A-Za-z0-9]", "_", name).strip(" _")

    # Get numerical ID of a node
    nodes = topology.nodes()
    node_map = dict((nodes[i], i) for i in range(len(nodes)))

    %>
    // This is the module modelling the nodes of network
    module node {
        //TODO: Implement it
    }

    // Create network
    network ${name} {
        connections allowunconnected:
    % for u, v in topology.edges_iter():
        <%
        attr_str = ""
        if set_delays:
            delay = delay_norm * topology.edge[u][v]['delay']
            attr_str += " delay=%sms;" % (str(delay))
        if set_capacities:
            capacity = capacity_norm * topology.edge[u][v]['capacity']
            attr_str += " datarate=%sMbps;" % (str(capacity))
        %>
        ${"node[%s].ppg$o++ --> {%s} --> node[%s].pppg$i++;" % (str(node_map[u]), attr_str.strip(), str(node_map[v]))}
        % if not topology.is_directed():
        ${"node[%s].ppg$i++ <-- {%s} <-- node[%s].pppg$o++;" % (str(node_map[u]), attr_str.strip(), str(node_map[v]))}
        % endif
    % endfor
    }
    """

    def to_omnetpp(topology, path=None):
        """Convert an FNSS topology into an Omnet++ NED script.

        Parameters
        ----------
        topology : Topology
            The topology object to convert
        path : str, optional
            The path to the output NED file.
            If not specified, prints to standard output
        """
        try:
            from mako.template import Template
        except ImportError:
            raise ImportError('Cannot import mako.template module. '
                              'Make sure mako is installed on this machine.')
        set_delays = True
        set_capacities = True
        # Check correctness of capacity and delay attributes
        if not 'capacity_unit' in topology.graph or not topology.graph['capacity_unit'] in capacity_units:
            warn('Missing or invalid capacity unit attribute in the topology. The '
                 'output file will be generated without link capacity attributes.')
            set_capacities = False
        if not 'delay_unit' in topology.graph or not topology.graph['delay_unit'] in time_units:
            warn('Missing or invalid delay unit attribute in the topology. The '
                 'output file will be generated without link delay attributes.')
            set_delays = False
        template = Template(__TEMPLATE)
        variables = {
            'topology':        topology,
            'set_capacities':  set_capacities,
            'set_delays':      set_delays,
                    }
        ned = template.render(**variables)
        if path:
            with open(path, "w") as out:
                out.write(ned)
        else:
            print(ned)

### Navigation

- index
- modules |
- modules |
- FNSS 0.6.1 documentation »
- Module code »