### Navigation

- index
- modules |
- modules |
- FNSS 0.6.1 documentation »
- Module code »

# Source code for fnss.adapters.mn

    """Adapter for Mininet.

    This module contains function to convert FNSS topologies into Mininet
    topologies and viceversa.
    """
    import re

    import networkx as nx

    from fnss.units import capacity_units, time_units
    from fnss.topologies.topology import Topology
    from fnss.netconfig import set_delays_constant

    __all__ = [
        'from_mininet',
        'to_mininet',
               ]

    def from_mininet(topology):
        """Convert a Mininet topology to an FNSS one.

        Parameters
        ----------
        topology : Mininet Topo
            A Mininet topology object

        Returns
        -------
        topology : Topology
            An FNSS Topology object
        """
        fnss_topo = Topology(capacity_unit='Mbps')
        for v in topology.switches():
            fnss_topo.add_node(v, type='switch')
        for v in topology.hosts():
            fnss_topo.add_node(v, type='host')
        for u, v in topology.links():
            fnss_topo.add_edge(u, v)
            opts = topology.linkInfo(u, v)
            if 'bw' in opts:
                fnss_topo.edge[u][v]['capacity'] = opts['bw']
            if 'delay' in opts:
                delay = opts['delay']
                val = re.findall("\d+\.?\d*", delay)[0]
                unit = delay.strip(val).strip(' ')
                set_delays_constant(fnss_topo, val, unit, [(u,v)])
        return fnss_topo

    def to_mininet(topology, switches=None, hosts=None, relabel_nodes=True):
        """Convert an FNSS topology to Mininet Topo object that can be used to
        deploy a Mininet network.

        If the links of the topology are labeled with delays, capacities or buffer
        sizes, the returned Mininet topology will also include those parameters.

        However, it should be noticed that buffer sizes are included in the
        converted topology only if they are expressed in packets. If buffer sizes
        are expressed in the form of bytes they will be discarded. This is because
        Mininet only supports buffer sizes expressed in packets.

        Parameters
        ----------
        topology : Topology, DirectedTopology or DatacenterTopology
            An FNSS Topology object
        switches : list, optional
            List of topology nodes acting as switches
        hosts : list, optional
            List of topology nodes acting as hosts
        relabel_nodes : bool, optional
            If *True*, rename node labels according to `Mininet conventions
            <https://github.com/mininet/mininet/wiki/Introduction-to-Mininet#naming-in-mininet>`_.
            In Mininet all node labels are strings whose values are "h1", "h2", ...
            if the node is a host or "s1", "s2", ... if the node is a switch.

        Returns
        -------
        topology : Mininet Topo
            A Mininet topology object

        Notes
        -----
        It is not necessary to provide a list of switch and host nodes if the
        topology object provided are already annotated with a type attribute that
        can have values *host* or *switch*. This is the case of datacenter
        topologies generated with FNSS which already include information about
        which nodes are hosts and which are switches.

        If switches and hosts are passed as arguments, then the hosts and switches
        sets must be disjoint and their union must coincide to the set of all
        topology nodes. In other words, there cannot be nodes labeled as both
        *host* and *switch* and there cannot be nodes that are neither a *host* nor
        a *switch*.

        It is important to point out that if the topology contains loops, it will
        not work with the *ovs-controller* and *controller* provided by Mininet. It
        will be necessary to use custom controllers. Further info `here
        <https://github.com/mininet/mininet/wiki/Introduction-to-Mininet#multipath-routing>`_.
        """
        try:
            from mininet.topo import Topo
        except ImportError:
            raise ImportError('Cannot import mininet.topo package. '
                              'Make sure Mininet is installed on this machine.')
        if hosts is None:
            hosts = (v for v in topology.nodes_iter()
                     if 'host' in topology.node[v]['type'])
        if switches is None:
            switches = (v for v in topology.nodes_iter()
                        if 'switch' in topology.node[v]['type'])
        nodes = set(topology.nodes_iter())
        switches = set(switches)
        hosts = set(hosts)
        if not switches.isdisjoint(hosts):
            raise ValueError('Some nodes are labeled as both host and switch. '
                             'Switches and hosts node lists must be disjoint')
        if nodes != switches.union(hosts):
            raise ValueError('Some nodes are not labeled as either host or switch '
                             'or some nodes listed as switches or hosts do not '
                             'belong to the topology')
        if relabel_nodes:
            hosts = sorted(hosts)
            switches = sorted(switches)
            mapping = dict([(hosts[i], "h%s" % str(i+1)) for i in range(len(hosts))] +
                           [(switches[i], "s%s" % str(i+1)) for i in range(len(switches))])
            hosts = set(mapping[v] for v in hosts)
            switches = set(mapping[v] for v in switches)
            nodes = hosts.union(switches)
            topology = nx.relabel_nodes(topology, mapping, copy=True)
        topo = Topo()
        for v in switches:
            topo.addSwitch(str(v))
        for v in hosts:
            topo.addHost(str(v))
        delay_unit = topology.graph['delay_unit'] \
                     if 'delay_unit' in topology.graph else None
        capacity_unit = topology.graph['capacity_unit'] \
                        if 'capacity_unit' in topology.graph else None
        buffer_unit = topology.graph['buffer_unit'] \
                      if 'buffer_unit' in topology.graph else None
        if capacity_unit:
            capacity_conversion = float(capacity_units[capacity_unit]) \
                                  / capacity_units['Mbps']
        if delay_unit:
            delay_conversion = float(time_units[delay_unit]) \
                                  / time_units['us']
        for u, v in topology.edges_iter():
            params = {}
            if 'capacity' in topology.edge[u][v] and capacity_unit:
                params['bw'] = topology.edge[u][v]['capacity'] * capacity_conversion
                # Use Token Bucket filter to implement rate limit
                params['use_htb'] = True
            if 'delay' in topology.edge[u][v] and delay_unit:
                params['delay'] = '%sus' % str(topology.edge[u][v]['delay']
                                               * delay_conversion)
            if 'buffer_size' in topology.edge[u][v] and buffer_unit == 'packets':
                params['max_queue_size'] = topology.edge[u][v]['buffer_size']
            topo.addLink(str(u), str(v), **params)
        return topo

### Navigation

- index
- modules |
- modules |
- FNSS 0.6.1 documentation »
- Module code »