# Source code for psychopy_ext.models

    #!/usr/bin/env python

    # Part of the psychopy_ext library
    # Copyright 2010-2013 Jonas Kubilius
    # The program is distributed under the terms of the GNU General Public License,
    # either version 3 of the License, or (at your option) any later version.

    """
    A library of simple models of vision

    Simple usage::

        import glob
        from psychopy_ext import models
        ims = glob.glob('Example_set/*.jpg')  # get all jpg images
        hmax = models.HMAX()
        # if you want to see how similar your images are to each other
        hmax.compare(ims)
        # or to simply get the output and use it further
        out = hmax.run(ims)
    """

    import sys
    import itertools
    import cPickle as pickle

    import numpy as np
    import matplotlib.pyplot as plt
    from mpl_toolkits.axes_grid1 import make_axes_locatable
    import scipy.misc
    import scipy.ndimage

    class Model(object):

        def get_teststim(self, size=(256, 256)):
            """
            Opens Lena image and resizes it to the specified size ((256, 256) by
            default)
            """
            lena = scipy.misc.lena()
            im = scipy.misc.imresize(lena, (256, 256))
            im = im.astype(float)

            return im

        def train(self, im):
            """
            A placeholder for a function for training a model.
            If the model is not trainable, then it will default to this function
            here that does nothing.
            """
            pass

        def test(self, im):
            """
            A placeholder for a function for testing a model.
            """
            pass

        def dissimilarity(self, outputs, kind='simple'):
            if kind == 'simple':
                dis = self._dis_simple(outputs)
            elif kind == 'gaborjet':
                dis = self._dis_gj_simple(outputs)
            elif kind == 'gaborjet-fast':
                dis = self._dis_gj_fast(outputs)
            elif kind == 'corr':
                #self._dis_corr(outputs)
                raise NotImplemented
            else:
                raise ValueError('Dissimilarity of %s not recognized' % kind)
            return dis

        def _dis_simple(self, outputs):
            # used in Grill-Spector et al. (1999), Op de Beeck et al. (2001),
            # Panis et al. (2011)
            outputs = np.array(outputs)
            dis = np.zeros((outputs.shape[0],outputs.shape[0]))
            for (i,j), value in np.ndenumerate(dis):
                dis[i,j] = np.sqrt(np.sum((outputs[i] - outputs[j])**2) / outputs.shape[1])
            return dis

        def _dis_gj_simple(self, outputs):
            """
            Calculate similarity between magnitudes of gabor jet.

            It may look complex but this is just a linear algebra implementation of
            1 - np.dot(f,g) / (np.sqrt(np.dot(g,g)) * np.sqrt(np.dot(f,f)) )
            """
            outputs = np.array(outputs)
            if outputs.ndim != 2:
                raise Exception('ERROR: 2 dimensions expected')
            length = np.sqrt(np.sum(outputs*outputs, axis=1))
            length = np.tile(length, (len(length), 1))  # make a square matrix
            return 1 - np.dot(outputs,outputs.T) / (length * length.T)

        def _dis_corr(self, outputs):
            """
            Calculate a correlation between magnitudes of gabor jet.

            DOESN'T WORK YET
            """
            outputs = np.array(outputs)
            outputs -= np.tile(np.mean(outputs, axis=1), (outputs.shape[1],1)).T
            if outputs.ndim != 2:
                sys.exit('ERROR: 2 dimensions expected')
            length = np.sqrt(np.sum(outputs*outputs, axis=1))
            length = np.tile(length, (len(length), 1))  # make a square matrix
            return .5 - np.dot(outputs,outputs.T) / (2 * length * length.T)

        def _dis_corr2(self, outputs):
            """
            Calculate a correlation between magnitudes of gabor jet.

            DOESN'T WORK YET
            """
            outputs = np.array(outputs)
            import pdb; pdb.set_trace()
            outputs -= np.tile(np.mean(outputs, axis=0), (outputs.shape[0],1))
            if outputs.ndim != 2:
                sys.exit('ERROR: 2 dimensions expected')
            length = np.sqrt(np.sum(outputs*outputs, axis=1))
            length = np.tile(length, (len(length), 1))  # make a square matrix
            return 1 - np.dot(outputs,outputs.T) / (2 * length * length.T)

        def _dis_fast(self, outputs):
            outputs = np.array(outputs)
            if outputs.ndim != 2:
                sys.exit('ERROR: 2 dimensions expected')
            def sq(c):
                return np.dot(c,c)
            def func(row):
                # difference between tuning and each C2 response
                diff = outputs - \
                        np.tile(row,(outputs.shape[0],1))
                # import pdb; pdb.set_trace()
                # this difference is then square-summed and then exponentiated :)
                return np.apply_along_axis(sq,1,diff)
            return np.apply_along_axis(func, 1, outputs)

        def input2array(self, names):
            try:
                names = eval(names)
            except:
                pass

            if type(names) == str:
                array = scipy.misc.imread(names, flatten=True)
                array = self._prepare_im(array)
            elif type(names) in [list, tuple]:
                if type(names[0]) == str:
                    arr = []
                    for n in names:
                        im = scipy.misc.imread(n, flatten=True)
                        im = self._prepare_im(im)
                        arr.append(im)
                    array = np.array(arr)
                else:
                    array = np.array(names)
            elif type(names) == np.ndarray:
                array = names
            else:
                raise ValueError('input type not recognized')
            if array.ndim == 2:
                array = np.reshape(array, (1,) + array.shape)
            array = array.astype(float)
            return array

        def _prepare_im(self, im):
            large = np.max(im.shape)
            if large > 256:
                im = scipy.misc.imresize(im, 256./large)
            return im

        def compare(self, ims):
            print ims
            print 'processing image',
            output = self.run(ims, oneval=True)
            dis = self.dissimilarity(output)
            print
            print 'Dissimilarity across stimuli'
            print '0: similar, 1: dissimilar'
            print dis

            ax = plt.subplot(111)
            matrix = ax.imshow(dis, interpolation='none')
            plt.title('Dissimilarity across stimuli\n'
                      '(blue: similar, red: dissimilar)')
            divider = make_axes_locatable(ax)
            cax = divider.append_axes("right", size="5%", pad=0.05)
            plt.colorbar(matrix, cax=cax)
            plt.show()

    class Pixelwise(Model):
        def run(self, test_ims, **kwargs):
            ims = self.input2array(test_ims)
            if ims.ndim != 3:
                sys.exit('ERROR: Input images must be two-dimensional')
            return ims.reshape((ims.shape[0], -1))

    class Zoccolan(Model):
        """
        Based on 10.1073/pnas.0811583106
        """
        def __init__(self):
            # receptive field sizes in degrees
            #self.rfs = np.array([.6,.8,1.])
            #self.rfs = np.array([.2,.35,.5])
            self.rfs = [10, 20, 30]  # deg visual angle
            self.oris = np.linspace(0, np.pi, 12)
            self.phases = [0, np.pi]
            self.sfs = range(1, 11)  # cycles per RF size
            self.winsize = [5, 5]  # size of each patch on the grid
            # window size will be fixed in pixels and we'll adjust degrees accordingly
            # self.win_size_px = 300

        def get_gabors(self, rf):
            lams =  float(rf[0])/self.sfs # lambda = 1./sf  #1./np.array([.1,.25,.4])
            sigma = rf[0]/2./np.pi
            # rf = [100,100]
            gabors = np.zeros(( len(oris),len(phases),len(lams), rf[0], rf[1] ))

            i = np.arange(-rf[0]/2+1,rf[0]/2+1)
            #print i
            j = np.arange(-rf[1]/2+1,rf[1]/2+1)
            ii,jj = np.meshgrid(i,j)
            for o, theta in enumerate(self.oris):
                x = ii*np.cos(theta) + jj*np.sin(theta)
                y = -ii*np.sin(theta) + jj*np.cos(theta)

                for p, phase in enumerate(self.phases):
                    for s, lam in enumerate(lams):
                        fxx = np.cos(2*np.pi*x/lam + phase) * np.exp(-(x**2+y**2)/(2*sigma**2))
                        fxx -= np.mean(fxx)
                        fxx /= np.linalg.norm(fxx)

                        #if p==0:
                            #plt.subplot(len(oris),len(lams),count+1)
                            #plt.imshow(fxx,cmap=mpl.cm.gray,interpolation='bicubic')
                            #count+=1

                        gabors[o,p,s,:,:] = fxx
            plt.show()
            return gabors

        def run(self, ims):
            ims = self.input2array(ims)
            output = [self.test(im) for im in ims]

        def test(self, im):
            field = im.shape
            num_tiles = (15,15)#[field[0]/10.,field[0]/10.]
            size = (field[0]/num_tiles[0], field[0]/num_tiles[0])

            V1 = []#np.zeros( gabors.shape + num_tiles )

        #    tiled_im = im.reshape((num_tiles[0],size[0],num_tiles[1],size[1]))
        #    tiled_im = np.rollaxis(tiled_im, 1, start=3)
        #    flat_im = im.reshape((num_tiles[0],num_tiles[1],-1))

            for r, rf in enumerate(self.rfs):

                def apply_filter(window, this_filter):
                    this_resp = np.dot(this_filter,window)/np.linalg.norm(this_filter)
        #            import pdb; pdb.set_trace()
                    return np.max((0,this_resp)) # returns at least zero

                def filter_bank(this_filter,rf):
                    #print 'done0'
                    resp = scipy.ndimage.filters.generic_filter(
                                    im, apply_filter, size=rf,mode='nearest',
                                    extra_arguments = (this_filter,))
        #            import pdb; pdb.set_trace()
                    #print 'done1'
                    ii,jj = np.meshgrid(np.arange(0,field[0],size[0]),
                                            np.arange(0,field[1],size[1]) )
                    selresp = resp[jj,ii]

        #            maxresp = scipy.ndimage.filters.maximum_filter(
        #                resp,
        #                size = size,
        #                mode = 'nearest'
        #            )
                    return np.ravel(selresp)

                gabors = self.get_gabors(rf)
                #import pdb; pdb.set_trace()
                gabors = gabors.reshape(gabors.shape[:3]+(-1,))
        #        gabors_norms = np.apply_along_axis(np.linalg.norm, -1, gabors)
        #        import pdb; pdb.set_trace()
        #        V1.append( np.apply_along_axis(filter_bank, -1, gabors,rf) )
                V1resp = np.zeros(gabors.shape[:-1]+num_tiles)
        #        import pdb; pdb.set_trace()
                for i,wi in enumerate(np.arange(0,field[0]-rf[0],size[0])):
                    for j,wj in enumerate(np.arange(0,field[1]-rf[1],size[1])):
                        window = im[wi:wi+rf[0],wj:wj+rf[1]]
                        resp = np.inner(gabors,np.ravel(window))
                        resp[resp<0] = 0
                        V1resp[:,:,:,i,j] = resp #/gabors_norms
        #                print 'done'
                V1.append(V1resp)
            return [V1]

    class GaborJet(Model):

        def __init__(self, nScale=5, nOrientation=8):
            """
            Python implementation of the Gabor-Jet model from Biederman lab.

            A given image is transformed with a
            Gabor wavelet and certain values on a grid are chosen for the output.
            Further details are in `Xu et al., 2009
            <http://dx.doi.org/10.1016/j.visres.2009.08.021>`_.

            Original implementation copyright 2004 'Xiaomin Yue
            <http://geon.usc.edu/GWTgrid_simple.m>`_.

            :Kwargs:
                - nScale (int, default: 5)
                    Spatial frequency scales
                - nOrientation (int, default: 8)
                    Orientation spacing; angle = np.pi/nOrientations
            """
            self.nScale = nScale
            self.nOrientation = nOrientation

        def run(self, ims, oneval=False):
            """
            Run GaborJet model.

            :Args:
                ims: str or list of str
                    Image(s) to process witht he model.
            :Kwargs:
                oneval: bool (default: False)
                    Whether only magnitude should be returned. If True, then also
                    phase and gird positions are returned.

            :Returns:
                Magnitude and, depending on 'oneval', phase and grid positions.
            """
            ims = self.input2array(ims)
            JetsMagnitudes = []
            JetsPhases = []
            for im in ims:
                JetsMagnitude, JetsPhase, grid_position = self.test(im)
                JetsMagnitudes.append(JetsMagnitude.ravel())
                JetsPhases.append(JetsPhase.ravel())
            if oneval:
                return np.array(JetsMagnitudes)
            else:
                return (np.array(JetsMagnitudes), np.array(JetsPhases), grid_position)

        def test(self,
                im,
                cell_type = 'complex',
                grid_size = 0,
                sigma = 2*np.pi
                ):
            """
            Apply GaborJet to given images.

            :Args:
                im (numpy.array)
                    input image; can be (128,128) or (256,256) px size

            :Kwargs:
                - cell_type (str, default: 'complex')
                    Choose between 'complex'(40 output values) and 'simple'
                    (80 values, NOT FULLY WORKING YET)
                - grid_size (int, default: 0)
                    How many positions within an image to take
                - sigma (float, default: 2*np.pi)
                    Control the size of gaussian envelope

            :Returns:
                (JetsMagnitude, JetsPhase, grid_position)

            """
            if im.shape[0]!=im.shape[1]:
                sys.exit('The image has to be square. Please try again')

            # generate the grid
            if len(im) in [128, 256]:
                if grid_size == 0:
                    rangeXY = np.arange(20, 110+1, 10)  # 10x10
                elif grid_size == 1:
                    rangeXY = np.arange(10, 120+1, 10)  # 12x12
                else:
                    rangeXY = np.arange(1, 128+1)  # 128x128
                rangeXY *= len(im) / 128  # if len(im)==256, scale up by two
                rangeXY -= 1  # shift from MatLab indexing to Python
            else:
                sys.exit('The image has to be 256*256 px or 128*128 px. Please try again')

            [xx,yy] = np.meshgrid(rangeXY,rangeXY)

            grid = xx + 1j*yy
            grid = grid.T.ravel()  # transpose just to match MatLab's grid(:) behavior
            grid_position = np.hstack([grid.imag, grid.real]).T

            # FFT of the image
            im_freq = np.fft.fft2(im)

            # setup the paramers
            xHalfResL = im.shape[0]/2
            yHalfResL = im.shape[1]/2
            kxFactor = 2*np.pi/im.shape[0]
            kyFactor = 2*np.pi/im.shape[1]

            # setup space coordinate
            [tx,ty] = np.meshgrid(np.arange(-xHalfResL,xHalfResL),np.arange(-yHalfResL,yHalfResL))
            tx = kxFactor*tx
            ty = kyFactor*(-ty)

            # initiallize useful variables
            nvars = self.nScale*self.nOrientation
            if cell_type == 'complex':
                JetsMagnitude  = np.zeros((len(grid), nvars))
                JetsPhase      = np.zeros((len(grid), nvars))
            else:
                JetsMagnitude  = np.zeros((len(grid), 2*nvars))
                JetsPhase      = np.zeros((len(grid), nvars))

            for LevelL in range(self.nScale):
                k0 = np.pi/2 * (1/np.sqrt(2))**LevelL
                for DirecL in range(self.nOrientation):
                    kA = np.pi * DirecL / self.nOrientation
                    k0x = k0 * np.cos(kA)
                    k0y = k0 * np.sin(kA)
                    # generate a kernel specified scale and orientation, which has DC on the center
                    # this is a FFT of a Morlet wavelet (http://en.wikipedia.org/wiki/Morlet_wavelet)
                    freq_kernel = 2*np.pi*(
                        np.exp( -(sigma/k0)**2/2 * ((k0x-tx)**2+(k0y-ty)**2) ) -\
                        np.exp( -(sigma/k0)**2/2 * (k0**2+tx**2+ty**2) )
                        )
                    # use fftshift to change DC to the corners
                    freq_kernel = np.fft.fftshift(freq_kernel)

                    # convolve the image with a kernel of the specified scale and orientation
                    TmpFilterImage = im_freq*freq_kernel
                    #
                    # calculate magnitude and phase
                    iTmpFilterImage = np.fft.ifft2(TmpFilterImage)
                    #
                    #eps = np.finfo(float).eps**(3./4)
                    #real = np.real(iTmpFilterImage)
                    #real[real<eps] = 0
                    #imag = np.imag(iTmpFilterImage)
                    #imag[imag<eps] = 0
                    #iTmpFilterImage = real + 1j*imag

                    TmpGWTPhase = np.angle(iTmpFilterImage)
                    tmpPhase = TmpGWTPhase[rangeXY,:][:,rangeXY] + np.pi
                    JetsPhase[:,LevelL*self.nOrientation+DirecL] = tmpPhase.ravel()
                    #import pdb; pdb.set_trace()

                    if cell_type == 'complex':
                        TmpGWTMag = np.abs(iTmpFilterImage)
                        # get magnitude and phase at specific positions
                        tmpMag = TmpGWTMag[rangeXY,:][:,rangeXY]
                        JetsMagnitude[:,LevelL*self.nOrientation+DirecL] = tmpMag.ravel()
                    else:
                        raise Exception('simple cell type not implemented yet')
                        #TmpGWTMag_real = np.real(iTmpFilterImage)
                        #TmpGWTMag_imag = np.imag(iTmpFilterImage)
                        ## get magnitude and phase at specific positions
                        #tmpMag_real = TmpGWTMag_real[rangeXY,:][:,rangeXY]
                        #tmpMag_imag = TmpGWTMag_imag[rangeXY,:][:,rangeXY]
                        #JetsMagnitude_real[:,LevelL*self.nOrientation+DirecL] = tmpMag_real.ravel()
                        #JetsMagnitude_imag[:,LevelL*self.nOrientation+DirecL] =  tmpMag_imag.ravel()

            if cell_type == 'simple':
                raise Exception('simple cell type not implemented yet')
                #JetsMagnitude = np.vstack((JetsMagnitude_real, JetsMagnitude_imag))
            # use magnitude for dissimilarity measures
            return (JetsMagnitude, JetsPhase, grid_position)

        def dissimilarity(self, *args, **kwargs):
            if 'kind' not in kwargs:
                kwargs['kind'] = 'gaborjet'  # we want this by default
            return super(GaborJet, self).dissimilarity(*args, **kwargs)

        def compare(self, ims):
            output = []
            print 'processing image',
            for imno, im in enumerate(ims):
                print imno,
                out = self.run(im)[0].ravel()  # use JetsMagnitude
                output.append(out)
            dis = self.dissimilarity(output)
            print
            print 'Dissimilarity across stimuli'
            print '0: similar, 1: dissimilar'
            print dis

            ax = plt.subplot(111)
            matrix = ax.imshow(dis, interpolation='none')
            plt.title('Dissimilarity across stimuli\n'
                      '(blue: similar, red: dissimilar)')
            divider = make_axes_locatable(ax)
            cax = divider.append_axes("right", size="5%", pad=0.05)
            plt.colorbar(matrix, cax=cax)
            plt.show()

    class HMAX(Model):
        """
        HMAX for Python

        Based on the original HMAX (`Riesenhuber & Poggio, 1999
        <http://dx.doi.org/10.1038/14819>`_)
        Code rewritten using a Pure MatLab implementation by Minjoon Kouh at the
        MIT Center for Biological and Computational Learning. Most of the
        structure, variable names and some of the comments come from this
        implementation. More comments have been added and code was optimized as
        much as possible while trying to maintain its structure close to the
        original. View-tuned units have been added by Hans Op de Beeck.

        Code's output is tested against the Pure MatLab output which can be tested
        against the Standard C/MatLab code featured at `Riesenhuber's lab
        <http://riesenhuberlab.neuro.georgetown.edu/hmax/index.html#code>`_.
        You can compare the outputs to the standard Lena image between the present
        and C/MatLab implementation using function :mod:test_models

        Note that this implementation is not the most current HMAX
        implementation that doesn't rely on hardcoding features anymore (e.g.,
        Serre et al., 2007).

        Copyright 2011-2012 Jonas Kubilius

        Original VTU implementation copyright 2007 Hans P. Op de Beeck

        Original MatLab implementation copyright 2004 Minjoon Kouh

        Since the original code did not specify a license type, I assume GNU GPL v3
        since it is used in `Jim Mutch's latest implementation of HMAX
        <http://cbcl.mit.edu/jmutch/cns/>`_

        :Kwargs:

            - matlab (boolean, default: False)
                If *True*, Gaussian filters will be implemented using the
                original models implementation which mimicks MatLab's behavior.
                Otherwise, a more efficient numerical method is used.
            - filt_type ({'gaussian', 'gabor'}, default: 'gaussian')
                Type of V1 filter. We default to gaussian as it was used originally
                in HMAX'99. However, many people prefer using Gabor filters as
                they presumambly model V1 better.

        """
        def __init__(self, matlab=False, filt_type='gaussian'):

            self.n_ori = 4 # number of orientations
            # S1 filter sizes for scale band 1, 2, 3, and 4
            self.filter_sizes_all = [[7, 9], [11, 13, 15], [17, 19, 21],
                                     [23, 25, 27, 29]]
            # specify (per scale band) how many S1 units will be used to pool over
            self.C1_pooling_all = [4, 6, 9, 12]
            self.S2_config = [2,2]  # how many C1 outputs to put into one "window" in S2 in each direction

            if filt_type == 'gaussian':  # "typically" used
                if matlab:  # exact replica of the MatLab implementation
                    self.filts = self.get_gaussians_matlab(self.filter_sizes_all,
                                                           self.n_ori)
                else:  # a faster and more elegant implementation
                    self.filts = self.get_gaussians(self.filter_sizes_all,
                                                    self.n_ori)
                self.mask_name = 'square'
            elif filt_type == 'gabor':
                self.filts = self.get_gabors(self.filter_sizes_all, self.n_ori)
                self.mask_name = 'circle'
            else:
                raise ValueError, "filter type not recognized"

            self.istrained = False  # initially VTUs are not set up

        def run(self, test_ims=None, train_ims=None, oneval=False):
            """
            This is the main function to run the model.
            First, it trains the model, i.e., sets up prototypes for VTU.
            Next, it runs the model.
            """
            if train_ims is not None:
                self.train(train_ims)
            if test_ims is None:
                test_ims = [self.get_teststim()]
            output = self.test(test_ims, oneval=oneval)
            if oneval:
                return output['C2']
            else:
                return output

        def train(self, train_ims):
            """
            Train the model, i.e., supply VTUs with C2 responses to 'prototype'
            images to which these units will be maximally tuned.
            """
            try:
                self.tuning = pickle.load(open(train_ims,'rb'))
                print 'done'
            except:
                train_ims = self.input2array(train_ims)
                self.tuning = self.test(train_ims, op='training')['C2']
            self.istrained = True

        def test(self, ims, op='testing', oneval=False):
            """
            Test the model on the given image
            """
            ims = self.input2array(ims)
            # Get number of filter sizes
            size_S1 = sum([len(fs) for fs in self.filter_sizes_all])
            # outputs from each layer are stored if you want to inspect them closer
            # but note that S1 is *massive*
            output = {}
            # S1 will not be in the output because it's too large:
            # with default parameters S1 takes 256*256*12*4*64bits = 24Mb per image
            S1 = np.zeros((ims.shape[1], ims.shape[2], size_S1, self.n_ori))
            output['C1'] = np.zeros(ims.shape + (self.n_ori,
                                    len(self.filter_sizes_all)))
            # S2 has an irregular shape which depends on the spatial frequency band
            # so we'll omit it as well
            S2 = []
            C2_tmp = np.zeros(((self.S2_config[0]*self.S2_config[1])**self.n_ori,
                                len(self.filter_sizes_all)))
            output['C2'] = np.zeros((len(ims),C2_tmp.shape[0]))

            for imNo, im in enumerate(ims):
                sys.stdout.write("\rRunning HMAX... %s: %d%%" %(op, 100*imNo/len(ims)))
                sys.stdout.flush()
                # Go through each scale band
                S1_idx = 0
                for which_band in range(len(self.filter_sizes_all)):
                    # calculate S1 responses
                    S1_tmp = self.get_S1(im, which_band)
                    num_filter = len(self.filter_sizes_all[which_band])
                    # store S1 responses for each scale band
                    S1[..., S1_idx:S1_idx + num_filter, :] = S1_tmp
                    S1_idx += num_filter
                    # calculate other layers
                    C1_tmp = self.get_C1(S1_tmp, which_band)
                    output['C1'][imNo, ..., which_band] = C1_tmp
                    S2_tmp = self.get_S2(C1_tmp, which_band)
                    S2.append(S2_tmp)
                    C2_tmp[:, which_band] = self.get_C2(S2_tmp, which_band)
                output['C2'][imNo] = np.max(C2_tmp, -1) # max over all scale bands
            output['S2'] = S2
            # calculate VTU if trained
            if self.istrained:
                output['VTU'] = self.get_VTU(output['C2'])
            sys.stdout.write("\rRunning HMAX... %s: done\n" %op)

            return output

        def get_gaussians(
            self,
            filter_sizes_all,
            n_ori = 4,
            sigDivisor = 4.
            ):
            """
            Generates 2D difference of Gaussians (DoG) filters.
            This function is a faster, more accurate and more elegant version of
            the original gaussian_filters_matlab but will not produce identical
            filters as the original (but very close). For practical purposes, this
            one is prefered. In case you want to mimic the identical behavior of
            the original HMAX, use gaussian_filters_matlab.

            **Parameters**
                filter_sizes_all: list (depth 2))
                    A nested list (grouped by filter bands) of integer filter sizes
                n_ori: int
                    A number of filter orientations (default: 4)
                    Orientations are spaced by np.pi/n_ori
                sigDivisor: float
                    A parameter to adjust DoG filter frequency (default: 4.)

            **Returns**
                gaussians: list (depth 2)
                    A nested list of filters of all orientations

            """
            gaussians = []
            # loop over filter bands
            for fNo, filter_sizes in enumerate(filter_sizes_all):
                gaussians.append([])

                # loop over filter sizes within a filter band
                for filter_size in filter_sizes:
                    fxx = np.zeros((filter_size,filter_size,n_ori))
                    sigmaq = (filter_size/sigDivisor)**2
                    i = np.arange(-filter_size/2+1,filter_size/2+1)
                    ii,jj = np.meshgrid(i,i)
                    for t in range(n_ori):
                        theta = t*np.pi/n_ori
                        x = ii*np.cos(theta) - jj*np.sin(theta)
                        y = ii*np.sin(theta) + jj*np.cos(theta)
                        # generate a 2D DoG of a particular orientation
                        gaussian = (y**2/sigmaq - 1) / sigmaq * \
                                    np.exp(-(x**2 + y**2) / (2*sigmaq))
                        # normalize the filter to zero mean and unit variance
                        gaussian -= np.mean(gaussian)
                        gaussian /= np.sqrt(np.sum(gaussian**2))
                        fxx[:,:,t] = gaussian

                    gaussians[fNo].append(fxx)

            return gaussians

        def get_gaussians_matlab(
            self,
            filter_sizes_all,
            n_ori = 4,
            sigDivisor = 4.):
            """
            Generates 2D difference of Gaussians (DoG) filters.
            This is the original version of DoG filters used in HMAX. It was
            written in a very cumbersome way and thus I replaced it by the
            gaussian_filters function. If you want to produce identical
            numerical values of the filters, you should use this function.
            Otherwise, gaussian_filters does the job just as well, but much nicer.

            **Parameters**
                filter_sizes_all: list (depth 2))
                    A nested list (grouped by filter bands) of integer filter sizes
                n_ori: int
                    A number of filter orientations (default: 4)
                    Orientations are spaced by np.pi/n_ori
                sigDivisor: float
                    A parameter to adjust DoG filter frequency (default: 4.)

            **Returns**
                gaussians: list (depth 2)
                    A nested list of filters of all orientations

            """

            gaussians = []
            # loop over filter bands
            for fNo, filter_sizes in enumerate(filter_sizes_all):
                gaussians.append([])

                # loop over filter sizes within a filter band
                for filter_size in filter_sizes:
                    fx1 = np.zeros((filter_size,filter_size,n_ori))

                    # we gonna use a trick here:
                    # make filters sqrt(2) times bigger so that we can rotate them
                    # without getting zeros around the edges
                    fieldSize = int(np.ceil(filter_size*np.sqrt(2)))
                    fieldSize = fieldSize + 1 - fieldSize%2 # make odd
                    filtSizeH = fieldSize/2
                    cropOff = (fieldSize-filter_size)/2
                    cropRange = slice(cropOff, cropOff+filter_size)
                    sigmaq = (filter_size/sigDivisor)**2

                    i = np.arange(-fieldSize/2+1,fieldSize/2+1)
                    ii,jj = np.meshgrid(i,i)

                    theta = 0
                    x = ii*np.cos(theta) - jj*np.sin(theta)
                    y = ii*np.sin(theta) + jj*np.cos(theta)
                    # generate a 2D DoG of 0 deg orientation
                    fxx = (y**2/sigmaq-1)/sigmaq * np.exp(-(x**2+y**2)/(2*sigmaq))

                    # now loop over the orientations, rotate and trim the filter
                    for t in range(n_ori):
                        fxx = self.addZeros(fxx,cropOff)
                        fxx = scipy.ndimage.interpolation.rotate(fxx,45,reshape=False,order=1)
                        fxx = fxx[cropOff:fieldSize+cropOff,cropOff:fieldSize+cropOff]
                        # we generate first rotated versions of a filter
                        # and end up with the one having 0 deg, but now having
                        # undergonne all interpolations and rotations
                        # to make things equall
                        count = (t+1)%n_ori
                        # crop the edges
                        # note that you should assign this cropped version to sth
                        # like fx1[:,:,count], and not a variable on its own
                        # as otherwise you only pass a reference to fxx
                        # so you'd modify fxx as well when normalizing
                        # and you really don't want that
                        fx1[:,:,count] = fxx[cropRange, cropRange]
                        # normalize the filter to zero mean and unit variance
                        fx1[:,:,count] -= np.mean(fx1[:,:,count])
                        fx1[:,:,count] /= np.sqrt(np.sum(fx1[:,:,count]**2))
                    gaussians[fNo].append(fx1)

            return gaussians

        def get_gabors(
            self,
            filter_sizes_all,
            n_ori = 4,
            k = 2.1,
            sx = 2*np.pi * 1/3.,
            sy = 2*np.pi * 1/1.8,
            phase = 0 # S1 Gabor function phase (0 for cosine and pi/2 for sine)

            ):
            """
            Generates 2D Gabor filters.
            This is the original version of Gabor filters used in HMAX.

            **Parameters**
                filter_sizes_all: list (depth 2))
                    A nested list (grouped by filter bands) of integer filter sizes
                n_ori: int
                    A number of filter orientations (default: 4)
                    Orientations are spaced by np.pi/n_ori
                k: float
                    Gabor wave number (default: 2.1)
                sx: float
                    Gabor sigma in x-dir (default: 2*np.pi * 1/3.)
                sy: float
                    Gabor sigma in y-dir (default: 2*np.pi * 1/1.8)
                phase: int
                    Gabor function phase (0 (default) for cosine (even),
                                          np.pi/2 for sine (odd))

            **Returns**
                gabors: list (depth 2)
                    A nested list of filters of all orientations
            """

            gabors = []
            # loop over filter bands
            for fNo, filter_sizes in enumerate(filter_sizes_all):
                gabors.append([])
                # loop over filter sizes within a filter band
                for filter_size in filter_sizes:
                    fxx = np.zeros((filter_size, filter_size, n_ori))
                    inc = 2. / filter_size
                    i = np.pi * np.arange(-1+inc/2, 1+inc/2, inc)
                    ii,jj = np.meshgrid(i,i)

                    circle = self.get_circle(filter_size)
                    circle_sum = np.sum(circle)

                    for t in range(n_ori):
                        theta = t*np.pi/n_ori
                        x = ii*np.cos(theta) - jj*np.sin(theta)
                        y = ii*np.sin(theta) + jj*np.cos(theta)
                        # generate a 2D DoG of a particular orientation
                        gabor = np.cos(k * x - phase) * \
                                np.exp(-( (x/sx)**2 + (y/sy)**2) / 2)
                        # apply circle mask
                        gabor *= circle
                        # normalize the filter to zero mean and unit variance
                        gabor -= circle * np.sum(gabor) / np.sum(circle)
                        gabor /= np.sqrt(np.sum(gabor**2))
                        fxx[:,:,t] = gabor
                    gabors[fNo].append(fxx)

            return gabors

        def get_circle(self, filter_size, radius=1.):
                inc = 2./filter_size
                r = np.arange(-1+inc/2, 1+inc/2, inc)
                x, y = np.meshgrid(r, r)
                return x**2 + y**2 <= radius**2

        def addZeros(self, matrix, numZeros):
            """
            Pads matrix with zeros

            **Parameters**
                matrix: numpy.array
                    A 2D numpy array to be padded
                numZeros: int
                    Number of rows and colums of zeros to pad

            **Returns**
                matrix_new: numpy.array
                    A zero-padded 2D numpy array
            """
            matrix_new = np.zeros((matrix.shape[0]+2*numZeros,
                matrix.shape[1]+2*numZeros))
            matrix_new[numZeros:matrix.shape[0]+numZeros,
                numZeros:matrix.shape[1]+numZeros] = matrix

            return matrix_new

        def get_S1(self, im, whichBand):
            """
            This function returns S1 responses,
            using the difference of the Gaussians or Gabors as S1 filters.
            Filters are based on the original HMAX model.
            """
            filter_sizes = self.filter_sizes_all[whichBand]
            num_filter = len(filter_sizes)
            # make S1 same size as stimulus
            S1 = np.zeros((im.shape[0], im.shape[1], num_filter, self.n_ori))

            for j in range(num_filter):
                S1_filter = self.filts[whichBand][j]
                fs = filter_sizes[j]
                if self.mask_name == 'circle':
                    mask = self.get_circle(fs)
                else:
                    mask = np.ones((fs,fs))
                # import pdb; pdb.set_trace()
                norm = scipy.ndimage.convolve(im**2, mask, mode='constant') + \
                                              sys.float_info.epsilon
                for i in range(self.n_ori):
                    S1_buf = scipy.ndimage.convolve(im, S1_filter[:,:,i],
                                                    mode='constant')
                    S1[:,:,j,i] = np.abs(S1_buf) / np.sqrt(norm)

            return S1

        def get_C1(self, S1, which_band):
            """
            Computes C1 responses given S1 as a max over a a couple of filter
            (as defined by C1_pooling)
            """
            C1_pooling = self.C1_pooling_all[which_band]
            C1 = scipy.ndimage.filters.maximum_filter(
                S1,
                size = (C1_pooling,C1_pooling,1,1),
                mode = 'constant',
                origin = -(C1_pooling/2)
                )

            # Max over scales;
            C1 = np.squeeze(np.max(C1,2))
            return C1

        def get_S2(self, C1, which_band, target=1., sigma=1.):
            """
            Calculates S2 responses given C1.

            First it pools over C1 activities over various combinations of 4
            filters.
            Then computes a distance to /target/ using /sigma/ as its tuning
            sharpness.
            """
            # half overlaped S2 sampling
            S2_shift = int(np.ceil(self.C1_pooling_all[which_band]/2.))
            # C1 afferents are adjacent for each S2
            C1_shift = S2_shift * 2 # distance/shift between C1 afferents
            S2_buf = [C1.shape[0] - C1_shift*(self.S2_config[0]-1),
                C1.shape[1] - C1_shift*(self.S2_config[1]-1)]

            # produce a sequence of all possible orientation combinations
            seq = itertools.product(range(self.n_ori),
                repeat = self.S2_config[0]*self.S2_config[1])
            # we have to keep the same order as in the original model
            seq = np.fliplr([s for s in seq])

            S2_permute = np.zeros((
                (S2_buf[0]-1)/S2_shift+1,
                (S2_buf[1]-1)/S2_shift+1,
                len(seq),
                self.S2_config[0]*self.S2_config[1]))

            for c1 in range(self.S2_config[0]):
                for c2 in range(self.S2_config[1]):
                    c = self.S2_config[0]*c2 + c1
                    r1 = np.arange(C1_shift*c1, S2_buf[0] + C1_shift*c1, S2_shift)
                    r2 = np.arange(C1_shift*c2, S2_buf[1] + C1_shift*c2, S2_shift)
                    ii,jj = np.meshgrid(r1, r2)
                    S2_permute[:,:,:,c] = np.take(C1[jj,ii], seq[:,c], axis=2)
                    # for si, s in enumerate(seq):
                    #     S2_permute[:,:,si,c] = C1[jj,ii,s[c]] # the window is
                                                             # sliding in the x-dir
            S2 = np.sum((S2_permute-target)**2,3)
            S2 = np.exp(-S2/(2.*sigma**2))

            return S2

        def get_C2(self, S2, which_band):
            """C2 is a max over space per an S2 filter quadruplet"""
            return  np.max(np.max(S2,0),0)

        def get_VTU(self, C2resp, tuningWidth = .1):
            """
            Calculate response of view-tuned units

            **Parameters**
                c2RespSpec: numpy.array
                    C2 responses to the stimuli
                tuningWidth: float
                    How sharply VTUs should be tuned; lower values are shaper
                    tuning (default: .1)
            **Returns**
                output: np.array
                    An array where each column represents view-tuned units
                    responses to a particular image (stimulus)
            """
            def sq(c):
                return np.dot(c,c)
            def func(row):
                # difference between tuning and each C2 response
                diff = self.tuning - \
                        np.tile(row,(self.tuning.shape[0],1))
                # this difference is then square-summed and then exponentiated :)
                return np.exp(-.5 * np.apply_along_axis(sq,1,diff) / tuningWidth)

            if not self.istrained:
                raise Exception("You must first train VTUs by providing prototype "
                                "images to them using the train() function")

            if C2resp.shape[1] != self.tuning.shape[1]:
                raise Exception("The size of exemplar matrix does not match "
                                "that of the prototype matrix")
            # apply func on each row
            return np.apply_along_axis(func, 1, C2resp)

        def compare(self, ims):
            print ims
            print 'processing image',
            output = self.run(ims)['C2']
            dis = self.dissimilarity(output)
            print
            print 'Dissimilarity across stimuli'
            print '0: similar, 1: dissimilar'
            print dis

            ax = plt.subplot(111)
            matrix = ax.imshow(dis, interpolation='none')
            plt.title('Dissimilarity across stimuli\n'
                      '(blue: similar, red: dissimilar)')
            divider = make_axes_locatable(ax)
            cax = divider.append_axes("right", size="5%", pad=0.05)
            plt.colorbar(matrix, cax=cax)
            plt.show()

    KNOWN_MODELS = {'px': Pixelwise, 'gaborjet': GaborJet, 'hmax': HMAX}
    #['px': Pixelwise, GaborJet, HMAX]

    def get_model(model_name):
        if model_name in KNOWN_MODELS:
            return KNOWN_MODELS[model_name]()
        else:
            raise Exception('Model %s not recognized' %model_name)

    if __name__ == '__main__':
        models = KNOWN_MODELS

        if len(sys.argv) == 1:
            m = HMAX()
        else:
            model_name = sys.argv[1]
            if model_name in models: m = models[model_name]()
        if len(sys.argv) > 2:  # give image file names using glob syntax
            ims = sys.argv[2:]
        else:
            ims = [m.get_teststim(), m.get_teststim().T]

        output = m.compare(ims)