# Coverage for pygeodesy/utmupsBase.py : 97%

## 236 statements 230 run 6 missing 21 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 | # -*- coding: utf-8 -*- u'''(INTERNAL) Private class C{UtmUpsBase}, functions and constants for L{epsg}, L{etm}, L{mgrs}, L{ups} and L{utm}. ''' from pygeodesy.basics import isint, isscalar, isstr, map1, neg_, \ _xinstanceof, _xsubclassof from pygeodesy.constants import _float, _0_0, _0_5, _N_90_0, _180_0 from pygeodesy.datums import _ellipsoidal_datum, _WGS84 from pygeodesy.dms import degDMS, parseDMS2 from pygeodesy.ellipsoidalBase import LatLonEllipsoidalBase as _LLEB from pygeodesy.errors import _or, ParseError, _parseX, _ValueError, \ _xkwds, _xkwds_get, _xkwds_not from pygeodesy.interns import NN, _A_, _B_, _COMMA_, _Error_, \ _gamma_, _n_a_, _not_, _N_, _NS_, _PLUS_, \ _scale_, _SPACE_, _Y_, _Z_, _UNDER from pygeodesy.lazily import _ALL_DOCS, _ALL_MODS as _MODS from pygeodesy.named import _NamedBase, nameof, notOverloaded, _xnamed from pygeodesy.namedTuples import EasNor2Tuple, LatLonDatum5Tuple from pygeodesy.props import deprecated_method, property_doc_, _update_all, \ deprecated_property_RO, Property_RO, property_RO from pygeodesy.streprs import Fmt, fstr, _fstrENH2, _xattrs, _xzipairs from pygeodesy.units import Band, Easting, Northing, Scalar, Zone from pygeodesy.utily import wrap360 __all__ = () __version__ = '22.10.05' _UPS_BANDS = _A_, _B_, _Y_, _Z_ # UPS polar bands SE, SW, NE, NW # _UTM_BANDS = _MODS.utm._Bands _UTM_LAT_MAX = _float( 84) # PYCHOK for export (C{degrees}) _UTM_LAT_MIN = _float(-80) # PYCHOK for export (C{degrees}) _UPS_LAT_MAX = _UTM_LAT_MAX - _0_5 # PYCHOK includes 30' UTM overlap _UPS_LAT_MIN = _UTM_LAT_MIN + _0_5 # PYCHOK includes 30' UTM overlap _UPS_LATS = {_A_: _N_90_0, _Y_: _UTM_LAT_MAX, # UPS band bottom latitudes, _B_: _N_90_0, _Z_: _UTM_LAT_MAX} # PYCHOK see .Mgrs.bandLatitude _UTM_ZONE_MAX = 60 # PYCHOK for export _UTM_ZONE_MIN = 1 # PYCHOK for export _UTM_ZONE_OFF_MAX = 60 # PYCHOK max Central meridian offset (C{degrees}) _UPS_ZONE = _UTM_ZONE_MIN - 1 # PYCHOK for export _UPS_ZONE_STR = Fmt.zone(_UPS_ZONE) # PYCHOK for export _UTMUPS_ZONE_INVALID = -4 # PYCHOK for export too _UTMUPS_ZONE_MAX = _UTM_ZONE_MAX # PYCHOK for export too, by .units.py _UTMUPS_ZONE_MIN = _UPS_ZONE # PYCHOK for export too, by .units.py # _MAX_PSEUDO_ZONE = -1 # _MIN_PSEUDO_ZONE = -4 # _UTMUPS_ZONE_MATCH = -3 # _UTMUPS_ZONE_STANDARD = -1 # _UTM = -2 def _hemi(lat, N=0): # imported by .ups, .utm '''Return the hemisphere letter. @arg lat: Latitude (C{degrees} or C{radians}). @kwarg N: Minimal North latitude, C{0} or C{_N_}. @return: C{'N'|'S'} for north-/southern hemisphere. ''' return _NS_[int(lat < N)] def _to4lldn(latlon, lon, datum, name): '''(INTERNAL) Return 4-tuple (C{lat, lon, datum, name}). ''' try: # if lon is not None: # raise AttributeError lat, lon = map1(float, latlon.lat, latlon.lon) _xinstanceof(_LLEB, LatLonDatum5Tuple, latlon=latlon) d = datum or latlon.datum except AttributeError: lat, lon = parseDMS2(latlon, lon) d = datum or _WGS84 return lat, lon, d, (name or nameof(latlon)) def _to3zBhp(zone, band, hemipole=NN, Error=_ValueError): # imported by .epsg, .ups, .utm, .utmups '''Parse UTM/UPS zone, Band letter and hemisphere/pole letter. @arg zone: Zone with/-out Band (C{scalar} or C{str}). @kwarg band: Optional I{longitudinal/polar} Band letter (C{str}). @kwarg hemipole: Optional hemisphere/pole letter (C{str}). @kwarg Error: Optional error to raise, overriding the default C{ValueError}. @return: 3-Tuple (C{zone, Band, hemisphere/pole}) as (C{int, str, 'N'|'S'}) where C{zone} is C{0} for UPS or C{1..60} for UTM and C{Band} is C{'A'..'Z'} I{NOT} checked for valid UTM/UPS bands. @raise ValueError: Invalid B{C{zone}}, B{C{band}} or B{C{hemipole}}. ''' try: B, z = band, _UTMUPS_ZONE_INVALID if isscalar(zone): z = int(zone) elif zone and isstr(zone): if zone.isdigit(): z = int(zone) elif len(zone) > 1: B = zone[-1:] z = int(zone[:-1]) elif zone.upper() in _UPS_BANDS: # single letter B = zone z = _UPS_ZONE if _UTMUPS_ZONE_MIN <= z <= _UTMUPS_ZONE_MAX: hp = hemipole[:1].upper() if hp in _NS_ or not hp: z = Zone(z) B = Band(B.upper()) if B.isalpha(): return z, B, (hp or _hemi(B, _N_)) elif not B: return z, B, hp raise ValueError # _invalid_ except (AttributeError, IndexError, TypeError, ValueError) as x: raise Error(zone=zone, band=B, hemipole=hemipole, cause=x) def _to3zll(lat, lon): # imported by .ups, .utm '''Wrap lat- and longitude and determine UTM zone. @arg lat: Latitude (C{degrees}). @arg lon: Longitude (C{degrees}). @return: 3-Tuple (C{zone, lat, lon}) as (C{int}, C{degrees90}, C{degrees180}) where C{zone} is C{1..60} for UTM. ''' x = wrap360(lon + _180_0) # use wrap360 to get ... z = int(x) // 6 + 1 # ... longitudinal UTM zone [1, 60] and ... return Zone(z), lat, (x - _180_0) # ... -180 <= lon < 180 class UtmUpsBase(_NamedBase): '''(INTERNAL) Base class for L{Utm} and L{Ups} coordinates. ''' _band = NN # latitude band letter ('A..Z') _Bands = NN # valid Band letters, see L{Utm} and L{Ups} _datum = _WGS84 # L{Datum} _easting = _0_0 # Easting, see B{C{falsed}} (C{meter}) _Error = None # I{Must be overloaded}, see function C{notOverloaded} _falsed = True # falsed easting and northing (C{bool}) _gamma = None # meridian conversion (C{degrees}) _hemisphere = NN # hemisphere ('N' or 'S'), different from UPS pole _latlon = None # cached toLatLon (C{LatLon} or C{._toLLEB}) _northing = _0_0 # Northing, see B{C{falsed}} (C{meter}) _scale = None # grid or point scale factor (C{scalar}) or C{None} # _scale0 = _K0 # central scale factor (C{scalar}) _ups = None # cached toUps (L{Ups}) _utm = None # cached toUtm (L{Utm}) def __init__(self, easting, northing, band=NN, datum=None, falsed=True, gamma=None, scale=None, **convergence): '''(INTERNAL) New L{UtmUpsBase}. ''' E = self._Error if not E: notOverloaded(self, callername=_UNDER(_Error_)) self._easting = Easting(easting, Error=E) self._northing = Northing(northing, Error=E) if band: self._band1(band) if datum not in (None, self._datum): self._datum = _ellipsoidal_datum(datum) # raiser=_datum_, name=band if not falsed: self._falsed = False if convergence: # for backward compatibility gamma = _xkwds_get(convergence, convergence=gamma) if gamma is not self._gamma: self._gamma = Scalar(gamma=gamma, Error=E) if scale is not self._scale: self._scale = Scalar(scale=scale, Error=E) def __repr__(self): return self.toRepr(B=True) def __str__(self): return self.toStr() def _band1(self, band): '''(INTERNAL) Re/set the latitudinal or polar band. ''' if band: _xinstanceof(str, band=band) # if not self._Bands: # notOverloaded(self, callername=_UNDER('Bands')) if band not in self._Bands: t = _or(*sorted(set(map(repr, self._Bands)))) raise self._Error(band=band, txt=_not_(t)) self._band = band elif self._band: # reset self._band = NN @deprecated_property_RO def convergence(self): '''DEPRECATED, use property C{gamma}.''' return self.gamma @property_doc_(''' the (ellipsoidal) datum of this coordinate.''') def datum(self): '''Get the datum (L{Datum}). ''' return self._datum @datum.setter # PYCHOK setter! def datum(self, datum): '''Set the (ellipsoidal) datum L{Datum}, L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}). ''' d = _ellipsoidal_datum(datum) if self._datum != d: _update_all(self) self._datum = d @Property_RO def easting(self): '''Get the easting (C{meter}). ''' return self._easting @Property_RO def eastingnorthing(self): '''Get easting and northing (L{EasNor2Tuple}C{(easting, northing)}). ''' return EasNor2Tuple(self.easting, self.northing) def eastingnorthing2(self, falsed=True): '''Return easting and northing, falsed or unfalsed. @kwarg falsed: If C{True} return easting and northing falsed (C{bool}), otherwise unfalsed. @return: An L{EasNor2Tuple}C{(easting, northing)} in C{meter}. ''' e, n = self.falsed2 if self.falsed and not falsed: e, n = neg_(e, n) elif falsed and not self.falsed: pass else: e = n = _0_0 return EasNor2Tuple(Easting( e + self.easting, Error=self._Error), Northing(n + self.northing, Error=self._Error)) @Property_RO def _epsg(self): '''(INTERNAL) Cache for method L{toEpsg}. ''' return _MODS.epsg.Epsg(self) @Property_RO def falsed(self): '''Get easting and northing falsed (C{bool}). ''' return self._falsed @Property_RO def falsed2(self): # PYCHOK no cover '''(INTERNAL) I{Must be overloaded}, see function C{notOverloaded}. ''' notOverloaded(self) @Property_RO def gamma(self): '''Get the meridian convergence (C{degrees}) or C{None} if not available. ''' return self._gamma @property_RO def hemisphere(self): '''Get the hemisphere (C{str}, 'N'|'S'). ''' if not self._hemisphere: self._toLLEB() return self._hemisphere def _latlon5(self, LatLon, **LatLon_kwds): '''(INTERNAL) Get cached C{._toLLEB} as B{C{LatLon}} instance. ''' ll = self._latlon if LatLon is None: r = LatLonDatum5Tuple(ll.lat, ll.lon, ll.datum, ll.gamma, ll.scale) else: _xsubclassof(_LLEB, LatLon=LatLon) kwds = _xkwds(LatLon_kwds, datum=ll.datum) r = _xattrs(LatLon(ll.lat, ll.lon, **kwds), ll, _UNDER(_gamma_), _UNDER(_scale_)) return _xnamed(r, ll.name) def _latlon5args(self, ll, _toBand, unfalse, *other): '''(INTERNAL) See C{._toLLEB} methods, functions C{ups.toUps8} and C{utm._toXtm8} ''' ll._toLLEB_args = (unfalse,) + other if unfalse: if not self._band: self._band = _toBand(ll.lat, ll.lon) if not self._hemisphere: self._hemisphere = _hemi(ll.lat) self._latlon = ll @Property_RO def _lowerleft(self): # by .ellipsoidalBase._lowerleft '''Get this UTM or UPS C{un}-centered (L{Utm} or L{Ups}) to its C{lowerleft}. ''' return _lowerleft(self, 0) @Property_RO def _mgrs(self): '''(INTERNAL) Cache for method L{toMgrs}. ''' return _toMgrs(self) @Property_RO def _mgrs_lowerleft(self): '''(INTERNAL) Cache for method L{toMgrs}, I{un}-centered. ''' utmups = self._lowerleft return self._mgrs if utmups is self else _toMgrs(utmups) @Property_RO def northing(self): '''Get the northing (C{meter}). ''' return self._northing @Property_RO def scale(self): '''Get the grid scale (C{float}) or C{None}. ''' return self._scale @Property_RO def scale0(self): '''Get the central scale factor (C{float}). ''' return self._scale0 @deprecated_method def to2en(self, falsed=True): # PYCHOK no cover '''DEPRECATED, use method C{eastingnorthing2}. @return: An L{EasNor2Tuple}C{(easting, northing)}. ''' return self.eastingnorthing2(falsed=falsed) def toEpsg(self): '''Determine the B{EPSG (European Petroleum Survey Group)} code. @return: C{EPSG} code (C{int}). @raise EPSGError: See L{Epsg}. ''' return self._epsg def _toLLEB(self, **kwds): # PYCHOK no cover '''(INTERNAL) I{Must be overloaded}. ''' notOverloaded(self, **kwds) def toMgrs(self, center=False): '''Convert this UTM/UPS coordinate to an MGRS grid reference. @kwarg center: If C{True}, I{un}-center this UTM or UPS to its C{lowerleft} (C{bool}) or by C{B{center} meter} (C{scalar}). @return: The MGRS grid reference (L{Mgrs}). @see: Function L{pygeodesy.toMgrs} in module L{mgrs} for more details. @note: If not specified, the I{latitudinal} C{band} is computed from the (geodetic) latitude and the C{datum}. ''' return self._mgrs if center in (False, 0, _0_0) else ( self._mgrs_lowerleft if center in (True,) else _toMgrs(_lowerleft(self, center))) # PYCHOK indent def _toRepr(self, fmt, B, cs, prec, sep): # PYCHOK expected '''(INTERNAL) Return a representation for this ETM/UTM/UPS coordinate. ''' t = self.toStr(prec=prec, sep=None, B=B, cs=cs) # hemipole T = 'ZHENCS'[:len(t)] return _xzipairs(T, t, sep=sep, fmt=fmt) def _toStr(self, hemipole, B, cs, prec, sep): '''(INTERNAL) Return a string for this ETM/UTM/UPS coordinate. ''' z = NN(Fmt.zone(self.zone), (self.band if B else NN)) # PYCHOK band t = (z, hemipole) + _fstrENH2(self, prec, None)[0] if cs: prec = cs if isint(cs) else 8 # for backward compatibility t += (_n_a_ if self.gamma is None else degDMS(self.gamma, prec=prec, pos=_PLUS_), _n_a_ if self.scale is None else fstr(self.scale, prec=prec)) return t if sep is None else sep.join(t) def _lowerleft(utmups, center): # by .ellipsoidalBase._lowerleft '''(INTERNAL) I{Un}-center a B{C{utmups}} to its C{lowerleft} by C{B{center} meter} or by a I{guess} if B{C{center}} is C{0}. ''' if center: e = n = -center else: c = 5 # center for _ in range(3): c *= 10 # 50, 500, 5000 t = c * 2 e = int(utmups.easting % t) n = int(utmups.northing % t) if (e == c and n in (c, c - 1)) or \ (n == c and e in (c, c - 1)): break else: return utmups # unchanged r = _xkwds_not(None, datum=utmups.datum, gamma=utmups.gamma, scale=utmups.scale) return utmups.classof(utmups.zone, utmups.hemisphere, utmups.easting - e, utmups.northing - n, band=utmups.band, falsed=utmups.falsed, **r) def _parseUTMUPS5(strUTMUPS, UPS, Error=ParseError, band=NN, sep=_COMMA_): '''(INTERNAL) Parse a string representing a UTM or UPS coordinate consisting of C{"zone[band] hemisphere/pole easting northing"}. @arg strUTMUPS: A UTM or UPS coordinate (C{str}). @kwarg band: Optional, default Band letter (C{str}). @kwarg sep: Optional, separator to split (","). @return: 5-Tuple (C{zone, hemisphere/pole, easting, northing, band}). @raise ParseError: Invalid B{C{strUTMUPS}}. ''' def _UTMUPS5(strUTMUPS, UPS, band, sep): u = strUTMUPS.lstrip() if UPS and not u.startswith(_UPS_ZONE_STR): raise ValueError(_not_(_UPS_ZONE_STR)) u = u.replace(sep, _SPACE_).strip().split() if len(u) < 4: raise ValueError(_not_(sep)) z, h = u[:2] if h[:1].upper() not in _NS_: raise ValueError(_SPACE_(h, _not_(_NS_))) if z.isdigit(): z, B = int(z), band else: for i in range(len(z)): if not z[i].isdigit(): # int('') raises ValueError z, B = int(z[:i]), z[i:] break else: raise ValueError(z) e, n = map(float, u[2:4]) return z, h.upper(), e, n, B.upper() return _parseX(_UTMUPS5, strUTMUPS, UPS, band, sep, strUTMUPS=strUTMUPS, Error=Error) def _toMgrs(utmups): '''(INTERNAL) Convert a L{Utm} or L{Ups} to an L{Mgrs} instance. ''' return _MODS.mgrs.toMgrs(utmups, datum=utmups.datum, name=utmups.name) __all__ += _ALL_DOCS(UtmUpsBase) # **) MIT License # # Copyright (C) 2016-2022 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.