# Coverage for pygeodesy/osgr.py : 97%

## 303 statements 294 run 9 missing 65 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 547 548 549 550 551 552 553 554 555 556 557 558 559 560 561 562 563 564 565 566 567 568 569 570 571 572 573 574 575 576 577 578 579 580 581 582 583 584 585 586 587 588 589 590 591 592 593 594 595 596 597 598 599 600 601 602 603 604 605 606 607 608 609 610 611 612 613 614 615 616 617 618 619 620 621 622 623 624 625 626 627 628 629 630 631 632 633 634 635 636 637 638 639 640 641 642 643 644 645 646 647 648 649 650 651 652 653 654 655 656 657 658 659 660 661 662 663 664 665 666 667 668 669 670 671 672 673 674 675 676 677 678 679 680 681 682 683 684 685 686 687 688 689 690 691 692 693 694 695 696 697 698 699 700 701 702 703 704 705 706 707 708 709 710 711 712 713 714 715 716 717 718 719 720 721 722 723 724 725 726 727 728 729 730 731 732 733 734 735 736 737 738 739 740 741 742 743 744 745 746 747 748 749 750 751 752 753 754 755 756 757 758 759 760 761 762 763 764 765 766 767 768 769 770 771 772 773 774 775 776 777 778 779 780 781 782 783 784 785 786 787 788 789 790 791 792 793 794 795 796 797 798 799 800 801 802 803 804 805 806 807 808 809 810 811 812 813 814 815 | # -*- coding: utf-8 -*- u'''Ordnance Survey Grid References (OSGR) references on the UK U{National Grid <https://www.OrdnanceSurvey.co.UK/documents/resources/guide-to-nationalgrid.pdf>}. Classes L{Osgr} and L{OSGRError} and functions L{parseOSGR} and L{toOsgr}. A pure Python implementation, transcoded from I{Chris Veness}' JavaScript originals U{OS National Grid <https://www.Movable-Type.co.UK/scripts/latlong-os-gridref.html>} and U{Module osgridref <https://www.Movable-Type.co.UK/scripts/geodesy/docs/module-osgridref.html>} and I{Charles Karney}'s C++ class U{OSGB<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1OSGB.html>}. OSGR provides geocoordinate references for UK mapping purposes, converted in 2015 to work with the C{WGS84} or the original C{OSGB36} datum. In addition, this implementation includes both the OS recommended and the Krüger-based method to convert between OSGR and geodetic coordinates (with keyword argument C{kTM} of function L{toOsgr}, method L{Osgr.toLatLon} and method C{toOsgr} of any ellipsoidal C{LatLon} class). See U{Transverse Mercator: Redfearn series<https://WikiPedia.org/wiki/Transverse_Mercator:_Redfearn_series>}, Karney's U{"Transverse Mercator with an accuracy of a few nanometers", 2011<https://Arxiv.org/pdf/1002.1417v3.pdf>} (building on U{"Konforme Abbildung des Erdellipsoids in der Ebene", 1912<https://bib.GFZ-Potsdam.DE/pub/digi/krueger2.pdf>}, U{"Die Mathematik der Gauß-Krueger-Abbildung", 2006<https://DE.WikiPedia.org/wiki/Gauß-Krüger-Koordinatensystem>}, U{A Guide<https://www.OrdnanceSurvey.co.UK/documents/resources/guide-coordinate-systems-great-britain.pdf>} and U{Ordnance Survey National Grid<https://WikiPedia.org/wiki/Ordnance_Survey_National_Grid>}. ''' # make sure int/int division yields float quotient, see .basics from __future__ import division as _; del _ # PYCHOK semicolon from pygeodesy.basics import halfs2, isbool, isfloat, map1, _xsubclassof from pygeodesy.constants import _1_0, _10_0, _N_2_0 # PYCHOK used! from pygeodesy.datums import Datums, _ellipsoidal_datum, _WGS84 # from pygeodesy.dms import parseDMS2 # _MODS from pygeodesy.ellipsoidalBase import LatLonEllipsoidalBase as _LLEB from pygeodesy.errors import _parseX, _TypeError, _ValueError, \ _xkwds, _xkwds_get from pygeodesy.fmath import Fdot, fpowers, Fsum # from pygeodesy.fsums import Fsum # from .fmath from pygeodesy.interns import MISSING, NN, _A_, _COLON_, _COMMA_, \ _COMMASPACE_, _DOT_, _ellipsoidal_, \ _latlon_, _not_, _SPACE_, _splituple from pygeodesy.lazily import _ALL_LAZY, _ALL_MODS as _MODS from pygeodesy.named import _NamedBase, nameof, _xnamed from pygeodesy.namedTuples import EasNor2Tuple, LatLon2Tuple, \ LatLonDatum3Tuple from pygeodesy.props import Property_RO, property_RO from pygeodesy.streprs import _EN_WIDE, enstr2, _enstr2m3, Fmt, \ _resolution10, unstr, _xzipairs from pygeodesy.units import Easting, Lam_, Lat, Lon, Northing, \ Phi_, Scalar, _10um, _100km from pygeodesy.utily import degrees90, degrees180, sincostan3, truncate from math import cos, radians, sin, sqrt __all__ = _ALL_LAZY.osgr __version__ = '22.09.12' _equivalent_ = 'equivalent' _OSGR_ = 'OSGR' _ord_A = ord(_A_) _TRIPS = 33 # .toLatLon convergence class _NG(object): '''Ordnance Survey National Grid parameters. ''' @Property_RO def a0(self): # equatoradius, scaled return self.ellipsoid.a * self.k0 @Property_RO def b0(self): # polaradius, scaled return self.ellipsoid.b * self.k0 @Property_RO def datum(self): # datum, Airy130 ellipsoid return Datums.OSGB36 @Property_RO def eas0(self): # False origin easting (C{meter}) return Easting(4 * _100km) @Property_RO def easX(self): # easting [0..extent] (C{meter}) return Easting(7 * _100km) @Property_RO def ellipsoid(self): # ellipsoid, Airy130 return self.datum.ellipsoid def forward2(self, latlon): # convert C{latlon} to (easting, norting), as I{Karney}'s # U{Forward<https://GeographicLib.SourceForge.io/C++/doc/OSGB_8hpp_source.html>} t = self.kTM.forward(latlon.lat, latlon.lon, lon0=self.lon0) e = t.easting + self.eas0 n = t.northing + self.nor0ffset return e, n @Property_RO def k0(self): # central scale (C{float}), like I{Karney}'s CentralScale # <https://GeographicLib.SourceForge.io/C++/doc/OSGB_8hpp_source.html> _0_9998268 = (9998268 - 10000000) / 10000000 return Scalar(_10_0**_0_9998268) # 0.9996012717... @Property_RO def kTM(self): # the L{KTransverseMercator} instance, like I{Karney}'s OSGBTM # <https://GeographicLib.SourceForge.io/C++/doc/OSGB_8cpp_source.html> return _MODS.ktm.KTransverseMercator(self.datum, lon0=0, k0=self.k0) @Property_RO def lam0(self): # True origin longitude C{radians} return Lam_(self.lon0) @Property_RO def lat0(self): # True origin latitude, 49°N return Lat(49.0) @Property_RO def lon0(self): # True origin longitude, 2°W return Lon(_N_2_0) @Property_RO def Mabcd(self): # meridional coefficients (a, b, c, d) n, n2, n3 = fpowers(self.ellipsoid.n, 3) M = (Fsum(4, 4 * n, 5 * n2, 5 * n3) / 4, Fsum( 24 * n, 24 * n2, 21 * n3) / 8, Fsum( 15 * n2, 15 * n3) / 8, (35 * n3 / 24)) return M def Mabcd0(self, a): # meridional arc, scaled c = a + self.phi0 s = a - self.phi0 R = Fdot(self.Mabcd, s, -sin(s) * cos(c), sin(s * 2) * cos(c * 2), -sin(s * 3) * cos(c * 3)) return float(R * self.b0) @Property_RO def nor0(self): # False origin northing (C{meter}) return Northing(-_100km) @Property_RO def nor0ffset(self): # like I{Karney}'s computenorthoffset # <https://GeographicLib.SourceForge.io/C++/doc/OSGB_8cpp_source.html> return self.nor0 - self.kTM.forward(self.lat0, 0).northing @Property_RO def norX(self): # northing [0..extent] (C{meter}) return Northing(13 * _100km) def nu_rho_eta3(self, sa): # 3-tuple (nu, nu / rho, eta2) E = self.ellipsoid # rho, nu = E.roc2_(sa) # .k0? s = E.e2s2(sa) # == 1 - E.e2 * sa**2 v = self.a0 / sqrt(s) # == nu, transverse roc # rho = .a0 * E.e21 / s**1.5 == v * E.e21 / s # r = v * E.e21 / s # == rho, meridional roc # nu / rho == v / (v * E.e21 / s) == s / E.e21 == ... s *= E._1_e21 # ... s * E._1_e21 == s * E.a2_b2 return v, s, (s - _1_0) # η2 = nu / rho - 1 @Property_RO def phi0(self): # True origin latitude C{radians} return Phi_(self.lat0) def reverse(self, osgr): # convert C{osgr} to (ellipsoidal} LatLon, as I{Karney}'s # U{Reverse<https://GeographicLib.SourceForge.io/C++/doc/OSGB_8hpp_source.html>} r = osgr._latlonTM if r is None: x = osgr.easting - self.eas0 y = osgr.northing - self.nor0ffset t = self.kTM.reverse(x, y, lon0=self.lon0) r = _LLEB(t.lat, t.lon, datum=self.datum, name=osgr.name) osgr._latlonTM = r return r _NG = _NG() # PYCHOK singleton class OSGRError(_ValueError): '''Error raised for a L{parseOSGR}, L{Osgr} or other OSGR issue. ''' pass class Osgr(_NamedBase): '''Ordnance Survey Grid References (OSGR) coordinates on the U{National Grid<https://www.OrdnanceSurvey.co.UK/ documents/resources/guide-to-nationalgrid.pdf>}. ''' _datum = _NG.datum # default datum (L{Datums.OSGB36}) _easting = 0 # Easting (C{meter}) _latlon = None # cached B{C{_toLatlon}} _latlonTM = None # cached B{C{_toLatlon kTM}} _northing = 0 # Nothing (C{meter}) _resolution = 0 # from L{parseOSGR} (C{meter}) def __init__(self, easting, northing, datum=None, name=NN, resolution=0): '''New L{Osgr} coordinate. @arg easting: Easting from the OS C{National Grid} origin (C{meter}). @arg northing: Northing from the OS C{National Grid} origin (C{meter}). @kwarg datum: Override default datum (C{Datums.OSGB36}). @kwarg name: Optional name (C{str}). @kwarg resolution: Optional resolution (C{meter}), C{0} for default. @raise OSGRError: Invalid or negative B{C{easting}} or B{C{northing}} or B{C{datum}} not an C{Datums.OSGB36} equivalent. ''' if datum: # PYCHOK no cover try: self._datum = _ellipsoidal_datum(datum) if self.datum != _NG.datum: raise ValueError(_not_(_NG.datum.name, _equivalent_)) except (TypeError, ValueError) as x: raise OSGRError(datum=datum, txt=str(x)) self._easting = Easting( easting, Error=OSGRError, high=_NG.easX) self._northing = Northing(northing, Error=OSGRError, high=_NG.norX) if name: self.name = name if resolution: self._resolution = _resolution10(resolution, Error=OSGRError) def __str__(self): return self.toStr(GD=True, sep=_SPACE_) @Property_RO def datum(self): '''Get the datum (L{Datum}). ''' return self._datum @Property_RO def easting(self): '''Get the easting (C{meter}). ''' return self._easting @Property_RO def falsing0(self): '''Get the C{OS National Grid} falsing (L{EasNor2Tuple}). ''' return EasNor2Tuple(_NG.eas0, _NG.nor0, name=_OSGR_) @property_RO def iteration(self): '''Get the most recent C{Osgr.toLatLon} iteration number (C{int}) or C{None} if not available/applicable. ''' return self._iteration @Property_RO def latlon0(self): '''Get the C{OS National Grid} origin (L{LatLon2Tuple}). ''' return LatLon2Tuple(_NG.lat, _NG.lon0, name=_OSGR_) @Property_RO def northing(self): '''Get the northing (C{meter}). ''' return self._northing def parse(self, strOSGR, name=NN): '''Parse an OSGR reference to a similar L{Osgr} instance. @arg strOSGR: The OSGR reference (C{str}), see function L{parseOSGR}. @kwarg name: Optional instance name (C{str}), overriding this name. @return: The similar instance (L{Osgr}) @raise OSGRError: Invalid B{C{strOSGR}}. ''' return parseOSGR(strOSGR, Osgr=self.classof, name=name or self.name) @property_RO def resolution(self): '''Get the OSGR resolution (C{meter}, power of 10) or C{0} if undefined. ''' return self._resolution def toLatLon(self, LatLon=None, datum=_WGS84, kTM=False, eps=_10um, **LatLon_kwds): '''Convert this L{Osgr} coordinate to an (ellipsoidal) geodetic point. @kwarg LatLon: Optional ellipsoidal class to return the geodetic point (C{LatLon}) or C{None}. @kwarg datum: Optional datum to convert to (L{Datum}, L{Ellipsoid}, L{Ellipsoid2}, L{Ellipsoid2} or L{a_f2Tuple}). @kwarg kTM: If C{True} use I{Karney}'s Krüger method from module L{ktm}, otherwise use the Ordnance Survey formulation (C{bool}). @kwarg eps: Tolerance for OS convergence (C{meter}). @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword arguments, ignored if C{B{LatLon} is None}. @return: A B{C{LatLon}} instance or if B{C{LatLon}} is C{None} a L{LatLonDatum3Tuple}C{(lat, lon, datum)}. @note: While OS grid references are based on the OSGB36 datum, the Ordnance Survey have deprecated the use of OSGB36 for lat-/longitude coordinates (in favour of WGS84). Hence, this method returns WGS84 by default with OSGB36 as an option, U{see<https://www.OrdnanceSurvey.co.UK/blog/2014/12/2>}. @note: The formulation implemented here due to Thomas, Redfearn, etc. is as published by the Ordnance Survey, but is inferior to Krüger as used by e.g. Karney 2011. @raise OSGRError: No convergence. @raise TypeError: If B{C{LatLon}} is not ellipsoidal or B{C{datum}} is invalid or conversion to B{C{datum}} failed. @example: >>> from pygeodesy import Datums, ellipsoidalVincenty as eV, Osgr >>> g = Osgr(651409.903, 313177.270) >>> p = g.toLatLon(eV.LatLon) # 52°39′28.723″N, 001°42′57.787″E >>> p = g.toLatLon(eV.LatLon, kTM=True) # 52°39′28.723″N, 001°42′57.787″E >>> # to obtain (historical) OSGB36 lat-/longitude point >>> p = g.toLatLon(eV.LatLon, datum=Datums.OSGB36) # 52°39′27.253″N, 001°43′04.518″E ''' NG = _NG if kTM: r = NG.reverse(self) elif self._latlon is None: e0 = self.easting - NG.eas0 n0 = m = self.northing - NG.nor0 _M = NG.Mabcd0 a0 = NG.a0 a = NG.phi0 _A = Fsum(a).fsum_ for self._iteration in range(1, _TRIPS): a = _A(m / a0) m = n0 - _M(a) # meridional arc if abs(m) < eps: break else: # PYCHOK no cover t = str(self) t = Fmt.PAREN(self.classname, repr(t)) t = _DOT_(t, self.toLatLon.__name__) t = unstr(t, eps=eps, kTM=kTM) raise OSGRError(Fmt.no_convergence(m), txt=t) sa, ca, ta = sincostan3(a) v, v_r, n2 = NG.nu_rho_eta3(sa) ta2 = ta**2 ta4 = ta2**2 ta *= v_r / 2 d = e0 / v d2 = d**2 a = (d2 * ta * (-1 + # Horner-like d2 / 12 * (Fsum( 5, 3 * ta2, -9 * ta2 * n2, n2) - d2 / 30 * Fsum(61, 90 * ta2, 45 * ta4)))).fsum_(a) b = (d / ca * (1 - # Horner-like d2 / 6 * (Fsum(v_r, 2 * ta2) - d2 / 20 * (Fsum( 5, 28 * ta2, 24 * ta4) + d2 / 42 * Fsum(61, 662 * ta2, 1320 * ta4, 720 * ta2 * ta4))))).fsum_(NG.lam0) r = _LLEB(degrees90(a), degrees180(b), datum=self.datum, name=self.name) r._iteration = self._iteration # only ellipsoidal LatLon self._latlon = r else: r = self._latlon return _ll2LatLon3(r, LatLon, datum, LatLon_kwds) @Property_RO def scale0(self): '''Get the C{OS National Grid} central scale (C{scalar}). ''' return _NG.k0 def toRepr(self, GD=None, fmt=Fmt.SQUARE, sep=_COMMASPACE_, **prec): # PYCHOK expected '''Return a string representation of this L{Osgr} coordinate. @kwarg GD: If C{bool}, in- or exclude the 2-letter grid designation and get the new B{C{prec}} behavior, otherwise if C{None}, default to the DEPRECATED definition C{B{prec}=5} I{for backward compatibility}. @kwarg fmt: Enclosing backets format (C{str}). @kwarg sep: Separator to join (C{str}) or C{None} to return an unjoined 2- or 3-C{tuple} of C{str}s. @kwarg prec: Precison C{B{prec}=0}, the number of I{decimal} digits (C{int}) or if negative, the number of I{units to drop}, like MGRS U{PRECISION <https://GeographicLib.SourceForge.io/C++/doc/GeoConvert.1.html#PRECISION>}. @return: This OSGR as (C{str}), C{"[G:GD, E:meter, N:meter]"} or if C{B{GD}=False} C{"[OSGR:easting,northing]"} or C{B{GD}=False} and C{B{prec} > 0} if C{"[OSGR:easting.d,northing.d]"}. @note: OSGR easting and northing values are truncated, not rounded. @raise OSGRError: If C{B{GD} not in (None, True, False)} or if C{B{prec} < -4} and C{B{GD}=False}. @raise ValueError: Invalid B{C{prec}}. ''' GD, prec = _GD_prec2(GD, fmt=fmt, sep=sep, **prec) if GD: t = self.toStr(GD=True, prec=prec, sep=None) t = _xzipairs('GEN', t, sep=sep, fmt=fmt) else: t = _COLON_(_OSGR_, self.toStr(GD=False, prec=prec)) if fmt: t = fmt % (t,) return t def toStr(self, GD=None, sep=NN, **prec): # PYCHOK expected '''Return this L{Osgr} coordinate as a string. @kwarg GD: If C{bool}, in- or exclude the 2-letter grid designation and get the new B{C{prec}} behavior, otherwise if C{None}, default to the DEPRECATED definition C{B{prec}=5} I{for backward compatibility}. @kwarg sep: Separator to join (C{str}) or C{None} to return an unjoined 2- or 3-C{tuple} of C{str}s. @kwarg prec: Precison C{B{prec}=0}, the number of I{decimal} digits (C{int}) or if negative, the number of I{units to drop}, like MGRS U{PRECISION <https://GeographicLib.SourceForge.io/C++/doc/GeoConvert.1.html#PRECISION>}. @return: This OSGR as (C{str}), C{"GD meter meter"} or if C{B{GD}=False} C{"easting,northing"} or if C{B{GD}=False} and C{B{prec} > 0} C{"easting.d,northing.d"} @note: OSGR easting and northing values are truncated, not rounded. @raise OSGRError: If C{B{GD} not in (None, True, False)} or if C{B{prec} < -4} and C{B{GD}=False}. @raise ValueError: Invalid B{C{prec}}. @example: >>> r = Osgr(651409, 313177) >>> str(r) # 'TG 5140 1317' >>> r.toStr() # 'TG5140913177' >>> r.toStr(GD=False) # '651409,313177' ''' def _i2c(i): if i > 7: i += 1 return chr(_ord_A + i) GD, prec = _GD_prec2(GD, sep=sep, **prec) if GD: E, e = divmod(self.easting, _100km) N, n = divmod(self.northing, _100km) E, N = int(E), int(N) if 0 > E or E > 6 or \ 0 > N or N > 12: raise OSGRError(E=E, e=e, N=N, n=n, prec=prec, sep=sep) N = 19 - N EN = _i2c( N - (N % 5) + (E + 10) // 5) + \ _i2c((N * 5) % 25 + (E % 5)) t = enstr2(e, n, prec, EN) s = sep elif prec <= -_EN_WIDE: raise OSGRError(GD=GD, prec=prec, sep=sep) else: t = enstr2(self.easting, self.northing, prec, dot=True, wide=_EN_WIDE + 1) s = sep if sep is None else (sep or _COMMA_) return t if s is None else s.join(t) def _GD_prec2(GD, **prec_et_al): '''(INTERNAL) Handle C{prec} backward compatibility. ''' if GD is None: # old C{prec} 5+ or neg prec = _xkwds_get(prec_et_al, prec=_EN_WIDE) GD = prec > 0 prec = (prec - _EN_WIDE) if GD else -prec elif isbool(GD): prec = _xkwds_get(prec_et_al, prec=0) else: raise OSGRError(GD=GD, **prec_et_al) return GD, prec def _ll2datum(ll, datum, name): '''(INTERNAL) Convert datum if needed. ''' if datum: try: if ll.datum != datum: ll = ll.toDatum(datum) except (AttributeError, TypeError, ValueError) as x: raise _TypeError(txt=str(x), datum=datum.name, **{name: ll}) return ll def _ll2LatLon3(ll, LatLon, datum, LatLon_kwds): '''(INTERNAL) Convert C{ll} to C{LatLon} ''' if LatLon is None: r = _ll2datum(ll, datum, LatLonDatum3Tuple.__name__) r = LatLonDatum3Tuple(r.lat, r.lon, r.datum) else: # must be ellipsoidal _xsubclassof(_LLEB, LatLon=LatLon) r = _ll2datum(ll, datum, LatLon.__name__) r = LatLon(r.lat, r.lon, datum=r.datum, **LatLon_kwds) if r._iteration != ll._iteration: r._iteration = ll._iteration return _xnamed(r, nameof(ll)) def parseOSGR(strOSGR, Osgr=Osgr, name=NN, **Osgr_kwds): '''Parse a string representing an OS Grid Reference, consisting of C{"[GD] easting northing"}. Accepts standard OS Grid References like "SU 387 148", with or without whitespace separators, from 2- up to 22-digit references, or all-numeric, comma-separated references in meters, for example "438700,114800". @arg strOSGR: An OSGR coordinate (C{str}). @kwarg Osgr: Optional class to return the OSGR coordinate (L{Osgr}) or C{None}. @kwarg name: Optional B{C{Osgr}} name (C{str}). @kwarg Osgr_kwds: Optional, additional B{C{Osgr}} keyword arguments, ignored if C{B{Osgr} is None}. @return: An (B{C{Osgr}}) instance or if B{C{Osgr}} is C{None} an L{EasNor2Tuple}C{(easting, northing)}. @raise OSGRError: Invalid B{C{strOSGR}}. @example: >>> r = parseOSGR('TG5140913177') >>> str(r) # 'TG 51409 13177' >>> r = parseOSGR('TG 51409 13177') >>> r.toStr() # 'TG5140913177' >>> r = parseOSGR('651409,313177') >>> r.toStr(sep=' ') # 'TG 51409 13177' >>> r.toStr(GD=False) # '651409,313177' ''' def _c2i(G): g = ord(G.upper()) - _ord_A if g > 7: g -= 1 if g < 0 or g > 25: raise ValueError return g def _OSGR(strOSGR, Osgr, name): s = _splituple(strOSGR.strip()) p = len(s) if not p: raise ValueError g = s[0] if p == 2 and isfloat(g): # "easting,northing" e, n, m = _enstr2m3(*s, wide=_EN_WIDE + 1) else: if p == 1: # "GReastingnorthing" s = halfs2(g[2:]) g = g[:2] elif p == 2: # "GReasting northing" s = g[2:], s[1] # for backward ... g = g[:2] # ... compatibility elif p != 3: raise ValueError else: # "GR easting northing" s = s[1:] e, n = map(_c2i, g) n, m = divmod(n, 5) E = ((e - 2) % 5) * 5 + m N = 19 - (e // 5) * 5 - n if 0 > E or E > 6 or \ 0 > N or N > 12: raise ValueError e, n, m = _enstr2m3(*s, wide=_EN_WIDE) e += E * _100km n += N * _100km if Osgr is None: _ = _MODS.osgr.Osgr(e, n, resolution=m) # validate r = EasNor2Tuple(e, n, name=name) else: r = Osgr(e, n, name=name, **_xkwds(Osgr_kwds, resolution=m)) return r return _parseX(_OSGR, strOSGR, Osgr, name, strOSGR=strOSGR, Error=OSGRError) def toOsgr(latlon, lon=None, kTM=False, datum=_WGS84, Osgr=Osgr, name=NN, # MCCABE 14 **prec_Osgr_kwds): '''Convert a lat-/longitude point to an OSGR coordinate. @arg latlon: Latitude (C{degrees}) or an (ellipsoidal) geodetic C{LatLon} point. @kwarg lon: Optional longitude in degrees (scalar or C{None}). @kwarg kTM: If C{True} use I{Karney}'s Krüger method from module L{ktm}, otherwise use the Ordnance Survey formulation (C{bool}). @kwarg datum: Optional datum to convert B{C{lat, lon}} from (L{Datum}, L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}). @kwarg Osgr: Optional class to return the OSGR coordinate (L{Osgr}) or C{None}. @kwarg name: Optional B{C{Osgr}} name (C{str}). @kwarg prec_Osgr_kwds: Optional L{truncate} precision C{B{prec}=ndigits} and/or additional B{C{Osgr}} keyword arguments, ignored if C{B{Osgr} is None}. @return: An (B{C{Osgr}}) instance or if B{C{Osgr}} is C{None} an L{EasNor2Tuple}C{(easting, northing)}. @note: If L{isint}C{(B{prec})} both easting and northing are L{truncate}d to the given number of digits. @raise OSGRError: Invalid B{C{latlon}} or B{C{lon}}. @raise TypeError: Non-ellipsoidal B{C{latlon}} or invalid B{C{datum}}, B{C{Osgr}}, B{C{Osgr_kwds}} or conversion to C{Datums.OSGB36} failed. @example: >>> p = LatLon(52.65798, 1.71605) >>> r = toOsgr(p) # [G:TG, E:51409, N:13177] >>> # for conversion of (historical) OSGB36 lat-/longitude: >>> r = toOsgr(52.65757, 1.71791, datum=Datums.OSGB36) >>> # alternatively and using Krüger >>> r = p.toOsgr(kTM=True) # [G:TG, E:51409, N:13177] ''' def _prec_kwds2(prec=MISSING, **kwds): return prec, kwds if lon is not None: try: lat, lon = _MODS.dms.parseDMS2(latlon, lon) latlon = _LLEB(lat, lon, datum=datum) except Exception as x: raise OSGRError(latlon=latlon, lon=lon, datum=datum, txt=str(x)) elif not isinstance(latlon, _LLEB): raise _TypeError(latlon=latlon, txt=_not_(_ellipsoidal_)) elif not name: # use latlon.name name = nameof(latlon) NG = _NG # convert latlon to OSGB36 first ll = _ll2datum(latlon, NG.datum, _latlon_) if kTM: e, n = NG.forward2(ll) else: try: a, b = ll.philam except AttributeError: a, b = map1(radians, ll.lat, ll.lon) sa, ca, ta = sincostan3(a) v, v_r, n2 = NG.nu_rho_eta3(sa) m0 = NG.Mabcd0(a) b -= NG.lam0 t = b * sa * v / 2 d = b * ca d2 = d**2 ta2 = -(ta**2) ta4 = ta2**2 e = (d * v * (1 + # Horner-like d2 / 6 * (Fsum(v_r, ta2) + d2 / 20 * Fsum(5, 18 * ta2, ta4, 14 * n2, 58 * n2 * ta2)))).fsum_(NG.eas0) n = (d * t * (1 + # Horner-like d2 / 12 * (Fsum( 5, ta2, 9 * n2) + d2 / 30 * Fsum(61, ta4, 58 * ta2)))).fsum_(m0, NG.nor0) p, kwds = _prec_kwds2(**prec_Osgr_kwds) if p is not MISSING: e = truncate(e, p) n = truncate(n, p) if Osgr is None: _ = _MODS.osgr.Osgr(e, n) # validate r = EasNor2Tuple(e, n) else: r = Osgr(e, n, **kwds) # datum=NG.datum if lon is None and isinstance(latlon, _LLEB): if kTM: r._latlonTM = latlon # XXX weakref(latlon)? else: r._latlon = latlon # XXX weakref(latlon)? return _xnamed(r, name or nameof(latlon)) if __name__ == '__main__': from pygeodesy.lazily import printf from random import random, seed from time import localtime seed(localtime().tm_yday) def _rnd(X, n): X -= 2 d = set() while len(d) < n: r = 1 + int(random() * X) if r not in d: d.add(r) yield r D = _NG.datum i = t = 0 t1 = t2 = 0, 0, 0, 0 for e in _rnd(_NG.easX, 256): for n in _rnd(_NG.norX, 512): p = False t += 1 g = Osgr(e, n) v = g.toLatLon(kTM=False, datum=D) k = g.toLatLon(kTM=True, datum=D) d = max(abs(v.lat - k.lat), abs(v.lon - k.lon)) if d > t1[2]: t1 = e, n, d, t p = True ll = _LLEB((v.lat + k.lat) / 2, (v.lon + k.lon) / 2, datum=D) v = ll.toOsgr(kTM=False) k = ll.toOsgr(kTM=True) d = max(abs(v.easting - k.easting), abs(v.northing - k.northing)) if d > t2[2]: t2 = ll.lat, ll.lon, d, t p = True if p: i += 1 printf('%5d: %s %s', i, 'll(%.2f, %.2f) %.3e %d' % t2, 'en(%d, %d) %.3e %d' % t1) printf('%d total %s', t, D.name) # **) MIT License # # Copyright (C) 2016-2022 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE. # % python3 -m pygeodesy.osgr # 1: ll(53.42, -0.59) 4.672e-07 1 en(493496, 392519) 2.796e-11 1 # 2: ll(60.86, -0.28) 2.760e-05 2 en(493496, 1220986) 2.509e-10 2 # 3: ll(61.41, -0.25) 3.045e-05 13 en(493496, 1281644) 2.774e-10 13 # 4: ll(61.41, -0.25) 3.045e-05 13 en(493496, 1192797) 3.038e-10 20 # 5: ll(61.41, -0.25) 3.045e-05 13 en(493496, 1192249) 3.073e-10 120 # 6: ll(61.55, -0.24) 3.120e-05 160 en(493496, 1192249) 3.073e-10 120 # 7: ll(61.55, -0.24) 3.122e-05 435 en(493496, 1192249) 3.073e-10 120 # 8: ll(61.57, -0.24) 3.130e-05 473 en(493496, 1192249) 3.073e-10 120 # 9: ll(58.66, -8.56) 8.084e-04 513 en(19711, 993800) 3.020e-06 513 # 10: ll(52.83, -7.65) 8.156e-04 518 en(19711, 993800) 3.020e-06 513 # 11: ll(51.55, -7.49) 8.755e-04 519 en(19711, 993800) 3.020e-06 513 # 12: ll(60.20, -8.87) 9.439e-04 521 en(19711, 1165686) 4.318e-06 521 # 13: ll(60.45, -8.92) 9.668e-04 532 en(19711, 1194002) 4.588e-06 532 # 14: ll(61.17, -9.08) 1.371e-03 535 en(19711, 1274463) 5.465e-06 535 # 15: ll(61.31, -9.11) 1.463e-03 642 en(19711, 1290590) 5.663e-06 642 # 16: ll(61.35, -9.12) 1.488e-03 807 en(19711, 1294976) 5.718e-06 807 # 17: ll(61.38, -9.13) 1.510e-03 929 en(19711, 1298667) 5.765e-06 929 # 18: ll(61.11, -9.24) 1.584e-03 11270 en(10307, 1268759) 6.404e-06 11270 # 19: ll(61.20, -9.26) 1.650e-03 11319 en(10307, 1278686) 6.545e-06 11319 # 20: ll(61.23, -9.27) 1.676e-03 11383 en(10307, 1282514) 6.600e-06 11383 # 21: ll(61.36, -9.30) 1.776e-03 11437 en(10307, 1297037) 6.816e-06 11437 # 22: ll(61.38, -9.30) 1.789e-03 11472 en(10307, 1298889) 6.844e-06 11472 # 23: ll(61.25, -9.39) 1.885e-03 91137 en(4367, 1285831) 7.392e-06 91137 # 24: ll(61.32, -9.40) 1.944e-03 91207 en(4367, 1293568) 7.519e-06 91207 # 25: ll(61.34, -9.41) 1.963e-03 91376 en(4367, 1296061) 7.561e-06 91376 # 26: ll(61.37, -9.41) 1.986e-03 91595 en(4367, 1298908) 7.608e-06 91595 # 131072 total OSGB36