### Navigation

- index
- pysmb 1.1.5 documentation »
- Module code »

# Source code for nmb.NetBIOSProtocol

    import os, logging, random, socket, time
    from twisted.internet import reactor, defer
    from twisted.internet.protocol import DatagramProtocol
    from base import NBNS

    class NetBIOSTimeout(Exception):
        """Raised in NBNSProtocol via Deferred.errback method when queryName method has timeout waiting for reply"""
        pass

    class NBNSProtocol(DatagramProtocol, NBNS):

        log = logging.getLogger('NMB.NBNSProtocol')

        def __init__(self, broadcast = True, listen_port = 0):
            """
            Instantiate a NBNSProtocol instance.

            This automatically calls reactor.listenUDP method to start listening for incoming packets, so you **must not** call the listenUDP method again.

            :param boolean broadcast: A boolean flag to indicate if we should setup the listening UDP port in broadcast mode
            :param integer listen_port: Specifies the UDP port number to bind to for listening. If zero, OS will automatically select a free port number.
            """
            self.broadcast = broadcast
            self.pending_trns = { }  # TRN ID -> ( expiry_time, name, Deferred instance )
            self.transport = reactor.listenUDP(listen_port, self)
            if self.broadcast:
                self.transport.getHandle().setsockopt(socket.SOL_SOCKET, socket.SO_BROADCAST, 1)
            reactor.callLater(1, self.cleanupPendingTrns)

        def datagramReceived(self, data, (host, port)):
            trn_id, ret = self.decodePacket(data)

            _, _, d = self.pending_trns.pop(trn_id, None)
            if d:
                d.callback(ret)

        def write(self, data, ip, port):
            # We don't use the transport.write method directly as it keeps raising DeprecationWarning for ip='<broadcast>'
            self.transport.getHandle().sendto(data, ( ip, port ))

        def queryName(self, name, ip = '', port = 137, timeout = 30):
            """
            Send a query on the network and hopes that if machine matching the *name* will reply with its IP address.

            :param string ip: If the NBNSProtocol instance was instianted with broadcast=True, then this parameter can be an empty string. We will leave it to the OS to determine an appropriate broadcast address.
                              If the NBNSProtocol instance was instianted with broadcast=False, then you should provide a target IP to send the query.
            :param integer port: The NetBIOS-NS port (IANA standard defines this port to be 137). You should not touch this parameter unless you know what you are doing.
            :param integer/float timeout: Number of seconds to wait for a reply, after which the returned Deferred instance will be called with a NetBIOSTimeout exception.
            :return: A *twisted.internet.defer.Deferred* instance. The callback function will be called with a list of IP addresses in dotted notation (aaa.bbb.ccc.ddd).
                     On timeout, the errback function will be called with a Failure instance wrapping around a NetBIOSTimeout exception
            """
            trn_id = random.randint(1, 0xFFFF)
            while True:
                if not self.pending_trns.has_key(trn_id):
                    break
                else:
                    trn_id = (trn_id + 1) & 0xFFFF

            data = self.prepareNameQuery(trn_id, name)
            if self.broadcast and not ip:
                ip = '<broadcast>'
            elif not ip:
                self.log.warning('queryName: ip parameter is empty. OS might not transmit this query to the network')

            self.write(data, ip, port)

            d = defer.Deferred()
            self.pending_trns[trn_id] = ( time.time()+timeout, name, d )
            return d

        def queryIPForName(self, ip, port = 137, timeout = 30):
            """
            Send a query to the machine with *ip* and hopes that the machine will reply back with its name.

            The implementation of this function is contributed by Jason Anderson.

            :param string ip: If the NBNSProtocol instance was instianted with broadcast=True, then this parameter can be an empty string. We will leave it to the OS to determine an appropriate broadcast address.
                              If the NBNSProtocol instance was instianted with broadcast=False, then you should provide a target IP to send the query.
            :param integer port: The NetBIOS-NS port (IANA standard defines this port to be 137). You should not touch this parameter unless you know what you are doing.
            :param integer/float timeout: Number of seconds to wait for a reply, after which the method will return None
            :return: A *twisted.internet.defer.Deferred* instance. The callback function will be called with a list of names of the machine at *ip*.
                     On timeout, the errback function will be called with a Failure instance wrapping around a NetBIOSTimeout exception
            """
            trn_id = random.randint(1, 0xFFFF)
            while True:
                if not self.pending_trns.has_key(trn_id):
                    break
                else:
                    trn_id = (trn_id + 1) & 0xFFFF

            data = self.prepareNetNameQuery(trn_id, name)
            self.write(data, ip, port)

            d = defer.Deferred()
            self.pending_trns[trn_id] = ( time.time()+timeout, name, d )
            return d

        def stopProtocol(self):
            DatagramProtocol.stopProtocol(self)

        def cleanupPendingTrns(self):
            now = time.time()
            for trn_id, ( expiry_time, name, d ) in self.pending_trns.items():
                if expiry_time < now:
                    del self.pending_trns[trn_id]
                    try:
                        d.errback(NetBIOSTimeout(name))
                    except: pass

            if self.transport:
                reactor.callLater(1, self.cleanupPendingTrns)

### Navigation

- index
- pysmb 1.1.5 documentation »
- Module code »