### Navigation

- index
- modules |
- pywws 13.03_7f9fc90 documentation »
- Code du module »

# Code source de USBQualityTest

    #!/usr/bin/env python

    # pywws - Python software for USB Wireless Weather Stations
    # http://github.com/jim-easterbrook/pywws
    # Copyright (C) 2008-13  Jim Easterbrook  jim@jim-easterbrook.me.uk

    # This program is free software; you can redistribute it and/or
    # modify it under the terms of the GNU General Public License
    # as published by the Free Software Foundation; either version 2
    # of the License, or (at your option) any later version.

    # This program is distributed in the hope that it will be useful,
    # but WITHOUT ANY WARRANTY; without even the implied warranty of
    # MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
    # GNU General Public License for more details.

    # You should have received a copy of the GNU General Public License
    # along with this program; if not, write to the Free Software
    # Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA  02110-1301, USA.

    """Test quality of USB connection to weather station

    ::

    %s

    The USB link to my weather station is not 100%% reliable. The data
    read from the station by the computer is occasionally corrupted,
    perhaps by interference. I've been trying to solve this by putting
    ferrite beads around the USB cable and relocating possible
    interference sources such as external hard drives. All without any
    success so far.

    This program tests the USB connection for errors by continuously
    reading the entire weather station memory (except for those parts that
    may be changing) looking for errors. Each 32-byte block is read twice,
    and if the two readings differ a warning message is displayed. Also
    displayed are the number of blocks read, and the number of errors
    found.

    I typically get one or two errors per hour, so the test needs to be
    run for several hours to produce a useful measurement. Note that other
    software that accesses the weather station (such as :doc:`Hourly` or
    :doc:`LiveLog`) must not be run while the test is in progress.

    If you run this test and get no errors at all, please let me know.
    There is something good about your setup and I'd love to know what it
    is!

    """

    __docformat__ = "restructuredtext en"

    __usage__ = """
     usage: python USBQualityTest.py [options]
     options are:
      -h | --help           display this help
      -v | --verbose        increase amount of reassuring messages
                            (repeat for even more messages e.g. -vvv)
    """

    __doc__ %= __usage__
    __usage__ = __doc__.split('\n')[0] + __usage__

    import getopt
    import sys

    from pywws.Logger import ApplicationLogger
    from pywws import WeatherStation

    def main(argv=None):
        if argv is None:
            argv = sys.argv
        try:
            opts, args = getopt.getopt(argv[1:], "hv", ('help', 'verbose'))
        except getopt.error, msg:
            print >>sys.stderr, 'Error: %s\n' % msg
            print >>sys.stderr, __usage__.strip()
            return 1
        # check arguments
        if len(args) != 0:
            print >>sys.stderr, 'Error: no arguments allowed\n'
            print >>sys.stderr, __usage__.strip()
            return 2
        # process options
        verbose = 0
        for o, a in opts:
            if o in ('-h', '--help'):
                print __usage__.strip()
                return 0
            elif o in ('-v', '--verbose'):
                verbose += 1
        # do it!
        logger = ApplicationLogger(verbose)
        ws = WeatherStation.weather_station()
        fixed_block = ws.get_fixed_block()
        if not fixed_block:
            print "No valid data block found"
            return 3
        # loop
        ptr = ws.data_start
        total_count = 0
        bad_count = 0
        while True:
            if total_count % 1000 == 0:
                active = ws.current_pos()
            while True:
                ptr += 0x20
                if ptr >= 0x10000:
                    ptr = ws.data_start
                if active < ptr - 0x10 or active >= ptr + 0x20:
                    break
            result_1 = ws._read_block(ptr, retry=False)
            result_2 = ws._read_block(ptr, retry=False)
            if result_1 != result_2:
                logger.warning('read_block changing %06x', ptr)
                logger.warning('  %s', str(result_1))
                logger.warning('  %s', str(result_2))
                bad_count += 1
            total_count += 1
            print "\r %d/%d " % (bad_count, total_count),
            sys.stdout.flush()
        print ''
        return 0

    if __name__ == "__main__":
        try:
            sys.exit(main())
        except KeyboardInterrupt:
            pass

### Navigation

- index
- modules |
- pywws 13.03_7f9fc90 documentation »
- Code du module »