### Navigation

- index
- modules |
- pywws 13.03_7f9fc90 documentation »
- Code du module »

# Code source de pywws.LogData

    #!/usr/bin/env python

    # pywws - Python software for USB Wireless Weather Stations
    # http://github.com/jim-easterbrook/pywws
    # Copyright (C) 2008-13  Jim Easterbrook  jim@jim-easterbrook.me.uk

    # This program is free software; you can redistribute it and/or
    # modify it under the terms of the GNU General Public License
    # as published by the Free Software Foundation; either version 2
    # of the License, or (at your option) any later version.

    # This program is distributed in the hope that it will be useful,
    # but WITHOUT ANY WARRANTY; without even the implied warranty of
    # MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
    # GNU General Public License for more details.

    # You should have received a copy of the GNU General Public License
    # along with this program; if not, write to the Free Software
    # Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA  02110-1301, USA.

    """Save weather station history to file
    ::

    %s

    This program / module gets data from the weather station's memory and
    stores it to file. Each time it is run it fetches all data that is
    newer than the last stored data, so it only needs to be run every hour
    or so. As the weather station typically stores two weeks' readings
    (depending on the logging interval), LogData.py could be run quite
    infrequently if you don't need up-to-date data.

    There is no date or time information in the raw weather station data,
    so LogData.py creates a time stamp for each reading. It uses the
    computer's clock, rather than the weather station clock which can not
    be read accurately by the computer. A networked computer should have
    its clock set accurately by `ntp
    <http://en.wikipedia.org/wiki/Network_Time_Protocol>`_.

    Synchronisation with the weather station is achieved by waiting for a
    change in the current data. There are two levels of synchronisation,
    set by the config file or a command line option. Level 0 is quicker,
    but is only accurate to around twelve seconds. Level 1 waits until the
    weather station stores a new logged record, and gets time stamps
    accurate to a couple of seconds. Note that this could take a long
    time, if the logging interval is greater than the recommended five
    minutes.

    """

    __docformat__ = "restructuredtext en"
    __usage__ = """
     usage: python RunModule.py LogData [options] data_dir
     options are:
      -h   | --help     display this help
      -c   | --clear    clear weather station's memory full indicator
      -s n | --sync n   set quality of synchronisation to weather station (0 or 1)
      -v   | --verbose  increase number of informative messages
     data_dir is the root directory of the weather data
    """
    __doc__ %= __usage__
    __usage__ = __doc__.split('\n')[0] + __usage__

    from datetime import datetime, timedelta
    import getopt
    import logging
    import os
    import sys
    import time

    from . import DataStore
    from .Logger import ApplicationLogger
    from .TimeZone import Local
    from . import WeatherStation

    def Catchup(ws, logger, raw_data, last_date, last_ptr):
        fixed_block = ws.get_fixed_block(unbuffered=True)
        # get time to go back to
        last_stored = raw_data.before(datetime.max)
        if last_stored == None:
            last_stored = datetime.min
        if datetime.utcnow() < last_stored:
            raise ValueError('Computer time is earlier than last stored data')
        last_stored += timedelta(seconds=fixed_block['read_period'] * 30)
        # data_count includes record currently being updated every 48 seconds
        max_count = fixed_block['data_count'] - 1
        count = 0
        while last_date > last_stored and count < max_count:
            data = ws.get_data(last_ptr)
            if data['delay'] is None or data['delay'] > 30:
                logger.error('invalid data at %04x, %s',
                             last_ptr, last_date.isoformat(' '))
                last_date -= timedelta(minutes=fixed_block['read_period'])
            else:
                raw_data[last_date] = data
                count += 1
                last_date -= timedelta(minutes=data['delay'])
            last_ptr = ws.dec_ptr(last_ptr)
        if count > 0:
            logger.info("%d catchup records", count)

    def CheckFixedBlock(ws, params, logger):
        fixed_block = ws.get_fixed_block(unbuffered=True)
        if not fixed_block:
            return None
        # check clocks
        try:
            s_time = DataStore.safestrptime(
                fixed_block['date_time'], '%Y-%m-%d %H:%M')
        except Exception:
            s_time = None
        if s_time:
            c_time = datetime.now().replace(second=0, microsecond=0)
            diff = abs(s_time - c_time)
            if diff > timedelta(minutes=2):
                logger.warning(
                    "Computer and weather station clocks disagree by %s (H:M:S).", str(diff))
        # store weather station type
        params.set('config', 'ws type', ws.ws_type)
        # store info from fixed block
        pressure_offset = fixed_block['rel_pressure'] - fixed_block['abs_pressure']
        old_offset = eval(params.get('fixed', 'pressure offset', 'None'))
        if old_offset and abs(old_offset - pressure_offset) > 0.01:
            # re-read fixed block, as can get incorrect values
            logger.warning('Re-read fixed block')
            fixed_block = ws.get_fixed_block(unbuffered=True)
            if not fixed_block:
                return None
            pressure_offset = fixed_block['rel_pressure'] - fixed_block['abs_pressure']
        if old_offset and abs(old_offset - pressure_offset) > 0.01:
            logger.warning(
                'Pressure offset change: %g -> %g', old_offset, pressure_offset)
        params.set('fixed', 'pressure offset', '%g' % (pressure_offset))
        params.set('fixed', 'fixed block', str(fixed_block))
        return fixed_block

    def LogData(params, raw_data, sync=None, clear=False):
        logger = logging.getLogger('pywws.LogData')
        # connect to weather station
        ws_type = params.get('fixed', 'ws type')
        if ws_type:
            params._config.remove_option('fixed', 'ws type')
            params.set('config', 'ws type', ws_type)
        ws_type = params.get('config', 'ws type', 'Unknown')
        ws = WeatherStation.weather_station(ws_type=ws_type, params=params)
        fixed_block = CheckFixedBlock(ws, params, logger)
        if not fixed_block:
            logger.error("Invalid data from weather station")
            return 3
        # check for valid weather station type
        if ws.ws_type not in ('1080', '3080'):
            print "Unknown weather station type. Please edit weather.ini"
            print "and set 'ws type' to '1080' or '3080', as appropriate."
            if fixed_block['lux_wm2_coeff'] == 0.0:
                print "Your station is probably a '1080' type."
            else:
                print "Your station is probably a '3080' type."
            sys.exit(1)
        # get sync config value
        if sync is None:
            if fixed_block['read_period'] <= 5:
                sync = int(params.get('config', 'logdata sync', '1'))
            else:
                sync = int(params.get('config', 'logdata sync', '0'))
        # get address and date-time of last complete logged data
        logger.info('Synchronising to weather station')
        range_hi = datetime.max
        range_lo = datetime.min
        last_delay = ws.get_data(ws.current_pos())['delay']
        if last_delay == 0:
            prev_date = datetime.min
        else:
            prev_date = datetime.utcnow()
        for data, last_ptr, logged in ws.live_data(logged_only=(sync > 1)):
            last_date = data['idx']
            logger.debug('Reading time %s', last_date.strftime('%H:%M:%S'))
            if logged:
                break
            if sync < 2 and ws._station_clock:
                err = last_date - datetime.fromtimestamp(ws._station_clock)
                last_date -= timedelta(
                    minutes=data['delay'], seconds=err.seconds % 60)
                logger.debug('log time %s', last_date.strftime('%H:%M:%S'))
                last_ptr = ws.dec_ptr(last_ptr)
                break
            if sync < 1:
                hi = last_date - timedelta(minutes=data['delay'])
                if last_date - prev_date > timedelta(seconds=50):
                    lo = hi - timedelta(seconds=60)
                elif data['delay'] == last_delay:
                    lo = hi - timedelta(seconds=60)
                    hi = hi - timedelta(seconds=48)
                else:
                    lo = hi - timedelta(seconds=48)
                last_delay = data['delay']
                prev_date = last_date
                range_hi = min(range_hi, hi)
                range_lo = max(range_lo, lo)
                err = (range_hi - range_lo) / 2
                last_date = range_lo + err
                logger.debug('est log time %s +- %ds (%s..%s)',
                             last_date.strftime('%H:%M:%S'), err.seconds,
                             lo.strftime('%H:%M:%S'), hi.strftime('%H:%M:%S'))
                if err < timedelta(seconds=15):
                    last_ptr = ws.dec_ptr(last_ptr)
                    break
        # go back through stored data, until we catch up with what we've already got
        logger.info('Fetching data')
        Catchup(ws, logger, raw_data, last_date, last_ptr)
        if clear:
            logger.info('Clearing weather station memory')
            ptr = ws.fixed_format['data_count'][0]
            ws.write_data([(ptr, 1), (ptr+1, 0)])

    def main(argv=None):
        if argv is None:
            argv = sys.argv
        try:
            opts, args = getopt.getopt(
                argv[1:], "hcs:v", ('help', 'clear', 'sync=', 'verbose'))
        except getopt.error, msg:
            print >>sys.stderr, 'Error: %s\n' % msg
            print >>sys.stderr, __usage__.strip()
            return 1
        # process options
        clear = False
        sync = None
        verbose = 0
        for o, a in opts:
            if o in ('-h', '--help'):
                print __usage__.strip()
                return 0
            elif o in ('-c', '--clear'):
                clear = True
            elif o in ('-s', '--sync'):
                sync = int(a)
            elif o in ('-v', '--verbose'):
                verbose += 1
        # check arguments
        if len(args) != 1:
            print >>sys.stderr, 'Error: 1 argument required\n'
            print >>sys.stderr, __usage__.strip()
            return 2
        logger = ApplicationLogger(verbose)
        root_dir = args[0]
        return LogData(
            DataStore.params(root_dir), DataStore.data_store(root_dir),
            sync=sync, clear=clear)

    if __name__ == "__main__":
        sys.exit(main())

### Navigation

- index
- modules |
- pywws 13.03_7f9fc90 documentation »
- Code du module »