# Source code for quat

    '''
    Functions for working with quaternions. Note that all the functions also
    work on arrays, and can deal with full quaternions as well as with
    quaternion vectors.

    A "Quaternion" class is defined, with

    - operator overloading for mult, div, and inv.
    - indexing

    '''

    '''
    author: Thomas Haslwanter
    date:   April 2016
    ver:    0.1
    '''

    import numpy as np
    import matplotlib.pyplot as plt

    from scipy import signal

    # The following construct is required since I want to run the module as a script
    # inside the thLib-directory
    import os
    import sys
    PACKAGE_PARENT = '..'
    SCRIPT_DIR = os.path.realpath(os.path.dirname(__file__))
    sys.path.append(os.path.normpath(os.path.join(SCRIPT_DIR, PACKAGE_PARENT)))

    import rotmat

    pi = np.pi

    class Quaternion():
        '''Quaternion class, with multiplocation, division, and inverse.
        A Quaternion can be created from vectors, rotation matrices,
        or from Fick-angles, Helmholtz-angles, or Euler angles (in deg).
        It provides

        * operator overloading for mult, div, and inv.
        * indexing
        * access to the data, in the attribute *values*.

        Parameters
        ----------
        inData : ndarray
                 Contains the data in one of the following formats:

                 * vector : (3 x n) or (4 x n) array, containing the quaternion values
                 * rotmat : array, shape (3,3) or (N,9)
                            single rotation matrix, or matrix with rotation-matrix elements.
                 * Fick : (3 x n) array, containing (psi, phi, theta) rotations about
                                    the (1,2,3) axes [deg] (Fick sequence)
                 * Helmholtz : (3 x n) array, containing (psi, phi, theta) rotations about
                                    the (1,2,3) axes [deg] (Helmholtz sequence)
                 * Euler : (3 x n) array, containing (alpha, beta, gamma) rotations about
                                    the (3,1,3) axes [deg] (Euler sequence)
        inType : string
               Specifies the type of the input and has to have one of the following values
               'vector'[Default], 'rotmat', 'Fick', 'Helmholtz', 'Euler'

        Attributes
        ----------

        values : (4 x n) array
            quaternion values

        Methods
        -------

        inv()
            Inverse of the quaterion
        export(to='rotmat')
            Export to one of the following formats: 'rotmat', 'Euler', 'Fick', 'Helmholtz'

        Notes
        -----
        .. math::
              \\vec {q}_{Euler}  = \\left[ {\\begin{array}{*{20}{c}}
              {\\cos \\frac{\\alpha }{2}*\\cos \\frac{\\beta }{2}*\\cos \\frac{\\gamma }{2} - \\sin \\frac{\\alpha }{2}\\cos \\frac{\\beta }{2}\\sin \\frac{\\gamma }{2}} \\\\
              {\\cos \\frac{\\alpha }{2}*\\sin \\frac{\\beta }{2}*\\cos \\frac{\\gamma }{2} + \\sin \\frac{\\alpha }{2}\\sin \\frac{\\beta }{2}\\sin \\frac{\\gamma }{2}} \\\\
              {\\cos \\frac{\\alpha }{2}*\\sin \\frac{\\beta }{2}*\\sin \\frac{\\gamma }{2} - \\sin \\frac{\\alpha }{2}\\sin \\frac{\\beta }{2}\\cos \\frac{\\gamma }{2}} \\\\
              {\\cos \\frac{\\alpha }{2}*\\cos \\frac{\\beta }{2}*\\sin \\frac{\\gamma }{2} + \\sin \\frac{\\alpha }{2}\\cos \\frac{\\beta }{2}\\cos \\frac{\\gamma }{2}}
            \\end{array}} \\right]

        .. math::
              \\vec {q}_{Fick}  = \\left[ {\\begin{array}{*{20}{c}}
              {\\cos \\frac{\\psi }{2}*\\cos \\frac{\\phi }{2}*\\cos \\frac{\\theta }{2} + \\sin \\frac{\\psi }{2}\\sin \\frac{\\phi }{2}\\sin \\frac{\\theta }{2}} \\\\
              {\\sin \\frac{\\psi }{2}*\\cos \\frac{\\phi }{2}*\\cos \\frac{\\theta }{2} - \\cos \\frac{\\psi }{2}\\sin \\frac{\\phi }{2}\\sin \\frac{\\theta }{2}} \\\\
              {\\cos \\frac{\\psi }{2}*\\sin \\frac{\\phi }{2}*\\cos \\frac{\\theta }{2} + \\sin \\frac{\\psi }{2}\\cos \\frac{\\phi }{2}\\sin \\frac{\\theta }{2}} \\\\
              {\\cos \\frac{\\psi }{2}*\\cos \\frac{\\phi }{2}*\\sin \\frac{\\theta }{2} - \\sin \\frac{\\psi }{2}\\sin \\frac{\\phi }{2}\\cos \\frac{\\theta }{2}}
            \\end{array}} \\right]

        .. math::
              \\vec {q}_{Helmholtz}  = \\left[ {\\begin{array}{*{20}{c}}
              {\\cos \\frac{\\psi }{2}*\\cos \\frac{\\phi }{2}*\\cos \\frac{\\theta }{2} - \\sin \\frac{\\psi }{2}\\sin \\frac{\\phi }{2}\\sin \\frac{\\theta }{2}} \\\\
              {\\sin \\frac{\\psi }{2}*\\cos \\frac{\\phi }{2}*\\cos \\frac{\\theta }{2} + \\cos \\frac{\\psi }{2}\\sin \\frac{\\phi }{2}\\sin \\frac{\\theta }{2}} \\\\
              {\\cos \\frac{\\psi }{2}*\\sin \\frac{\\phi }{2}*\\cos \\frac{\\theta }{2} + \\sin \\frac{\\psi }{2}\\cos \\frac{\\phi }{2}\\sin \\frac{\\theta }{2}} \\\\
              {\\cos \\frac{\\psi }{2}*\\cos \\frac{\\phi }{2}*\\sin \\frac{\\theta }{2} - \\sin \\frac{\\psi }{2}\\sin \\frac{\\phi }{2}\\cos \\frac{\\theta }{2}}
            \\end{array}} \\right]

        Examples
        --------

        >>> q = Quaternion(array([[0,0,0.1],
                                  [0,0,0.2],
                                  [0,0,0.5]]))
        >>> p = Quaternion(array([0,0,0.2]))
        >>> fick = Quaternion( array([[0,0,10],
                                      [0,10,10]]), 'Fick')
        >>> combined = p * q
        >>> divided = q / p
        >>> extracted = q[1:2]
        >>> len(q)
        >>> data = q.values
        >>> 2
        >>> inv(q)

        '''

        def __init__(self, inData, inType='vector'):
            '''Initialization'''

            if inType.lower() == 'vector':
                if isinstance(inData, np.ndarray) or isinstance(inData, list):
                    self.values = vect2quat(inData)
                elif isinstance(inData, Quaternion):
                    self.values = inData.values
                else:
                    raise TypeError('Quaternions can only be based on ndarray or Quaternions!')

            elif inType.lower() == 'rotmat':
                '''Conversion from rotation matrices to quaternions.'''
                self.values = rotmat2quat(inData)

            elif inType.lower() == 'euler':
                ''' Conversion from Euler angles to quaternions.
                (a,b,g) stands for (alpha, beta, gamma) '''

                inData[inData<0] += 360
                inData = np.deg2rad(inData/2)

                (ca, cb, cg) = np.cos(inData.T)
                (sa, sb, sg) = np.sin(inData.T)

                self.values = np.vstack( (ca*cb*cg - sa*cb*sg,
                                          ca*sb*cg + sa*sb*sg,
                                          ca*sb*sg - sa*sb*cg,
                                          ca*cb*sg + sa*cb*cg) ).T
            elif inType.lower() == 'fick':
                ''' Conversion from Fick angles to quaternions.
                (p,f,t) stands for (psi, phi, theta) '''

                inData[inData<0] += 360
                inData = np.deg2rad(inData/2)

                (cp, cf, ct) = np.cos(inData.T)
                (sp, sf, st) = np.sin(inData.T)

                self.values = np.vstack( (cp*cf*ct + sp*sf*st,
                                          sp*cf*ct - cp*sf*st,
                                          cp*sf*ct + sp*cf*st,
                                          cp*cf*st - sp*sf*ct) ).T

            elif inType.lower() == 'helmholtz':
                ''' Conversion from Helmholtz angles to quaternions.
                (p,f,t) stands for (psi, phi, theta) '''

                inData[inData<0] += 360
                inData = np.deg2rad(inData/2)

                (cp, cf, ct) = np.cos(inData.T)
                (sp, sf, st) = np.sin(inData.T)

                self.values = np.vstack( (cp*cf*ct - sp*sf*st,
                                          sp*cf*ct + cp*sf*st,
                                          cp*sf*ct + sp*cf*st,
                                          cp*cf*st - sp*sf*ct ) ).T

        def __len__(self):
            '''The "length" is given by the number of quaternions.'''
            return len(self.values)

        def __mul__(self, other):
            '''Operator overloading for multiplication.'''
            if isinstance(other, int) or isinstance(other, float):
                return Quaternion(self.values * other)
            else:
                return Quaternion(quatmult(self.values, other.values))

        def __div__(self, other):
            '''Operator overloading for division.'''
            if isinstance(other, int) or isinstance(other, float):
                return Quaternion(self.values / other)
            else:
                return Quaternion(quatmult(self.values, quatinv(other.values)))

        def __truediv__(self, other):
            '''Operator overloading for division.'''
            if isinstance(other, int) or isinstance(other, float):
                return Quaternion(self.values / other)
            else:
                return Quaternion(quatmult(self.values, quatinv(other.values)))

        def __getitem__(self, select):
            return Quaternion(self.values[select])

        def __setitem__(self, select, item):
            self.values[select] = vect2quat(item)

        #def __delitem__(self, select):
            #np.delete(self.values, select, axis=0)

        def inv(self):
            '''Inverse of a quaternion.'''
            return Quaternion(quatinv(self.values))

        def __repr__(self):
            return 'Quaternion ' + str(self.values)

        def export(self, to='rotmat'):
            '''
            Conversion to other formats. May be slow for "Fick", "Helmholtz", and "Euler".

            Parameters
            ----------
            to : string
                content of returned values

                * 'rotmat' : rotation matrices (default), each flattened to a 9-dim vector
                * 'Euler' : Euler angles
                * 'Fick' : Fick angles
                * 'Helmholtz' : Helmholtz angles
                * 'vector' : vector part of the quaternion

            Returns
            -------
            ndarray, with the specified content

            Examples
            --------

            >>> q = Quaternion([0,0.2,0.1])
            >>> rm = q.export()
            >>> fick = q.export('Fick')

            '''
            if to.lower() == 'rotmat' :
               return quat2rotmat(self.values)

            if to.lower() == 'vector' :
                return self.values[:,1:]

            if to.lower == 'euler':
                Euler = np.zeros((len(self),3))
                rm = self.export()
                if rm.shape == (3,3):
                    rm = rm.reshape((1,9))
                for ii in range(len(self)):
                   Euler[ii,:] = rotmat.rotmat2Euler(rm[ii].reshape((3,3)))
                return Euler

            if to.lower() == 'fick':
                Fick = np.zeros((len(self),3))
                rm = self.export()
                if rm.shape == (3,3):
                    rm = rm.reshape((1,9))
                for ii in range(len(self)):
                   Fick[ii,:] = rotmat.rotmat2Fick(rm[ii].reshape((3,3)))
                return Fick

            if to.lower() == 'helmholtz':
                Helmholtz = np.zeros((len(self),3))
                rm = self.export()
                if rm.shape == (3,3):
                    rm = rm.reshape((1,9))
                for ii in range(len(self)):
                   Helmholtz[ii,:] = rotmat.rotmat2Helmholtz(rm[ii].reshape((3,3)))
                return Helmholtz

    def deg2quat(inDeg):
        '''
        Convert axis-angles or plain degree into the corresponding quaternion values.
        Can be used with a plain number or with an axis angle.

        Parameters
        ----------
        inDeg : float or (N,3)
            quaternion magnitude or quaternion vectors.

        Returns
        -------
        outQuat : float or array (N,3)
            number or quaternion vector.

        Notes
        -----

        .. math::
            | \\vec{q} | = sin(\\theta/2)

        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------
        >>> quat.deg2quat(array([[10,20,30], [20,30,40]]))
        array([[ 0.08715574,  0.17364818,  0.25881905],
           [ 0.17364818,  0.25881905,  0.34202014]])

        >>> quat.deg2quat(10)
        0.087155742747658166

        '''
        deg = (inDeg+180)%360-180
        return np.sin(0.5 * deg * pi/180)

    def quatconj(q):
        ''' Conjugate quaternion

        Parameters
        ----------
        q: array_like, shape ([3,4],) or (N,[3/4])
            quaternion or quaternion vectors

        Returns
        -------
        qconj : conjugate quaternion(s)

        Examples
        --------
        >>>  quat.quatconj([0,0,0.1])
        array([ 0., -0., -0., -1.])

        >>> quat.quatconj([[cos(0.1),0,0,sin(0.1)],
        >>>    [cos(0.2), 0, sin(0.2), 0]])
        array([[ 0.99500417, -0.        , -0.        , -0.09983342],
               [ 0.98006658, -0.        , -0.19866933, -0.        ]])

        '''

        q = np.atleast_2d(q)
        if q.shape[1]==3:
            q = vect2quat(q)

        qConj = q * np.r_[1, -1,-1,-1]

        if q.shape[0]==1:
            qConj=qConj.ravel()

        return qConj

    def quatinv(q):
        ''' Quaternion inversion

        Parameters
        ----------
        q: array_like, shape ([3,4],) or (N,[3/4])
            quaternion or quaternion vectors

        Returns
        -------
        qinv : inverse quaternion(s)

        Notes
        -----

        .. math::
              q^{-1} = \\frac{q_0 - \\vec{q}}{|q|^2}

        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------
        >>>  quat.quatinv([0,0,0.1])
        array([[-0. , -0. , -0.1]])

        >>> quat.quatinv([[cos(0.1),0,0,sin(0.1)],
        >>> [cos(0.2),0,sin(0.2),0]])
        array([[ 0.99500417, -0.        , -0.        , -0.09983342],
               [ 0.98006658, -0.        , -0.19866933, -0.        ]])
        '''

        q = np.atleast_2d(q)
        if q.shape[1]==3:
            return -q
        else:
            qLength = np.sum(q**2, 1)
            qConj = q * np.r_[1, -1,-1,-1]
            return (qConj.T / qLength).T

    def quatmult(p,q):
        '''
        Quaternion multiplication: Calculates the product of two quaternions r = p * q
        If one of both of the quaterions have only three columns,
        the scalar component is calculated such that the length
        of the quaternion is one.
        The lengths of the quaternions have to match, or one of
        the two quaternions has to have the length one.
        If both p and q only have 3 components, the returned quaternion
        also only has 3 components (i.e. the quaternion vector)

        Parameters
        ----------
        p,q : array_like, shape ([3,4],) or (N,[3,4])
            quaternions or quaternion vectors

        Returns
        -------
        r : quaternion or quaternion vector (if both
            p and q are contain quaternion vectors).

        Notes
        -----

        .. math::
            q \\circ p = \\sum\\limits_{i=0}^3 {q_i I_i} * \\sum\\limits_{j=0}^3 \\
            {p_j I_j} = (q_0 p_0 - \\vec{q} \\cdot \\vec{p}) + (q_0 \\vec{p} + p_0 \\
            \\vec{q} + \\vec{q} \\times \\vec{p}) \\cdot \\vec{I}

        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------
        >>> p = [cos(0.2), 0, 0, sin(0.2)]
        >>> q = [[0, 0, 0.1],
        >>>    [0, 0.1, 0]]
        >>> r = quat.quatmult(p,q)

        '''

        flag3D = False
        p = np.atleast_2d(p)
        q = np.atleast_2d(q)
        if p.shape[1]==3 & q.shape[1]==3:
            flag3D = True

        if len(p) != len(q):
            assert (len(p)==1 or len(q)==1), \
                'Both arguments in the quaternion multiplication must have the same number of rows, unless one has only one row.'

        p = vect2quat(p).T
        q = vect2quat(q).T

        if np.prod(np.shape(p)) > np.prod(np.shape(q)):
            r=np.zeros(np.shape(p))
        else:
            r=np.zeros(np.shape(q))

        r[0] = p[0]*q[0] - p[1]*q[1] - p[2]*q[2] - p[3]*q[3]
        r[1] = p[1]*q[0] + p[0]*q[1] + p[2]*q[3] - p[3]*q[2]
        r[2] = p[2]*q[0] + p[0]*q[2] + p[3]*q[1] - p[1]*q[3]
        r[3] = p[3]*q[0] + p[0]*q[3] + p[1]*q[2] - p[2]*q[1]

        if flag3D:
            # for rotations > 180 deg
            r[:,r[0]<0] = -r[:,r[0]<0]
            r = r[1:]

        r = r.T
        return r

    def quat2deg(inQuat):
        '''Calculate the axis-angle corresponding to a given quaternion.

        Parameters
        ----------
        inQuat: float, or array_like, shape ([3/4],) or (N,[3/4])
            quaternion(s) or quaternion vector(s)

        Returns
        -------
        axAng : corresponding axis angle(s)
            float, or shape (3,) or (N,3)

        Notes
        -----

        .. math::
            | \\vec{q} | = sin(\\theta/2)

        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------
        >>> quat.quat2deg(0.1)
        array([ 11.47834095])

        >>> quat.quat2deg([0.1, 0.1, 0])
        array([ 11.47834095,  11.47834095,   0.        ])

        >>> quat.quat2deg([cos(0.1), 0, sin(0.1), 0])
        array([  0.       ,  11.4591559,   0.       ])
        '''
        return 2 * np.arcsin(quat2vect(inQuat)) * 180 / pi

    def quat2rotmat(inQuat):
        ''' Calculate the rotation matrix corresponding to the quaternion. If
        "inQuat" contains more than one quaternion, the matrix is flattened (to
        facilitate the work with rows of quaternions), and can be restored to
        matrix form by "reshaping" the resulting rows into a (3,3) shape.

        Parameters
        ----------
        inQuat : array_like, shape ([3,4],) or (N,[3,4])
            quaternions or quaternion vectors

        Returns
        -------
        rotMat : corresponding rotation matrix/matrices (flattened)

        Notes
        -----

        .. math::
            {\\bf{R}} = \\left( {\\begin{array}{*{20}{c}}
            {q_0^2 + q_1^2 - q_2^2 - q_3^2}&{2({q_1}{q_2} - {q_0}{q_3})}&{2({q_1}{q_3} + {q_0}{q_2})}\\\\
            {2({q_1}{q_2} + {q_0}{q_3})}&{q_0^2 - q_1^2 + q_2^2 - q_3^2}&{2({q_2}{q_3} - {q_0}{q_1})}\\\\
            {2({q_1}{q_3} - {q_0}{q_2})}&{2({q_2}{q_3} + {q_0}{q_1})}&{q_0^2 - q_1^2 - q_2^2 + q_3^2} \\\\
            \\end{array}} \\right)

        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------
        >>> r = quat.quat2rotmat([0, 0, 0.1])
        >>> r.shape
        (1, 9)
        >>> r.reshape((3,3))
        array([[ 0.98      , -0.19899749,  0.        ],
            [ 0.19899749,  0.98      ,  0.        ],
            [ 0.        ,  0.        ,  1.        ]])
        '''

        q = vect2quat(inQuat).T

        R = np.zeros((9, q.shape[1]))
        R[0] = q[0]**2 + q[1]**2 - q[2]**2 - q[3]**2
        R[1] = 2*(q[1]*q[2] - q[0]*q[3])
        R[2] = 2*(q[1]*q[3] + q[0]*q[2])
        R[3] = 2*(q[1]*q[2] + q[0]*q[3])
        R[4] = q[0]**2 - q[1]**2 + q[2]**2 - q[3]**2
        R[5] = 2*(q[2]*q[3] - q[0]*q[1])
        R[6] = 2*(q[1]*q[3] - q[0]*q[2])
        R[7] = 2*(q[2]*q[3] + q[0]*q[1])
        R[8] = q[0]**2 - q[1]**2 - q[2]**2 + q[3]**2

        if R.shape[1] == 1:
            return np.reshape(R, (3,3))
        else:
            return R.T

    def quat2vect(inQuat):
        '''
        Extract the quaternion vector from a full quaternion.

        Parameters
        ----------
        inQuat : array_like, shape ([3,4],) or (N,[3,4])
            quaternions or quaternion vectors.

        Returns
        -------
        vect : array, shape (3,) or (N,3)
            corresponding quaternion vectors

        Notes
        -----
        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------
        >>> quat.quat2vect([[cos(0.2), 0, 0, sin(0.2)],[cos(0.1), 0, sin(0.1), 0]])
        array([[ 0.        ,  0.        ,  0.19866933],
               [ 0.        ,  0.09983342,  0.        ]])

        '''

        inQuat = np.atleast_2d(inQuat)
        if inQuat.shape[1] == 4:
            vect = inQuat[:,1:]
        else:
            vect = inQuat
        if np.min(vect.shape)==1:
            vect = vect.ravel()
        return vect

    def rotmat2quat(rMat):
        '''
        Assumes that R has the shape (3,3), or the matrix elements in columns

        Parameters
        ----------
        rMat : array, shape (3,3) or (N,9)
            single rotation matrix, or matrix with rotation-matrix elements.

        Returns
        -------
        outQuat : array, shape (4,) or (N,4)
            corresponding quaternion vector(s)

        Notes
        -----

        .. math::
             \\vec q = 0.5*copysign\\left( {\\begin{array}{*{20}{c}}
            {\\sqrt {1 + {R_{11}} - {R_{22}} - {R_{33}}} ,}\\\\
            {\\sqrt {1 - {R_{11}} + {R_{22}} - {R_{33}}} ,}\\\\
            {\\sqrt {1 - {R_{11}} - {R_{22}} + {R_{33}}} ,}
            \\end{array}\\begin{array}{*{20}{c}}
            {{R_{32}} - {R_{23}}}\\\\
            {{R_{13}} - {R_{31}}}\\\\
            {{R_{21}} - {R_{12}}}
            \\end{array}} \\right)

        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------

        >>> rotMat = array([[cos(alpha), -sin(alpha), 0],
        >>>    [sin(alpha), cos(alpha), 0],
        >>>    [0, 0, 1]])
        >>> quat.rotmat2quat(rotMat)
        array([[ 0.99500417,  0.        ,  0.        ,  0.09983342]])

        '''

        if rMat.shape == (3,3) or rMat.shape == (9,):
            rMat=np.atleast_2d(rMat.ravel()).T
        else:
            rMat = rMat.T
        q = np.zeros((4, rMat.shape[1]))

        R11 = rMat[0]
        R12 = rMat[1]
        R13 = rMat[2]
        R21 = rMat[3]
        R22 = rMat[4]
        R23 = rMat[5]
        R31 = rMat[6]
        R32 = rMat[7]
        R33 = rMat[8]

        q[1] = 0.5 * np.copysign(np.sqrt(1+R11-R22-R33), R32-R23)
        q[2] = 0.5 * np.copysign(np.sqrt(1-R11+R22-R33), R13-R31)
        q[3] = 0.5 * np.copysign(np.sqrt(1-R11-R22+R33), R21-R12)
        q[0] = np.sqrt(1-(q[1]**2+q[2]**2+q[3]**2))

        return q.T

    def vect2quat(inData):
        ''' Utility function, which turns a quaternion vector into a unit quaternion.

        Parameters
        ----------
        inData : array_like, shape (3,) or (N,3)
            quaternions or quaternion vectors

        Returns
        -------
        quats : array, shape (4,) or (N,4)
            corresponding unit quaternions.

        Notes
        -----
        More info under
        http://en.wikipedia.org/wiki/Quaternion

        Examples
        --------
        >>> quats = array([[0,0, sin(0.1)],[0, sin(0.2), 0]])
        >>> quat.vect2quat(quats)
        array([[ 0.99500417,  0.        ,  0.        ,  0.09983342],
               [ 0.98006658,  0.        ,  0.19866933,  0.        ]])

        '''
        inData = np.atleast_2d(inData)
        (m,n) = inData.shape
        if (n!=3)&(n!=4):
            raise ValueError('Quaternion must have 3 or 4 columns')
        if n == 3:
            qLength = 1-np.sum(inData**2,1)
            numLimit = 1e-12
            # Check for numerical problems
            if np.min(qLength) < -numLimit:
                raise ValueError('Quaternion is too long!')
            else:
                # Correct for numerical problems
                qLength[qLength<0] = 0
            outData = np.hstack((np.c_[np.sqrt(qLength)], inData))

        else:
            outData = inData

        return outData

    def vel2quat(omega, q0, rate, CStype):
        '''
        Take an angular velocity (in rad/s), and convert it into the
        corresponding orientation quaternion.

        Parameters
        ----------
        omega : array, shape (3,) or (N,3)
            angular velocity [rad/s].
        q0 : array (3,)
            vector-part of quaternion (!!)
        rate : float
            sampling rate (in [Hz])
        CStype:  string
            coordinate_system, space-fixed ("sf") or body_fixed ("bf")

        Returns
        -------
        quats : array, shape (N,4)
            unit quaternion vectors.

        Notes
        -----
        1) The output has the same length as the input. As a consequence, the last velocity vector is ignored.
        2) For angular velocity with respect to space ("sf"), the orientation is given by

          .. math::
              q(t) = \\Delta q(t_n) \\circ \\Delta q(t_{n-1}) \\circ ... \\circ \\Delta q(t_2) \\circ \\Delta q(t_1) \\circ q(t_0)

          .. math::
            \\Delta \\vec{q_i} = \\vec{n(t)}\\sin (\\frac{\\Delta \\phi (t_i)}{2}) = \\frac{\\vec \\omega (t_i)}{\\left| {\\vec \\omega (t_i)} \\right|}\\sin \\left( \\frac{\\left| {\\vec \\omega ({t_i})} \\right|\\Delta t}{2} \\right)

        3) For angular velocity with respect to the body ("bf"), the sequence of quaternions is inverted.

        4) Take care that you choose a high enough sampling rate!

        Examples
        --------
        >>> v0 = np.r_[0., 0., 100.] * np.pi/180.
        >>> omega = np.tile(v0, (1000,1))
        >>> rate = 100
        >>> out = quat.vel2quat(omega, [0., 0., 0.], rate, 'sf')
        array([[ 1.        ,  0.        ,  0.        ,  0.        ],
           [ 0.99996192,  0.        ,  0.        ,  0.00872654],
           [ 0.9998477 ,  0.        ,  0.        ,  0.01745241],
           ...,
           [-0.74895572,  0.        ,  0.        ,  0.66262005],
           [-0.75470958,  0.        ,  0.        ,  0.65605903],
           [-0.76040597,  0.        ,  0.        ,  0.64944805]])
        '''

        omega = np.atleast_2d(omega)

        # The following is (approximately) the quaternion-equivalent of the trapezoidal integration (cumtrapz)
        if omega.shape[1]>1:
            omega[:-1] = 0.5*(omega[:-1] + omega[1:])

        omega_t = np.sqrt(np.sum(omega**2, 1))
        omega_nonZero = omega_t>0

        # initialize the quaternion
        q_delta = np.zeros(omega.shape)
        q_pos = np.zeros((len(omega),4))
        q_pos[0,:] = vect2quat(q0)

        # magnitude of position steps
        dq_total = np.sin(omega_t[omega_nonZero]/(2*rate))

        q_delta[omega_nonZero,:] = omega[omega_nonZero,:] * np.tile(dq_total/omega_t[omega_nonZero], (3,1)).T

        for ii in range(len(omega)-1):
            q1 = vect2quat(q_delta[ii,:])
            q2 = q_pos[ii,:]
            if CStype == 'sf':
                qm = quatmult(q1,q2)
            elif CStype == 'bf':
                qm = quatmult(q2,q1)
            else:
                print('I don''t know this type of coordinate system!')
            q_pos[ii+1,:] = qm

        return q_pos

    def quat2vel(q, rate=1, winSize=5, order=2):
        '''
        Take a quaternion, and convert it into the
        corresponding angular velocity

        Parameters
        ----------
        q : array, shape (N,[3,4])
            unit quaternion vectors.
        rate : float
            sampling rate (in [Hz])
        winSize : integer
            window size for the calculation of the velocity.
            Has to be odd.
        order : integer
            Order of polynomial used by savgol to calculate the first derivative

        Returns
        -------
        vel : array, shape (3,) or (N,3)
            angular velocity [rad/s].

        Notes
        -----
        The angular velocity is given by

          .. math::
            \\omega = 2 * \\frac{dq}{dt} \\circ q^{-1}

        Examples
        --------
        >>> rate = 1000
        >>> t = np.arange(0,10,1/rate)
        >>> x = 0.1 * np.sin(t)
        >>> y = 0.2 * np.sin(t)
        >>> z = np.zeros_like(t)
        array([[ 0.20000029,  0.40000057,  0.        ],
               [ 0.19999989,  0.39999978,  0.        ],
               [ 0.19999951,  0.39999901,  0.        ]])
                .......
        '''

        if np.mod(winSize, 2) != 1:
            raise ValueError('Window size must be odd!')

        numCols = q.shape[1]
        if numCols < 3 or numCols > 4:
            raise TypeError('quaternions must have 3 or 4 columns')

        # This has to be done: otherwise quatmult will "complete" dq_dt to be a unit
        # quaternion, resulting in wrong value
        if numCols == 3:
            q = vect2quat(q)

        dq_dt = signal.savgol_filter(q, window_length=winSize, polyorder=order, deriv=1, delta=1./rate, axis=0)
        angVel = 2 * quatmult(dq_dt, quatinv(q))

        return angVel[:,1:]

    if __name__=='__main__':
        '''These are some simple tests to see if the functions produce the
        proper output.
        More extensive tests are found in tests/test_quat.py'''

        from vector import rotate_vector

        v0 = np.r_[0., 0., 100.] * np.pi/180.
        vel = np.tile(v0, (1000,1))
        rate = 100
        out = vel2quat(vel, [0., 0., 0.], rate, 'sf')

        rate = 1000
        t = np.arange(0,10,1/rate)
        x = 0.1 * np.sin(t)
        y = 0.2 * np.sin(t)
        z = np.zeros_like(t)

        q = np.column_stack( (x,y,z) )
        vel = quat2vel(q, rate, 5, 2)
        qReturn = vel2quat(vel, q[0], rate, 'sf' )
        plt.plot(q)
        plt.hold(True)
        plt.plot(qReturn[:,1:],'--')
        plt.show()

        q = Quaternion(np.array([0,0,10]), 'Fick')
        print(q)
        rm = q.export(to='rotmat')
        print(rm)
        q2 = Quaternion(rm, inType='rotmat')
        print(q2)

        a = np.r_[np.cos(0.1), 0,0,np.sin(0.1)]
        b = np.r_[np.cos(0.1),0,np.sin(0.1), 0]
        c = np.vstack((a,b))
        d = np.r_[np.sin(0.1), 0, 0]
        e = np.r_[2, 0, np.sin(0.1), 0]

        print(quatmult(a,a))
        print(quatmult(a,b))
        print(quatmult(c,c))
        print(quatmult(c,a))
        print(quatmult(d,d))

        print('The inverse of {0} is {1}'.format(a, quatinv(a)))
        print('The inverse of {0} is {1}'.format(d, quatinv(d)))
        print('The inverse of {0} is {1}'.format(e, quatinv(e)))
        print(quatmult(e, quatinv(e)))

        print(quat2vect(a))
        print('{0} is {1} degree'.format(a, quat2deg(a)))
        print('{0} is {1} degree'.format(c, quat2deg(c)))
        print(quat2deg(0.2))
        x = np.r_[1,0,0]
        vNull = np.r_[0,0,0]
        print(rotate_vector(x, a))

        v0 = [0., 0., 100.]
        vel = np.tile(v0, (1000,1))
        rate = 100

        out = vel2quat(vel, [0., 0., 0.], rate, 'sf')
        print(out[-1:])
        plt.plot(out[:,1:4])
        plt.show()

        print(deg2quat(15))
        print(deg2quat(quat2deg(a)))

        q = np.array([[0, 0, np.sin(0.1)],
                   [0, np.sin(0.01), 0]])
        rMat = quat2rotmat(q)
        print(rMat[1].reshape((3,3)))
        qNew = rotmat2quat(rMat)
        print(qNew)

        q = Quaternion(np.array([0,0,0.5]))
        p = Quaternion(np.array([[0,0,0.5], [0,0,0.1]]))
        r = Quaternion([0,0,0.5])
        print(p*q)
        print(q*3)
        print(q*pi)
        print(q/p)
        print(q/5)

        Fick = p.export('Fick')
        Q_fick = q.export('Fick')

        import pprint
        pprint.pprint(Fick)
        pprint.pprint(np.rad2deg(Fick))

        p = Quaternion(np.array([[0,0,0.5], [0,0,0.1], [0,0,0.1]]))
        p[1:] = [[0,0,0],[0,0,0.01]]
        print(p)

        '''
        '''