# Source code for imus

    '''
    Utilities for movements recordins with inertial measurement units (IMUs)
    Currently data from the following systems are supported

        - XIO
        - XSens
        - YEI
    '''

    '''
    Author: Thomas Haslwanter
    Version: 1.5
    Date: April-2016
    '''

    import numpy as np
    import scipy as sp
    from scipy.integrate import cumtrapz
    import matplotlib.pyplot as plt
    import pandas as pd
    from numpy import r_, sum
    import re

    # The following construct is required since I want to run the module as a script
    # inside the skinematics-directory
    import os
    import sys
    PACKAGE_PARENT = '..'
    SCRIPT_DIR = os.path.realpath(os.path.dirname(__file__))
    sys.path.append(os.path.normpath(os.path.join(SCRIPT_DIR, PACKAGE_PARENT)))

    from skinematics import quat, vector
    import easygui

    class IMU:
        '''
        Class for working with working with inertial measurement units (IMUs)

        An IMU object can be initialized
            - by giving a filename
            - by providing measurement data and a samplerate
            - without giving any parameter; in that case the user is prompted
              to select an infile

        Parameters
        ----------
        inFile : string
            path- and file-name of infile, if you get the sound from a file.
        inData : dictionary
            The following fields are required:

            acc : (N x 3) array
                 Linear acceleration [m/s^2], in the x-, y-, and z-direction
            omega : (N x 3) array
                 Angular velocity [deg/s], about the x-, y-, and z-axis
            [mag] : (N x 3) array (optional)
                 Local magnetic field, in the x-, y-, and z-direction
            rate: integer
                sample rate [Hz]

        Notes
        -----

        IMU-Properties:
            - source
            - acc
            - omega
            - mag
            - rate
            - totalSamples
            - duration
            - dataType

        Examples
        --------
    	>>> myimu = IMU(r'.\Data\data_xsens.txt')
    	>>>
    	>>> initialOrientation = np.array([[1,0,0],
    	>>>                                [0,0,-1],
    	>>>                                [0,1,0]])
    	>>> initialPosition = np.r_[0,0,0]
    	>>>
    	>>> myimu.calc_orientation(initialOrientation)
    	>>> q_simple = myimu.quat[:,1:]
    	>>>
    	>>> calcType = 'Madgwick'
    	>>> myimu.calc_orientation(initialOrientation, type=calcType)
    	>>> q_Kalman = myimu.quat[:,1:]

        '''

        def __init__(self, inFile = None, inData = None):
            '''Initialize an IMU-object'''

            if inData is not None:
                self.setData(inData, inRate)
            else:
                if inFile is None:
                    inFile = self._selectInput()
                if os.path.exists(inFile):
                    self.source = inFile

                    try:
                        data = import_data(inFile=self.source, type='XSens', paramList=['rate', 'acc', 'gyr', 'mag'])
                        self.rate = data[0]
                        self.acc= data[1]
                        self.omega = data[2]
                        self.mag = data[3]
                        self._setInfo()

                        print('data read in!')
                    except IOError:
                        print('Could not read ' + inFile)
                else:
                    print(inFile + ' does NOT exist!')

        def setData(self, data):
            ''' Set the properties of an IMU-object. '''

            if 'rate' not in data.keys():
                print('Set the "rate" to the default value (100 Hz).')
                data['rate'] = 100.0

            self.rate = data['rate']
            self.acc= data['acc']
            self.omega = data['omega']
            if 'mag' in data.keys():
                self.mag = data['mag']
            self.source = None
            self._setInfo()

        def calc_orientation(self, R_initialOrientation, type='quatInt'):
            '''
            Calculate the current orientation

            Parameters
            ----------
            R_initialOrientation : 3x3 array
                    approximate alignment of sensor-CS with space-fixed CS
            type : string
                    - 'quatInt' .... quaternion integration of angular velocity
                    - 'Kalman' ..... quaternion Kalman filter
                    - 'Madgwick' ... gradient descent method, efficient
                    - 'Mahony' ....  formula from Mahony, as implemented by Madgwick

            '''

            initialPosition = np.r_[0,0,0]

            if type == 'quatInt':
                (quaternion, position) = calc_QPos(R_initialOrientation, self.omega, initialPosition, self.acc, self.rate)

            elif type == 'Kalman':
                self._checkRequirements()
                quaternion =  kalman_quat(self.rate, self.acc, self.omega, self.mag)

            elif type == 'Madgwick':
                self._checkRequirements()

                # Initialize object
                AHRS = MadgwickAHRS(SamplePeriod=1./self.rate, Beta=0.1)
                quaternion = np.zeros((self.totalSamples, 4))

                # The "Update"-function uses angular velocity in radian/s, and only the directions of acceleration and magnetic field
                Gyr = self.omega
                Acc = vector.normalize(self.acc)
                Mag = vector.normalize(self.mag)

                #for t in range(len(time)):
                for t in misc.progressbar(range(self.totalSamples), 'Calculating the Quaternions ', 25) :
                    AHRS.Update(Gyr[t], Acc[t], Mag[t])
                    quaternion[t] = AHRS.Quaternion

            elif type == 'Mahony':
                self._checkRequirements()

                # Initialize object
                AHRS = MahonyAHRS(SamplePeriod=1./self.rate, Kp=0.5)
                quaternion = np.zeros((self.totalSamples, 4))

                # The "Update"-function uses angular velocity in radian/s, and only the directions of acceleration and magnetic field
                Gyr = self.omega
                Acc = vector.normalize(self.acc)
                Mag = vector.normalize(self.mag)

                #for t in range(len(time)):
                for t in misc.progressbar(range(self.totalSamples), 'Calculating the Quaternions ', 25) :
                    AHRS.Update(Gyr[t], Acc[t], Mag[t])
                    quaternion[t] = AHRS.Quaternion

            else:
                print('Unknown orientation type: {0}'.format(type))
                return

            self.quat = quaternion

        def calc_position(self, initialPosition):
            '''Calculate the position, assuming that the orientation is already known.'''

            # Acceleration, velocity, and position ----------------------------
            # From q and the measured acceleration, get the \frac{d^2x}{dt^2}
            g = sp.constants.g
            g_v = np.r_[0, 0, g]
            accReSensor = self.acc - vector.rotate_vector(g_v, quat.quatinv(self.quat))
            accReSpace = vector.rotate_vector(accReSensor, self.quat)

            # Position and Velocity through integration, assuming 0-velocity at t=0
            vel = np.nan*np.ones_like(accReSpace)
            pos = np.nan*np.ones_like(accReSpace)

            for ii in range(accReSpace.shape[1]):
                vel[:,ii] = cumtrapz(accReSpace[:,ii], dx=1./self.rate, initial=0)
                pos[:,ii] = cumtrapz(vel[:,ii],        dx=1./self.rate, initial=initialPosition[ii])

            self.pos = pos

        def _checkRequirements(self):
            '''Check if all the necessary variables are available.'''
            required = [ 'rate', 'acc', 'omega', 'mag' ]

            for field in required:
                if field not in vars(self):
                    print('Cannot find {0} in calc_orientation!'.format(field))

        def _selectInput(self):
            '''GUI for the selection of an in-file. '''

            fullInFile = easygui.fileopenbox(msg='Input data: ', title='Selection', default='*.txt')
            print('Selection: ' + fullInFile)
            return fullInFile

        def _setInfo(self):
            '''Set the information properties of that IMU'''

            self.totalSamples = len(self.omega)
            self.duration = np.float(self.totalSamples)/self.rate # [sec]
            self.dataType = str(self.omega.dtype)

    def import_data(inFile=None, type='XSens', paramList=[]):
        '''
        Read in Rate and stored 3D parameters from IMUs

        Parameters
        ----------
        inFile : string
                 Path and name of input file
        type : sensor-type. Has to be either ['XSens', 'xio', 'yei']
        paramList: list of strings
                   You can select between ['acc', 'gyr', 'mag', 'rate', 'others']

        Returns
        -------
        List, containing
        rate : float
            Sampling rate
        [List of x/y/z Parameter Values]

        Examples
        --------
        >>> data = import_data(fullInFile, type='XSens', paramList=['rate', 'acc', 'gyr'])
        >>> rate = data[0]
        >>> accValues = data[1]
        >>> Omega = data[2]

        '''

        if inFile is None:
            inFile = easygui.fileopenbox(msg='Please select an in-file: ', title='Data-selection', default='*.txt')

        varList = ['acc', 'gyr', 'mag', 'rate', 'others']

        dataDict = {}
        for var in varList:
            dataDict[var]=None

        if type == 'XSens':
            from sensors import xsens
            data = xsens.get_data(inFile)
        elif type == 'xio':
            from sensors import xio
            data = xio.get_data(inFile)
        elif type == 'yei':
            from sensors import yei
            data = yei.get_data(inFile)
        else:
            raise ValueError

        dataDict['rate'] = data[0]
        dataDict['acc']  = data[1]
        dataDict['gyr']  = data[2]
        dataDict['mag']  = data[3]

        returnValues = []

        # By default, return all values, in alphabetical order
        if paramList == []:
            paramList = list(dataDict.keys())
            paramList.sort()
            print('Return-values: {0}'.format(paramList))

        for param in paramList:
            try:
                returnValues.append(dataDict[param])
            except KeyError as err:
                print('Please check the parameter {0}'.format(param))
                print(err)

        return returnValues

    def _read_xsens(inFile):
        '''Read data from an XSens sensor.
        The data returned are (in that order): [rate, acceleration, angular_velocity, mag_field_direction]'''

        # Get the sampling rate from the second line in the file
        try:
            fh = open(inFile)
            fh.readline()
            line = fh.readline()
            rate = np.float(line.split(':')[1].split('H')[0])
            fh.close()
            returnValues = [rate]

        except FileNotFoundError:
            print('{0} does not exist!'.format(inFile))
            return -1

        # Read the data
        data = pd.read_csv(inFile,
                           sep='\t',
                           skiprows=4,
                           index_col=False)

        # Extract the columns that you want, by name
        paramList=['Acc', 'Gyr', 'Mag']
        for param in paramList:
            Expression = param + '*'
            returnValues.append(data.filter(regex=Expression).values)

        return returnValues

    def _read_xio(inFile):
        '''Read data from an XIO sensor.
        The data returned are (in that order): [rate, acceleration, angular_velocity, mag_field_direction, packet_nr]'''

        # XIO-definition of the sampling rate
        # Get the "Register"
        inFile = '_'.join(inFile.split('_')[:-1]) + '_Registers.csv'

        # Make sure that we read in the correct one
        inFile = '_'.join(inFile.split('_')[:-1]) + '_CalInertialAndMag.csv'
        data = pd.read_csv(inFile)

        # Generate a simple list of column names
        rate = 256  # currently hardcoded

        returnValues = [rate]

        # Extract the columns that you want, by name
        paramList=['Acc', 'Gyr', 'Mag', 'Packet']
        for Expression in paramList:
            returnValues.append(data.filter(regex=Expression).values)

        return returnValues

    def _read_yei(inFile):
        '''Read data from an YEI sensor.
        The data returned are (in that order): [rate, acceleration, angular_velocity, mag_field_direction]'''

        data = pd.read_csv(inFile)

        # Generate a simple list of column names
        newColumns = []
        pattern = re.compile('.*%(\w+)\((\w+)\)')
        for name in data.columns:
            newColumns.append(pattern.match(name).groups()[1])
        data.columns = newColumns

        # Calculate rate (ChipTime is in microsec)
        start = data.ChipTimeUS[0] * 1e-6    # microseconds to seconds
        stop = data.ChipTimeUS.values[-1] * 1e-6    # pandas can't count backwards
        rate = len(data) / (stop-start)

        returnValues = [rate]

        # Extract the columns that you want, by name
        paramList=['Accel', 'Gyro', 'Compass']
        for Expression in paramList:
            returnValues.append(data.filter(regex=Expression).values)

        return returnValues

    def calc_QPos(R_initialOrientation, omega, initialPosition, accMeasured, rate):
        ''' Reconstruct position and orientation, from angular velocity and linear acceleration.
        Assumes a start in a stationary position. No compensation for drift.

        Parameters
        ----------
        omega : ndarray(N,3)
            Angular velocity, in [rad/s]
        accMeasured : ndarray(N,3)
            Linear acceleration, in [m/s^2]
        initialPosition : ndarray(3,)
            initial Position, in [m]
        R_initialOrientation: ndarray(3,3)
            Rotation matrix describing the initial orientation of the sensor,
            except a mis-orienation with respect to gravity
        rate : float
            sampling rate, in [Hz]

        Returns
        -------
        q : ndarray(N,3)
            Orientation, expressed as a quaternion vector
        pos : ndarray(N,3)
            Position in space [m]

        Example
        -------
        >>> q1, pos1 = calc_QPos(R_initialOrientation, omega, initialPosition, acc, rate)

        '''

        # Transform recordings to angVel/acceleration in space --------------

        # Orientation of \vec{g} with the sensor in the "R_initialOrientation"
        g = 9.81
        g0 = np.linalg.inv(R_initialOrientation).dot(r_[0,0,g])

        # for the remaining deviation, assume the shortest rotation to there
        q0 = vector.qrotate(accMeasured[0], g0)
        R0 = quat.quat2rotmat(q0)

        # combine the two, to form a reference orientation. Note that the sequence
        # is very important!
        R_ref = R_initialOrientation.dot(R0)
        q_ref = quat.rotmat2quat(R_ref)

        # Calculate orientation q by "integrating" omega -----------------
        q = quat.vel2quat(omega, q_ref, rate, 'bf')

        # Acceleration, velocity, and position ----------------------------
        # From q and the measured acceleration, get the \frac{d^2x}{dt^2}
        g_v = r_[0, 0, g]
        accReSensor = accMeasured - vector.rotate_vector(g_v, quat.quatinv(q))
        accReSpace = vector.rotate_vector(accReSensor, q)

        # Make the first position the reference position
        q = quat.quatmult(q, quat.quatinv(q[0]))

        # compensate for drift
        #drift = np.mean(accReSpace, 0)
        #accReSpace -= drift*0.7

        # Position and Velocity through integration, assuming 0-velocity at t=0
        vel = np.nan*np.ones_like(accReSpace)
        pos = np.nan*np.ones_like(accReSpace)

        for ii in range(accReSpace.shape[1]):
            vel[:,ii] = cumtrapz(accReSpace[:,ii], dx=1./rate, initial=0)
            pos[:,ii] = cumtrapz(vel[:,ii],        dx=1./rate, initial=initialPosition[ii])

        return (q, pos)

    def kalman_quat(rate, acc, gyr, mag):
        '''
        Calclulate the orientation from IMU magnetometer data.

        Parameters
        ----------
        rate : float
        	   sample rate [Hz]
        acc : (N,3) ndarray
        	  linear acceleration [m/sec^2]
        gyr : (N,3) ndarray
        	  angular velocity [rad/sec]
        mag : (N,3) ndarray
        	  magnetic field orientation

        Returns
        -------
        qOut : (N,4) ndarray
        	   unit quaternion, describing the orientation relativ to the coordinate system spanned by the local magnetic field, and gravity

        Notes
        -----
        Based on "Design, Implementation, and Experimental Results of a Quaternion-Based Kalman Filter for Human Body Motion Tracking" Yun, X. and Bachman, E.R., IEEE TRANSACTIONS ON ROBOTICS, VOL. 22, 1216-1227 (2006)

        '''

        numData = len(acc)

        # Set parameters for Kalman Filter
        tstep = 1/rate
        tau = [0.5, 0.5, 0.5]	# from Yun, 2006

        # Initializations
        x_k = np.zeros(7)	# state vector
        z_k = np.zeros(7)   # measurement vector
        z_k_pre = np.zeros(7)
        P_k = np.matrix( np.eye(7) )		 # error covariance matrix P_k

        Phi_k = np.matrix( np.zeros((7,7)) ) # discrete state transition matrix Phi_k
        for ii in range(3):
            Phi_k[ii,ii] = np.exp(-tstep/tau[ii])

        H_k = np.matrix( np.eye(7) )		# Identity matrix

        Q_k = np.matrix( np.zeros((7,7)) )	# process noise matrix Q_k
        D = 0.0001*r_[0.4, 0.4, 0.4]		# [rad^2/sec^2]; from Yun, 2006
                                                                                # check 0.0001 in Yun
        for ii in range(3):
            Q_k[ii,ii] =  D[ii]/(2*tau[ii])  * ( 1-np.exp(-2*tstep/tau[ii]) )

        # Evaluate measurement noise covariance matrix R_k
        R_k = np.matrix( np.zeros((7,7)) )
        r_angvel = 0.01;      # [rad**2/sec**2]; from Yun, 2006
        r_quats = 0.0001;     # from Yun, 2006
        for ii in range(7):
            if ii<3:
                R_k[ii,ii] = r_angvel
            else:
                R_k[ii,ii] = r_quats

        # Calculation of orientation for every time step
        qOut = np.zeros( (numData,4) )

        for ii in range(numData):
            accelVec  = acc[ii,:]
            magVec    = mag[ii,:]
            angvelVec = gyr[ii,:]
            z_k_pre = z_k.copy()	# watch out: by default, Python passes the reference!!

            # Evaluate quaternion based on acceleration and magnetic field data
            accelVec_n = vector.normalize(accelVec)
            magVec_hor = magVec - accelVec_n * accelVec_n.dot(magVec)
            magVec_n   = vector.normalize(magVec_hor)
            basisVectors = np.vstack( (magVec_n, np.cross(accelVec_n, magVec_n), accelVec_n) ).T
            quatRef = quat.quatinv(quat.rotmat2quat(basisVectors)).flatten()

            # Update measurement vector z_k
            z_k[:3] = angvelVec
            z_k[3:] = quatRef

            # Calculate Kalman Gain
            # K_k = P_k * H_k.T * inv(H_k*P_k*H_k.T + R_k)
            # Check: why is H_k used in the original formulas?
            K_k = P_k * np.linalg.inv(P_k + R_k)

            # Update state vector x_k
            x_k += np.array( K_k.dot(z_k-z_k_pre) ).ravel()

            # Evaluate discrete state transition matrix Phi_k
            Phi_k[3,:] = r_[-x_k[4]*tstep/2, -x_k[5]*tstep/2, -x_k[6]*tstep/2,              1, -x_k[0]*tstep/2, -x_k[1]*tstep/2, -x_k[2]*tstep/2]
            Phi_k[4,:] = r_[ x_k[3]*tstep/2, -x_k[6]*tstep/2,  x_k[5]*tstep/2, x_k[0]*tstep/2,               1,  x_k[2]*tstep/2, -x_k[1]*tstep/2]
            Phi_k[5,:] = r_[ x_k[6]*tstep/2,  x_k[3]*tstep/2, -x_k[4]*tstep/2, x_k[1]*tstep/2, -x_k[2]*tstep/2,               1,  x_k[0]*tstep/2]
            Phi_k[6,:] = r_[-x_k[5]*tstep/2,  x_k[4]*tstep/2,  x_k[3]*tstep/2, x_k[2]*tstep/2,  x_k[1]*tstep/2, -x_k[0]*tstep/2,               1]

            # Update error covariance matrix
            #P_k = (eye(7)-K_k*H_k)*P_k
            # Check: why is H_k used in the original formulas?
            P_k = (H_k - K_k) * P_k

            # Projection of state quaternions
            x_k[3:] += quat.quatmult(0.5*x_k[3:],r_[0, x_k[:3]]).flatten()
            x_k[3:] = vector.normalize( x_k[3:] )
            x_k[:3] = np.zeros(3)
            x_k[:3] = tstep * (-x_k[:3]+z_k[:3])

            qOut[ii,:] = x_k[3:]

            # Projection of error covariance matrix
            P_k = Phi_k * P_k * Phi_k.T + Q_k

        # Make the first position the reference position
        qOut = quat.quatmult(qOut, quat.quatinv(qOut[0]))

        return qOut

    class MadgwickAHRS:
        '''Madgwick's gradient descent filter.
        '''

        def __init__(self, SamplePeriod=1./256, Beta=1.0, Quaternion=[1,0,0,0]):
            '''Initialization

            Parameters
            ----------
            SamplePeriod : sample period
            Beta : algorithm gain
            Quaternion : output quaternion describing the Earth relative to the sensor
            '''
            self.SamplePeriod = SamplePeriod
            self.Beta = Beta
            self.Quaternion = Quaternion

        def Update(self, Gyroscope, Accelerometer, Magnetometer):
            '''Calculate the best quaternion to the given measurement values.'''

            q = self.Quaternion; # short name local variable for readability

            # Reference direction of Earth's magnetic field
            h = vector.rotate_vector(Magnetometer, q)
            b = np.hstack((0, np.sqrt(h[0]**2+h[1]**2), 0, h[2]))

            # Gradient decent algorithm corrective step
            F = [2*(q[1]*q[3] - q[0]*q[2])   - Accelerometer[0],
                 2*(q[0]*q[1] + q[2]*q[3])   - Accelerometer[1],
                 2*(0.5 - q[1]**2 - q[2]**2) - Accelerometer[2],
                 2*b[1]*(0.5 - q[2]**2 - q[3]**2) + 2*b[3]*(q[1]*q[3] - q[0]*q[2])   - Magnetometer[0],
                 2*b[1]*(q[1]*q[2] - q[0]*q[3])   + 2*b[3]*(q[0]*q[1] + q[2]*q[3])   - Magnetometer[1],
                 2*b[1]*(q[0]*q[2] + q[1]*q[3])   + 2*b[3]*(0.5 - q[1]**2 - q[2]**2) - Magnetometer[2]]

            J = np.array([
                [-2*q[2],                 	2*q[3],                    -2*q[0],                         2*q[1]],
                [ 2*q[1],                 	2*q[0],                	    2*q[3],                         2*q[2]],
                [0,                        -4*q[1],                    -4*q[2],                         0],
                [-2*b[3]*q[2],              2*b[3]*q[3],               -4*b[1]*q[2]-2*b[3]*q[0],       -4*b[1]*q[3]+2*b[3]*q[1]],
                [-2*b[1]*q[3]+2*b[3]*q[1],	2*b[1]*q[2]+2*b[3]*q[0],    2*b[1]*q[1]+2*b[3]*q[3],       -2*b[1]*q[0]+2*b[3]*q[2]],
                [ 2*b[1]*q[2],              2*b[1]*q[3]-4*b[3]*q[1],    2*b[1]*q[0]-4*b[3]*q[2],        2*b[1]*q[1]]])

            step = J.T.dot(F)
            step = vector.normalize(step)	# normalise step magnitude

            # Compute rate of change of quaternion
            qDot = 0.5 * quat.quatmult(q, np.hstack([0, Gyroscope])) - self.Beta * step

            # Integrate to yield quaternion
            q = q + qDot * self.SamplePeriod
            self.Quaternion = vector.normalize(q).flatten()

    class MahonyAHRS:
        '''Madgwick's implementation of Mayhony's AHRS algorithm
        '''
        def __init__(self, SamplePeriod=1./256, Kp=1.0, Ki=0, Quaternion=[1,0,0,0]):
            '''Initialization

            Parameters
            ----------
            SamplePeriod : sample period
            Kp : algorithm proportional gain
            Ki : algorithm integral gain
            Quaternion : output quaternion describing the Earth relative to the sensor
            '''
            self.SamplePeriod = SamplePeriod
            self.Kp = Kp
            self.Ki = Ki
            self.Quaternion = Quaternion
            self._eInt = [0, 0, 0]  # integral error

        def Update(self, Gyroscope, Accelerometer, Magnetometer):
            '''Calculate the best quaternion to the given measurement values.'''

            q = self.Quaternion; # short name local variable for readability

            # Reference direction of Earth's magnetic field
            h = vector.rotate_vector(Magnetometer, q)
            b = np.hstack((0, np.sqrt(h[0]**2+h[1]**2), 0, h[2]))

            # Estimated direction of gravity and magnetic field
            v = np.array([
                 2*(q[1]*q[3] - q[0]*q[2]),
                 2*(q[0]*q[1] + q[2]*q[3]),
                 q[0]**2 - q[1]**2 - q[2]**2 + q[3]**2])

            w = np.array([
                 2*b[1]*(0.5 - q[2]**2 - q[3]**2) + 2*b[3]*(q[1]*q[3] - q[0]*q[2]),
                 2*b[1]*(q[1]*q[2] - q[0]*q[3]) + 2*b[3]*(q[0]*q[1] + q[2]*q[3]),
                 2*b[1]*(q[0]*q[2] + q[1]*q[3]) + 2*b[3]*(0.5 - q[1]**2 - q[2]**2)])

            # Error is sum of cross product between estimated direction and measured direction of fields
            e = np.cross(Accelerometer, v) + np.cross(Magnetometer, w)

            if self.Ki > 0:
                self._eInt += e * self.SamplePeriod
            else:
                self._eInt = np.array([0, 0, 0], dtype=np.float)

            # Apply feedback terms
            Gyroscope += self.Kp * e + self.Ki * self._eInt;

            # Compute rate of change of quaternion
            qDot = 0.5 * quat.quatmult(q, np.hstack([0, Gyroscope])).flatten()

            # Integrate to yield quaternion
            q += qDot * self.SamplePeriod

            self.Quaternion = vector.normalize(q)

    if __name__ == '__main__':
        myimu = IMU(r'.\tests\data_xsens.txt')

        initialOrientation = np.array([[1,0,0],
                                       [0,0,-1],
                                       [0,1,0]])

        myimu.calc_orientation(initialOrientation, type='quatInt')
        q_simple = myimu.quat[:,1:]

        #calcType = 'Mahony'
        calcType = 'Madgwick'
        calcType = 'Kalman'
        myimu.calc_orientation(initialOrientation, type=calcType)
        q_Kalman = myimu.quat[:,1:]

        #myimu.calc_position(initialPosition)

        t = np.arange(myimu.totalSamples)/myimu.rate
        plt.plot(t, q_simple, '-', label='simple')
        plt.hold(True)
        plt.plot(t, q_Kalman, '--', label=calcType)
        plt.legend()
        #plt.plot(t, myimu.pos)
        plt.show()

        print('Done')