skrf.vi.vna.ZVA40
=================

.. currentmodule:: skrf.vi.vna

.. autoclass:: ZVA40
  :no-members:



.. rubric:: Attributes

.. autosummary::
  :toctree:
  :nosignatures:

  ~ZVA40.cal_coefs_list
  ~ZVA40.continuous
  ~ZVA40.corr_state_of_channel
  ~ZVA40.corr_state_of_meas
  ~ZVA40.f_npoints
  ~ZVA40.f_start
  ~ZVA40.f_stop
  ~ZVA40.frequency
  ~ZVA40.frequency_cw
  ~ZVA40.idn
  ~ZVA40.if_bw
  ~ZVA40.npoints
  ~ZVA40.ntraces
  ~ZVA40.power_level
  ~ZVA40.snp_format
  ~ZVA40.sweep_mode
  ~ZVA40.sweep_type
  ~ZVA40.trigger_mode
  ~ZVA40.trigger_source





.. rubric:: Methods

.. autosummary::
  :toctree:
  :nosignatures:

  ~ZVA40.__init__
  ~ZVA40.ask
  ~ZVA40.ask_for_values
  ~ZVA40.create_cset
  ~ZVA40.create_meas
  ~ZVA40.create_meas_hidden
  ~ZVA40.delete_all_meas
  ~ZVA40.delete_cset
  ~ZVA40.delete_meas
  ~ZVA40.disable_gating
  ~ZVA40.display_trace
  ~ZVA40.doc
  ~ZVA40.enable_gating
  ~ZVA40.enable_transform
  ~ZVA40.func_on_all_traces
  ~ZVA40.get_active_cset
  ~ZVA40.get_active_meas
  ~ZVA40.get_cal_coefs
  ~ZVA40.get_cal_coefs_list
  ~ZVA40.get_calibration
  ~ZVA40.get_corr_state_of_channel
  ~ZVA40.get_corr_state_of_meas
  ~ZVA40.get_cset_list
  ~ZVA40.get_data
  ~ZVA40.get_data_snp
  ~ZVA40.get_f_npoints
  ~ZVA40.get_f_start
  ~ZVA40.get_f_stop
  ~ZVA40.get_fdata
  ~ZVA40.get_frequency
  ~ZVA40.get_frequency_cw
  ~ZVA40.get_meas_list
  ~ZVA40.get_network
  ~ZVA40.get_network_all_meas
  ~ZVA40.get_oneport
  ~ZVA40.get_power_level
  ~ZVA40.get_rdata
  ~ZVA40.get_sdata
  ~ZVA40.get_snp_format
  ~ZVA40.get_sweep_mode
  ~ZVA40.get_sweep_type
  ~ZVA40.get_switch_terms
  ~ZVA40.get_trigger_mode
  ~ZVA40.get_trigger_source
  ~ZVA40.get_twoport
  ~ZVA40.get_win_trace
  ~ZVA40.get_window_list
  ~ZVA40.help
  ~ZVA40.normalize
  ~ZVA40.opc
  ~ZVA40.reset
  ~ZVA40.save_active_cset
  ~ZVA40.select_meas
  ~ZVA40.set_active_cset
  ~ZVA40.set_cal_coefs
  ~ZVA40.set_calibration
  ~ZVA40.set_corr_state_of_channel
  ~ZVA40.set_corr_state_of_meas
  ~ZVA40.set_display_format
  ~ZVA40.set_display_format_all
  ~ZVA40.set_f_npoints
  ~ZVA40.set_f_start
  ~ZVA40.set_f_stop
  ~ZVA40.set_frequency
  ~ZVA40.set_frequency_cw
  ~ZVA40.set_port_power_level
  ~ZVA40.set_power_level
  ~ZVA40.set_snp_format
  ~ZVA40.set_source_freq_conversion
  ~ZVA40.set_source_power_permanent
  ~ZVA40.set_sweep_mode
  ~ZVA40.set_sweep_type
  ~ZVA40.set_trigger_mode
  ~ZVA40.set_trigger_source
  ~ZVA40.set_window_arrangement
  ~ZVA40.set_yscale
  ~ZVA40.set_yscale_auto
  ~ZVA40.set_yscale_couple
  ~ZVA40.setup_oneport
  ~ZVA40.setup_twoport
  ~ZVA40.sweep
  ~ZVA40.toggle_port_power
  ~ZVA40.trigger
  ~ZVA40.trigger_and_wait_till_done
  ~ZVA40.write




