TITLE: Versatile Express Images Configuration File
[IMAGES]
TOTALIMAGES: 9                  ;Number of Images (Max: 32)
NOR0UPDATE: AUTO                 ;Image Update:NONE/AUTO/FORCE
NOR0ADDRESS: BOOT                ;Image Flash Address
NOR0FILE: \SOFTWARE\$bm_image    ;Image File Name

NOR1UPDATE: AUTO                 ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR1ADDRESS: 0x0E000000          ;Image Flash Address
NOR1FILE: \SOFTWARE\kern_mp.bin  ;Image File Name
NOR1LOAD: 0x80008000
NOR1ENTRY: 0x80008000

NOR2UPDATE: AUTO                 ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR2ADDRESS: 0x0E800000          ;Image Flash Address
NOR2FILE: \SOFTWARE\mp_a7.dtb ;Image File Name for booting in A7 cluster
NOR2LOAD: 0x84000000
NOR2ENTRY: 0x84000000

NOR3UPDATE: AUTO                 ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR3ADDRESS: 0x0E900000          ;Image Flash Address
NOR3FILE: \SOFTWARE\mp_a15.dtb    ;Image File Name
NOR3LOAD: 0x84000000
NOR3ENTRY: 0x84000000

NOR4UPDATE: AUTO                 ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR4ADDRESS: 0x0EA00000          ;Image Flash Address
NOR4FILE: \SOFTWARE\mp_a7bc.dtb   ;Image File Name
NOR4LOAD: 0x84000000
NOR4ENTRY: 0x84000000

NOR5UPDATE: AUTO                    ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR5ADDRESS: 0x0EB00000             ;Image Flash Address
NOR5FILE: \SOFTWARE\mp_a15bc.dtb    ;Image File Name
NOR5LOAD: 0x84000000
NOR5ENTRY: 0x84000000

NOR6UPDATE: AUTO                 ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR6ADDRESS: 0x0EC00000          ;Image Flash Address
NOR6FILE: \SOFTWARE\init_mp.bin  ;Image File Name
NOR6LOAD: 0x85000000
NOR6ENTRY: 0x85000000

NOR7UPDATE: AUTO                 ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR7ADDRESS: 0x0C000000          ;Image Flash Address
NOR7FILE: \SOFTWARE\tc2_sec.bin   ;Image File Name
NOR7LOAD: 0
NOR7ENTRY: 0

NOR8UPDATE: AUTO                 ;IMAGE UPDATE:NONE/AUTO/FORCE
NOR8ADDRESS: 0x0D000000          ;Image Flash Address
NOR8FILE: \SOFTWARE\tc2_uefi.bin   ;Image File Name
NOR8LOAD: 0
NOR8ENTRY: 0

