1

2# -*- coding: utf-8 -*-

3

4 u'''Wrapper to invoke I{Karney}'s U{GeodSolve

5<https://GeographicLib.SourceForge.io/C++/doc/GeodSolve.1.html>} utility

6 as an (exact) geodesic, but intended I{for testing purposes only}.

7

8 Set env variable C{PYGEODESY_GEODSOLVE} to the (fully qualified) path

9 of the C{GeodSolve} executable.

10'''

11

12# from pygeodesy.basics import _xinstanceof # from .karney

13 from pygeodesy.interns import NN, _a12_, _azi1_, _azi2_, \

14 _lat1_, _lat2_, _lon1_, _lon2_, _m12_, \

15 _M12_, _M21_, _s12_, _S12_, _UNDER_

16 from pygeodesy.interns import _not_ # PYCHOK used!

17 from pygeodesy.karney import _Azi, Caps, _Deg, GeodesicError, _GTuple, \

18 _Pass, _Lat, _Lon, _M, _M2, _sincos2d, \

19 _xinstanceof, wrap360

20 from pygeodesy.lazily import _ALL_DOCS, _ALL_LAZY, _ALL_MODS as _MODS, \

21 _getenv, printf

22 from pygeodesy.namedTuples import Destination3Tuple, Distance3Tuple

23 from pygeodesy.props import Property, Property_RO

24 from pygeodesy.solveBase import _LineSolveBase, _SolveBase

25# from pygeodesy.utily import wrap360 # from .karney

26

27__all__ = _ALL_LAZY.geodsolve

28__version__ = '22.10.11'

29

30_PYGEODESY_GEODSOLVE_ = 'PYGEODESY_GEODSOLVE' # PYCHOK used!

31

32

33 class GeodSolve12Tuple(_GTuple):

34 '''12-Tuple C{(lat1, lon1, azi1, lat2, lon2, azi2, s12, a12, m12, M12, M21, S12)} with

35 angles C{lat1}, C{lon1}, C{azi1}, C{lat2}, C{lon2} and C{azi2} and arc C{a12} all in

36 C{degrees}, initial C{azi1} and final C{azi2} forward azimuths, distance C{s12} and

37 reduced length C{m12} in C{meter}, area C{S12} in C{meter} I{squared} and geodesic

38 scale factors C{M12} and C{M21}, both C{scalar}, see U{GeodSolve

39 <https://GeographicLib.SourceForge.io/C++/doc/GeodSolve.1.html>}.

40 '''

41 # from GeodSolve --help option -f ... lat1 lon1 azi1 lat2 lon2 azi2 s12 a12 m12 M12 M21 S12

42 _Names_ = (_lat1_, _lon1_, _azi1_, _lat2_, _lon2_, _azi2_, _s12_, _a12_, _m12_, _M12_, _M21_, _S12_)

43 _Units_ = (_Lat, _Lon, _Azi, _Lat, _Lon, _Azi, _M, _Deg, _Pass, _Pass, _Pass, _M2)

44

45

46 class _GeodesicSolveBase(_SolveBase):

47 '''(INTERNAL) Base class for L{GeodesicSolve} and L{GeodesicLineSolve}.

48 '''

49 _Error = GeodesicError

50 _Names_Direct = \

51 _Names_Inverse = GeodSolve12Tuple._Names_

52 _Solve_name = 'GeodSolve'

53 _Solve_path = _getenv(_PYGEODESY_GEODSOLVE_, _PYGEODESY_GEODSOLVE_)

54

55 @Property_RO

56 def _b_option(self):

57 return ('-b',) if self.reverse2 else ()

58

59 @Property_RO

60 def _cmdBasic(self):

61 '''(INTERNAL) Get the basic C{GeodSolve} cmd (C{tuple}).

62 '''

63 return (self.GeodSolve,) + self._b_option \

64 + self._e_option \

65 + self._E_option \

66 + self._p_option \

67 + self._u_option + ('-f',)

68

69 @Property_RO

70 def _E_option(self):

71 return ('-E',) if self.Exact else ()

72

73 @Property

74 def GeodSolve(self):

75 '''Get the U{GeodSolve<https://GeographicLib.SourceForge.io/C++/doc/GeodSolve.1.html>}

76 executable (C{filename}).

77 '''

78 return self._Solve_path

79

80 @GeodSolve.setter # PYCHOK setter!

81 def GeodSolve(self, path):

82 '''Set the U{GeodSolve<https://GeographicLib.SourceForge.io/C++/doc/GeodSolve.1.html>}

83 executable (C{filename}), the (fully qualified) path to the C{GeodSolve} executable.

84

85 @raise GeodesicError: Invalid B{C{path}}, B{C{path}} doesn't exist or

86 isn't the C{GeodSolve} executable.

87 '''

88 self._setSolve(path)

89

90 def toStr(self, **prec_sep): # PYCHOK signature

91 '''Return this C{GeodesicSolve} as string.

92

93 @kwarg prec_sep: Keyword argumens C{B{prec}=6} and C{B{sep}=', '}

94 for the C{float} C{prec}ision, number of decimal digits

95 (0..9) and the C{sep}arator string to join. Trailing

96 zero decimals are stripped for B{C{prec}} values of

97 1 and above, but kept for negative B{C{prec}} values.

98

99 @return: GeodesicSolve items (C{str}).

100 '''

101 return _SolveBase._toStr(self, GeodSolve=self.GeodSolve, **prec_sep)

102

103 @Property_RO

104 def _u_option(self):

105 return ('-u',) if self.unroll else ()

106

107

108 class GeodesicSolve(_GeodesicSolveBase):

109 '''Wrapper to invoke I{Karney}'s U{GeodSolve<https://GeographicLib.SourceForge.io/C++/doc/GeodSolve.1.html>}

110 as an C{Exact} version of I{Karney}'s Python class U{Geodesic<https://GeographicLib.SourceForge.io/C++/doc/

111 python/code.html#geographiclib.geodesic.Geodesic>}.

112

113 @note: Use property C{GeodSolve} or env variable C{PYGEODESY_GEODSOLVE} to specify the (fully

114 qualified) path to the C{GeodSolve} executable.

115

116 @note: This C{geodesic} is intended I{for testing purposes only}, it invokes the C{GeodSolve}

117 executable for I{every} method call.

118 '''

119

120 def Area(self, polyline=False, name=NN):

121 '''Set up a L{GeodesicAreaExact} to compute area and

122 perimeter of a polygon.

123

124 @kwarg polyline: If C{True} perimeter only, otherwise

125 area and perimeter (C{bool}).

126 @kwarg name: Optional name (C{str}).

127

128 @return: A L{GeodesicAreaExact} instance.

129

130 @note: The B{C{debug}} setting is passed as C{verbose}

131 to the returned L{GeodesicAreaExact} instance.

132 '''

133 gaX = _MODS.geodesicx.GeodesicAreaExact(self, polyline=polyline,

134 name=name or self.name)

135 if self.verbose or self.debug: # PYCHOK no cover

136 gaX.verbose = True

137 return gaX

138

139 Polygon = Area # for C{geographiclib} compatibility

140

141 def Direct3(self, lat1, lon1, azi1, s12): # PYCHOK outmask

142 '''Return the destination lat, lon and reverse azimuth

143 (final bearing) in C{degrees}.

144

145 @return: L{Destination3Tuple}C{(lat, lon, final)}.

146 '''

147 r = self._GDictDirect(lat1, lon1, azi1, False, s12, floats=False)

148 return Destination3Tuple(float(r.lat2), float(r.lon2), wrap360(r.azi2),

149 iteration=r._iteration)

150

151 def Inverse3(self, lat1, lon1, lat2, lon2): # PYCHOK outmask

152 '''Return the distance in C{meter} and the forward and

153 reverse azimuths (initial and final bearing) in C{degrees}.

154

155 @return: L{Distance3Tuple}C{(distance, initial, final)}.

156 '''

157 r = self._GDictInverse(lat1, lon1, lat2, lon2, floats=False)

158 return Distance3Tuple(float(r.s12), wrap360(r.azi1), wrap360(r.azi2),

159 iteration=r._iteration)

160

161 def Line(self, lat1, lon1, azi1, caps=Caps.ALL):

162 '''Set up a L{GeodesicLineSolve} to compute several points

163 on a single geodesic.

164

165 @arg lat1: Latitude of the first point (C{degrees}).

166 @arg lon1: Longitude of the first point (C{degrees}).

167 @arg azi1: Azimuth at the first point (compass C{degrees}).

168 @kwarg caps: Bit-or'ed combination of L{Caps} values specifying

169 the capabilities the L{GeodesicLineSolve} instance

170 should possess, always C{Caps.ALL}.

171

172 @return: A L{GeodesicLineSolve} instance.

173

174 @note: If the point is at a pole, the azimuth is defined by keeping

175 B{C{lon1}} fixed, writing C{B{lat1} = ±(90 − ε)}, and taking

176 the limit C{ε → 0+}.

177

178 @see: C++ U{GeodesicExact.Line

179 <https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1GeodesicExact.html>}

180 and Python U{Geodesic.Line<https://GeographicLib.SourceForge.io/C++/doc/python/code.html>}.

181 '''

182 return GeodesicLineSolve(self, lat1, lon1, azi1, caps=caps, name=self.name)

183

184

185 class GeodesicLineSolve(_GeodesicSolveBase, _LineSolveBase):

186 '''Wrapper to invoke I{Karney}'s U{GeodSolve<https://GeographicLib.SourceForge.io/C++/doc/GeodSolve.1.html>}

187 as an C{Exact} version of I{Karney}'s Python class U{GeodesicLine<https://GeographicLib.SourceForge.io/C++/doc/

188 python/code.html#geographiclib.geodesicline.GeodesicLine>}.

189

190 @note: Use property C{GeodSolve} or env variable C{PYGEODESY_GEODSOLVE} to specify the (fully

191 qualified) path to the C{GeodSolve} executable.

192

193 @note: This C{geodesic} is intended I{for testing purposes only}, it invokes the C{GeodSolve}

194 executable for I{every} method call.

195 '''

196

197 def __init__(self, geodesic, lat1, lon1, azi1, caps=Caps.ALL, name=NN):

198 '''New L{GeodesicLineSolve} instance, allowing points to be found along

199 a geodesic starting at C{(B{lat1}, B{lon1})} with azimuth B{C{azi1}}.

200

201 @arg geodesic: The geodesic to use (L{GeodesicSolve}).

202 @arg lat1: Latitude of the first point (C{degrees}).

203 @arg lon1: Longitude of the first point (C{degrees}).

204 @arg azi1: Azimuth at the first points (compass C{degrees}).

205 @kwarg caps: Bit-or'ed combination of L{Caps} values specifying

206 the capabilities the L{GeodesicLineSolve} instance

207 should possess, always C{Caps.ALL}. Use C{Caps.LINE_OFF}

208 if updates to the B{C{geodesic}} should I{not} be

209 reflected in this L{GeodesicLineSolve} instance.

210 @kwarg name: Optional name (C{str}).

211

212 @raise GeodesicError: Invalid path for the C{GeodSolve} executable or

213 or isn't the C{GeodSolve} executable, see

214 property C{geodesic.GeodSolve}.

215

216 @raise TypeError: Invalid B{C{geodesic}}.

217 '''

218 _xinstanceof(GeodesicSolve, geodesic=geodesic)

219 if (caps & Caps.LINE_OFF): # copy to avoid updates

220 geodesic = geodesic.copy(deep=False, name=NN(_UNDER_, geodesic.name))

221 _LineSolveBase.__init__(self, geodesic, lat1, lon1, caps, name, azi1=azi1)

222 try:

223 self.GeodSolve = geodesic.GeodSolve # geodesic or copy of geodesic

224 except GeodesicError:

225 pass

226

227 def ArcPosition(self, a12, *unused):

228 '''Find the position on the line given B{C{a12}}.

229

230 @arg a12: Spherical arc length from the first point to the

231 second point (C{degrees}).

232

233 @return: A C{GDict} with 12 items C{lat1, lon1, azi1, lat2, lon2,

234 azi2, m12, a12, s12, M12, M21, S12}.

235 '''

236 return self._GDictInvoke(self._cmdArc, True, self._Names_Direct, a12)

237

238 @Property_RO

239 def azi1(self):

240 '''Get the azimuth at the first point (compass C{degrees}).

241 '''

242 return self._lla1.azi1

243

244 azi12 = azi1 # like RhumbLineSolve

245

246 @Property_RO

247 def azi1_sincos2(self):

248 '''Get the sine and cosine of the first point's azimuth (2-tuple C{(sin, cos)}).

249 '''

250 return _sincos2d(self.azi1)

251

252 azi12_sincos2 = azi1_sincos2

253

254 @Property_RO

255 def _cmdArc(self):

256 '''(INTERNAL) Get the C{GeodSolve} I{-a -L} cmd (C{tuple}).

257 '''

258 return self._cmdDistance + ('-a',)

259

260 def Position(self, s12, *unused):

261 '''Find the position on the line given B{C{s12}}.

262

263 @arg s12: Distance from the first point to the second (C{meter}).

264

265 @return: A C{GDict} with 12 items C{lat1, lon1, azi1, lat2, lon2,

266 azi2, m12, a12, s12, M12, M21, S12}, possibly C{a12=NAN}.

267 '''

268 return self._GDictInvoke(self._cmdDistance, True, self._Names_Direct, s12)

269

270 def toStr(self, **prec_sep): # PYCHOK signature

271 '''Return this C{GeodesicLineSolve} as string.

272

273 @kwarg prec_sep: Keyword argumens C{B{prec}=6} and C{B{sep}=', '}

274 for the C{float} C{prec}ision, number of decimal digits

275 (0..9) and the C{sep}arator string to join. Trailing

276 zero decimals are stripped for B{C{prec}} values of

277 1 and above, but kept for negative B{C{prec}} values.

278

279 @return: GeodesicLineSolve items (C{str}).

280 '''

281 return _LineSolveBase._toStr(self, azi1=self.azi1, geodesic=self._solve,

282 GeodSolve=self.GeodSolve, **prec_sep)

283

284

285__all__ += _ALL_DOCS(_GeodesicSolveBase)

286

287 if __name__ == '__main__':

288

289 from sys import argv

290

291 gS = GeodesicSolve(name='Test')

292 gS.verbose = '--verbose' in argv # or '-v' in argv

293

294 if gS.GeodSolve in (_PYGEODESY_GEODSOLVE_, None): # not set

295 gS.GeodSolve = '/opt/local/bin/GeodSolve' # '/opt/local/Cellar/geographiclib/1.51/bin/GeodSolve' # HomeBrew

296 printf('version: %s', gS.version)

297

298 r = gS.Direct(40.6, -73.8, 51, 5.5e6)

299 printf('Direct: %r', r, nl=1)

300 printf('Direct3: %r', gS.Direct3(40.6, -73.8, 51, 5.5e6))

301

302 printf('Inverse: %r', gS.Inverse( 40.6, -73.8, 51.6, -0.5), nl=1)

303 printf('Inverse1: %r', gS.Inverse1(40.6, -73.8, 51.6, -0.5))

304 printf('Inverse3: %r', gS.Inverse3(40.6, -73.8, 51.6, -0.5))

305

306 glS = GeodesicLineSolve(gS, 40.6, -73.8, 51, name='LineTest')

307 p = glS.Position(5.5e6)

308 printf('Position: %s %r', p == r, p, nl=1)

309 p = glS.ArcPosition(49.475527)

310 printf('ArcPosition: %s %r', p == r, p)

311

312# % python3 -m pygeodesy.geodsolve

313

314# version: /opt/local/bin/GeodSolve: GeographicLib version 1.51

315

316# version: /opt/local/bin/GeodSolve: GeographicLib version 1.51

317

318# Direct: GDict(M12=0.650911, M21=0.651229, S12=39735075134877.09375, a12=49.475527, azi1=51.0, azi2=107.189397, lat1=40.6, lat2=51.884565, lon1=-73.8, lon2=-1.141173, m12=4844148.703101, s12=5500000.0)

319# Direct3: Destination3Tuple(lat=51.884565, lon=-1.141173, final=107.189397)

320

321# Inverse: GDict(M12=0.64473, M21=0.645046, S12=40041368848742.53125, a12=49.94131, azi1=51.198883, azi2=107.821777, lat1=40.6, lat2=51.6, lon1=-73.8, lon2=-0.5, m12=4877684.602706, s12=5551759.400319)

322# Inverse1: 49.94131021789904

323# Inverse3: Distance3Tuple(distance=5551759.400319, initial=51.198883, final=107.821777)

324

325# Position: True GDict(M12=0.650911, M21=0.651229, S12=39735075134877.09375, a12=49.475527, azi1=51.0, azi2=107.189397, lat1=40.6, lat2=51.884565, lon1=-73.8, lon2=-1.141173, m12=4844148.703101, s12=5500000.0)

326# ArcPosition: False GDict(M12=0.650911, M21=0.651229, S12=39735074737272.734375, a12=49.475527, azi1=51.0, azi2=107.189397, lat1=40.6, lat2=51.884565, lon1=-73.8, lon2=-1.141174, m12=4844148.669561, s12=5499999.948497)

327

328

329# % python3 -m pygeodesy.geodsolve --verbose

330

331# GeodesicSolve 'Test' 1: /opt/local/bin/GeodSolve --version (invoke)

332# GeodesicSolve 'Test' 1: /opt/local/bin/GeodSolve: GeographicLib version 1.51 (0)

333# version: /opt/local/bin/GeodSolve: GeographicLib version 1.51

334# GeodesicSolve 'Test' 2: /opt/local/bin/GeodSolve -E -p 10 -f \ 40.600000000000001 -73.799999999999997 51.0 5500000.0 (Direct)

335# GeodesicSolve 'Test' 2: lat1=40.600000000000001, lon1=-73.799999999999997, azi1=51.0, lat2=51.884564505606761, lon2=-1.141172861200829, azi2=107.189397162605886, s12=5500000.0, a12=49.475527463251467, m12=4844148.703101486, M12=0.65091056699808603, M21=0.65122865892196558, S12=39735075134877.094 (0)

336

337# Direct: GDict(M12=0.650911, M21=0.651229, S12=39735075134877.09375, a12=49.475527, azi1=51.0, azi2=107.189397, lat1=40.6, lat2=51.884565, lon1=-73.8, lon2=-1.141173, m12=4844148.703101, s12=5500000.0)

338# GeodesicSolve 'Test' 3: /opt/local/bin/GeodSolve -E -p 10 -f \ 40.600000000000001 -73.799999999999997 51.0 5500000.0 (Direct3)

339# GeodesicSolve 'Test' 3: lat1=40.600000000000001, lon1=-73.799999999999997, azi1=51.0, lat2=51.884564505606761, lon2=-1.141172861200829, azi2=107.189397162605886, s12=5500000.0, a12=49.475527463251467, m12=4844148.703101486, M12=0.65091056699808603, M21=0.65122865892196558, S12=39735075134877.094 (0)

340# Direct3: Destination3Tuple(lat=51.884565, lon=-1.141173, final=107.189397)

341# GeodesicSolve 'Test' 4: /opt/local/bin/GeodSolve -E -p 10 -f -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse)

342# GeodesicSolve 'Test' 4: lat1=40.600000000000001, lon1=-73.799999999999997, azi1=51.198882845579824, lat2=51.600000000000001, lon2=-0.5, azi2=107.821776735514248, s12=5551759.4003186841, a12=49.941310217899037, m12=4877684.6027061976, M12=0.64472969205948238, M21=0.64504567852134398, S12=40041368848742.531 (0)

343

344# Inverse: GDict(M12=0.64473, M21=0.645046, S12=40041368848742.53125, a12=49.94131, azi1=51.198883, azi2=107.821777, lat1=40.6, lat2=51.6, lon1=-73.8, lon2=-0.5, m12=4877684.602706, s12=5551759.400319)

345# GeodesicSolve 'Test' 5: /opt/local/bin/GeodSolve -E -p 10 -f -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse1)

346# GeodesicSolve 'Test' 5: lat1=40.600000000000001, lon1=-73.799999999999997, azi1=51.198882845579824, lat2=51.600000000000001, lon2=-0.5, azi2=107.821776735514248, s12=5551759.4003186841, a12=49.941310217899037, m12=4877684.6027061976, M12=0.64472969205948238, M21=0.64504567852134398, S12=40041368848742.531 (0)

347# Inverse1: 49.94131021789904

348# GeodesicSolve 'Test' 6: /opt/local/bin/GeodSolve -E -p 10 -f -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse3)

349# GeodesicSolve 'Test' 6: lat1=40.600000000000001, lon1=-73.799999999999997, azi1=51.198882845579824, lat2=51.600000000000001, lon2=-0.5, azi2=107.821776735514248, s12=5551759.4003186841, a12=49.941310217899037, m12=4877684.6027061976, M12=0.64472969205948238, M21=0.64504567852134398, S12=40041368848742.531 (0)

350# Inverse3: Distance3Tuple(distance=5551759.400319, initial=51.198883, final=107.821777)

351

352# Position: True GDict(M12=0.650911, M21=0.651229, S12=39735075134877.09375, a12=49.475527, azi1=51.0, azi2=107.189397, lat1=40.6, lat2=51.884565, lon1=-73.8, lon2=-1.141173, m12=4844148.703101, s12=5500000.0)

353# ArcPosition: False GDict(M12=0.650911, M21=0.651229, S12=39735074737272.734375, a12=49.475527, azi1=51.0, azi2=107.189397, lat1=40.6, lat2=51.884565, lon1=-73.8, lon2=-1.141174, m12=4844148.669561, s12=5499999.948497)

354

355

356# **) MIT License

357#

358# Copyright (C) 2016-2023 -- mrJean1 at Gmail -- All Rights Reserved.

359#

360# Permission is hereby granted, free of charge, to any person obtaining a

361# copy of this software and associated documentation files (the "Software"),

362# to deal in the Software without restriction, including without limitation

363# the rights to use, copy, modify, merge, publish, distribute, sublicense,

364# and/or sell copies of the Software, and to permit persons to whom the

365# Software is furnished to do so, subject to the following conditions:

366#

367# The above copyright notice and this permission notice shall be included

368# in all copies or substantial portions of the Software.

369#

370# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

371# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

372# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

373# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

374# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

375# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

376# OTHER DEALINGS IN THE SOFTWARE.