1

2# -*- coding: utf-8 -*-

3

4 u'''Base classes C{RhumbBase} and C{RhumbLineBase}, pure Python version of I{Karney}'s C++

5 classes U{Rhumb<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1Rhumb.html>}

6 and U{RhumbLine<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1RhumbLine.html>}

7 from I{GeographicLib versions 2.0} and I{2.2} and I{Karney}'s C++ example U{Rhumb intersect

8<https://SourceForge.net/p/geographiclib/discussion/1026620/thread/2ddc295e/>}.

9

10 Class L{RhumbLine} has been enhanced with methods C{intersection2} and C{nearestOn4} to iteratively

11 find the intersection of two rhumb lines, respectively the nearest point on a rumb line along a

12 geodesic or perpendicular rhumb line.

13

14 For more details, see the C++ U{GeographicLib<https://GeographicLib.SourceForge.io/C++/doc/index.html>}

15 documentation, especially the U{Class List<https://GeographicLib.SourceForge.io/C++/doc/annotated.html>},

16 the background information on U{Rhumb lines<https://GeographicLib.SourceForge.io/C++/doc/rhumb.html>},

17 the utily U{RhumbSolve<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>} and U{Online

18 rhumb line calculations<https://GeographicLib.SourceForge.io/cgi-bin/RhumbSolve>}.

19

20 Copyright (C) U{Charles Karney<mailto:Karney@Alum.MIT.edu>} (2014-2023) and licensed under the MIT/X11

21 License. For more information, see the U{GeographicLib<https://GeographicLib.SourceForge.io>} documentation.

22'''

23# make sure int/int division yields float quotient

24 from __future__ import division as _; del _ # PYCHOK semicolon

25

26# from pygeodesy.basics import _xinstanceof # from .karney

27 from pygeodesy.constants import EPS, EPS1, INT0, _EPSqrt as _TOL, \

28 _0_0, _0_01, _1_0, _90_0, _180_0

29# from pygeodesy.datums import _spherical_datum # _MODS

30# from pygeodesy.ellipsoids import _EWGS84 # from .karney

31 from pygeodesy.errors import IntersectionError, itemsorted, RhumbError, \

32 _xdatum, _xkwds, _Xorder

33# from pygeodesy.etm import ExactTransverseMercator # _MODS

34 from pygeodesy.fmath import euclid, favg, fabs

35# from pygeodesy.fsums import Fsum # _MODS

36 from pygeodesy.interns import NN, _coincident_, _COMMASPACE_, _intersection_, \

37 _no_, _parallel_, _under

38 from pygeodesy.karney import Caps, _CapsBase, _diff182, _fix90, _norm180, \

39 _EWGS84, _xinstanceof

40 from pygeodesy.ktm import KTransverseMercator, _AlpCoeffs # PYCHOK used!

41 from pygeodesy.lazily import _ALL_DOCS, _ALL_MODS as _MODS

42# from pygeodesy.named import notOverloaded # _MODS

43 from pygeodesy.namedTuples import Distance2Tuple, LatLon2Tuple, NearestOn4Tuple

44 from pygeodesy.props import Property, Property_RO, property_RO, _update_all

45 from pygeodesy.streprs import Fmt, pairs, unstr

46 from pygeodesy.units import Float_, Lat, Lon, Meter

47 from pygeodesy.utily import sincos2d, sincos2d_, _unrollon, _Wrap

48 from pygeodesy.vector3d import _intersect3d3, Vector3d # in .intersection2 below

49

50# from math import fabs # from .fmath

51

52__all__ = ()

53__version__ = '23.08.20'

54

55_rls = [] # instances of C{RbumbLine...} to be updated

56_TRIPS = 65 # .intersection2, .nearestOn4, 18+

57

58

59 class _Lat(Lat):

60 '''(INTERNAL) Latitude B{C{lat}}.

61 '''

62 def __init__(self, *lat, **Error_name):

63 kwds = _xkwds(Error_name, clip=0, Error=RhumbError)

64 Lat.__new__(_Lat, *lat, **kwds)

65

66

67 class _Lon(Lon):

68 '''(INTERNAL) Longitude B{C{lon}}.

69 '''

70 def __init__(self, *lon, **Error_name):

71 kwds = _xkwds(Error_name, clip=0, Error=RhumbError)

72 Lon.__new__(_Lon, *lon, **kwds)

73

74

75 def _update_all_rls(r):

76 '''(INTERNAL) Zap cached/memoized C{Property[_RO]}s

77 of any C{RhumbLine} instances tied to the given

78 C{Rhumb} instance B{C{r}}.

79 '''

80 # _xinstanceof(_MODS.rhumbaux.RhumbAux, _MODS.rhumbx.Rhumb, r=r)

81 _update_all(r)

82 for rl in _rls: # PYCHOK use weakref?

83 if rl._rhumb is r:

84 _update_all(rl)

85

86

87 class RhumbBase(_CapsBase):

88 '''(INTERNAL) Base class for C{rhumbaux.RhumbAux} and C{rhumbx.Rhumb}.

89 '''

90 _E = _EWGS84

91 _exact = True

92 _f_max = _0_01

93 _mTM = 6 # see .TMorder

94

95 def __init__(self, a_earth, f, exact, name):

96 '''New C{rhumbaux.RhumbAux} or C{rhumbx.Rhum}.

97 '''

98 if f is not None:

99 self.ellipsoid = a_earth, f

100 elif a_earth not in (_EWGS84, None):

101 self.ellipsoid = a_earth

102 if not exact:

103 self.exact = False

104 if name:

105 self.name = name

106

107 @Property_RO

108 def a(self):

109 '''Get the C{ellipsoid}'s equatorial radius, semi-axis (C{meter}).

110 '''

111 return self.ellipsoid.a

112

113 equatoradius = a

114

115 @Property_RO

116 def b(self):

117 '''Get the C{ellipsoid}'s polar radius, semi-axis (C{meter}).

118 '''

119 return self.ellipsoid.b

120

121 polaradius = b

122

123 def _Direct(self, ll1, azi12, s12, **outmask):

124 '''(INTERNAL) Short-cut version, see .latlonBase.

125 '''

126 return self.Direct(ll1.lat, ll1.lon, azi12, s12, **outmask)

127

128 def Direct(self, lat1, lon1, azi12, s12, outmask=0): # PYCHOK no cover

129 '''I{Must be overloaded}, see function C{notOverloaded}.

130 '''

131 _MODS.named.notOverloaded(self, lat1, lon1, azi12, s12, outmask=outmask)

132

133 def Direct8(self, lat1, lon1, azi12, s12, outmask=Caps.LATITUDE_LONGITUDE_AREA):

134 '''Like method L{Rhumb.Direct} but returning a L{Rhumb8Tuple} with area C{S12}.

135 '''

136 return self.Direct(lat1, lon1, azi12, s12, outmask=outmask).toRhumb8Tuple()

137

138 def _DirectLine(self, ll1, azi12, **caps_name):

139 '''(INTERNAL) Short-cut version, see .latlonBase.

140 '''

141 return self.DirectLine(ll1.lat, ll1.lon, azi12, **caps_name)

142

143 def DirectLine(self, lat1, lon1, azi12, **caps_name):

144 '''Define a C{RhumbLine} in terms of the I{direct} rhumb

145 problem to compute several points on a single rhumb line.

146

147 @arg lat1: Latitude of the first point (C{degrees90}).

148 @arg lon1: Longitude of the first point (C{degrees180}).

149 @arg azi12: Azimuth of the rhumb line (compass C{degrees}).

150 @kwarg caps_name: Optional keyword arguments C{B{name}=NN} and

151 C{B{caps}=Caps.STANDARD}, a bit-or'ed combination of

152 L{Caps} values specifying the required capabilities.

153 Include C{Caps.LINE_OFF} if updates to the B{C{rhumb}}

154 should I{not} be reflected in this rhumb line.

155

156 @return: A C{RhumbLine...} instance and invoke its method

157 C{.Position} to compute each point.

158

159 @note: Updates to this rhumb are reflected in the returned

160 rhumb line, unless C{B{caps} |= Caps.LINE_OFF}.

161 '''

162 return self._RhumbLine(self, lat1=lat1, lon1=lon1, azi12=azi12,

163 **caps_name)

164

165 Line = DirectLine # synonyms

166

167 @Property

168 def ellipsoid(self):

169 '''Get this rhumb's ellipsoid (L{Ellipsoid}).

170 '''

171 return self._E

172

173 @ellipsoid.setter # PYCHOK setter!

174 def ellipsoid(self, a_earth_f):

175 '''Set this rhumb's ellipsoid (L{Ellipsoid}, L{Ellipsoid2}, L{Datum} or

176 L{a_f2Tuple}) or (equatorial) radius and flattening (2-tuple C{(a, f)}).

177

178 @raise RhumbError: If C{abs(B{f}} exceeds non-zero C{f_max} and C{exact=False}.

179 '''

180 E = _MODS.datums._spherical_datum(a_earth_f, Error=RhumbError).ellipsoid

181 if self._E != E:

182 self._exactest(self.exact, E, self.f_max)

183 _update_all_rls(self)

184 self._E = E

185

186 @Property

187 def exact(self):

188 '''Get the I{exact} option (C{bool}).

189 '''

190 return self._exact

191

192 @exact.setter # PYCHOK setter!

193 def exact(self, exact):

194 '''Set the I{exact} option (C{bool}). If C{True}, use I{exact} rhumb

195 expressions, otherwise a series expansion (accurate for oblate or

196 prolate ellipsoids with C{abs(flattening)} below C{f_max}.

197

198 @raise RhumbError: If C{B{exact}=False} and C{abs(flattening})

199 exceeds non-zero C{f_max}.

200

201 @see: Option U{B{-s}<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>}

202 and U{ACCURACY<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html#ACCURACY>}.

203 '''

204 x = bool(exact)

205 if self._exact != x:

206 self._exactest(x, self.ellipsoid, self.f_max)

207 _update_all_rls(self)

208 self._exact = x

209

210 def _exactest(self, exact, ellipsoid, f_max):

211 # Helper for property setters C{ellipsoid}, C{exact} and C{f_max}

212 if fabs(ellipsoid.f) > f_max > 0 and not exact:

213 raise RhumbError(exact=exact, f=ellipsoid.f, f_max=f_max)

214

215 @Property_RO

216 def f(self):

217 '''Get the C{ellipsoid}'s flattening (C{float}).

218 '''

219 return self.ellipsoid.f

220

221 flattening = f

222

223 @property

224 def f_max(self):

225 '''Get the I{max.} flattening (C{float}).

226 '''

227 return self._f_max

228

229 @f_max.setter # PYCHOK setter!

230 def f_max(self, f_max): # PYCHOK no cover

231 '''Set the I{max.} flattening, not to exceed (C{float}).

232

233 @raise RhumbError: If C{exact=False} and C{abs(flattening})

234 exceeds non-zero C{f_max}.

235 '''

236 f = Float_(f_max=f_max, low=_0_0, high=EPS1)

237 if self._f_max != f:

238 self._exactest(self.exact, self.ellipsoid, f)

239 self._f_max = f

240

241 def _Inverse(self, ll1, ll2, wrap, **outmask):

242 '''(INTERNAL) Short-cut version, see .latlonBase.

243 '''

244 if wrap:

245 ll2 = _unrollon(ll1, _Wrap.point(ll2))

246 return self.Inverse(ll1.lat, ll1.lon, ll2.lat, ll2.lon, **outmask)

247

248 def Inverse(self, lat1, lon1, lat2, lon2, outmask=0): # PYCHOK no cover

249 '''I{Must be overloaded}, see function C{notOverloaded}.

250 '''

251 _MODS.named.notOverloaded(self, lat1, lon1, lat2, lon2, outmask=outmask)

252

253 def Inverse8(self, lat1, lon1, azi12, s12, outmask=Caps.AZIMUTH_DISTANCE_AREA):

254 '''Like method L{Rhumb.Inverse} but returning a L{Rhumb8Tuple} with area C{S12}.

255 '''

256 return self.Inverse(lat1, lon1, azi12, s12, outmask=outmask).toRhumb8Tuple()

257

258 def _InverseLine(self, ll1, ll2, wrap, **caps_name):

259 '''(INTERNAL) Short-cut version, see .latlonBase.

260 '''

261 if wrap:

262 ll2 = _unrollon(ll1, _Wrap.point(ll2))

263 return self.InverseLine(ll1.lat, ll1.lon, ll2.lat, ll2.lon, **caps_name)

264

265 def InverseLine(self, lat1, lon1, lat2, lon2, **caps_name):

266 '''Define a C{RhumbLine} in terms of the I{inverse} rhumb problem.

267

268 @arg lat1: Latitude of the first point (C{degrees90}).

269 @arg lon1: Longitude of the first point (C{degrees180}).

270 @arg lat2: Latitude of the second point (C{degrees90}).

271 @arg lon2: Longitude of the second point (C{degrees180}).

272 @kwarg caps_name: Optional keyword arguments C{B{name}=NN} and

273 C{B{caps}=Caps.STANDARD}, a bit-or'ed combination of

274 L{Caps} values specifying the required capabilities.

275 Include C{Caps.LINE_OFF} if updates to the B{C{rhumb}}

276 should I{not} be reflected in this rhumb line.

277

278 @return: A C{RhumbLine...} instance and invoke its method

279 C{.Position} to compute each point.

280

281 @note: Updates to this rhumb are reflected in the returned

282 rhumb line, unless C{B{caps} |= Caps.LINE_OFF}.

283 '''

284 r = self.Inverse(lat1, lon1, lat2, lon2, outmask=Caps.AZIMUTH)

285 return self._RhumbLine(self, lat1=lat1, lon1=lon1, azi12=r.azi12,

286 **caps_name)

287

288 @Property_RO

289 def _RhumbLine(self): # PYCHOK no cover

290 '''I{Must be overloaded}, see function C{notOverloaded}.

291 '''

292 _MODS.named.notOverloaded(self)

293

294 def _TMorder(self, order):

295 '''(INTERNAL) Set the I{Transverse Mercator} order (C{int}).

296

297 @note: Setting C{TMorder} turns property C{exact} off.

298 '''

299 x = self.exact

300 n = _Xorder(_MODS.ktm._AlpCoeffs, RhumbError, TMorder=order)

301 if self._mTM != n:

302 _update_all_rls(self)

303 self._mTM = n

304 x = False

305 return x

306

307 def toStr(self, prec=6, sep=_COMMASPACE_, **unused): # PYCHOK no cover

308 '''I{Must be overloaded}, see function C{notOverloaded}.

309 '''

310 _MODS.named.notOverloaded(self, prec=prec, sep=sep)

311

312

313 class RhumbLineBase(RhumbBase):

314 '''(INTERNAL) Class C{RhumbLine}

315 '''

316 _azi12 = _0_0

317# _caps = 0

318# _debug = 0

319# _lat1 = _0_0

320# _lon1 = _0_0

321# _lon12 = _0_0

322 _salp = _0_0

323 _calp = _1_0

324 _Rhumb = RhumbBase # compatible C{Rhumb} class

325 _rhumb = None # C{Rhumb} instance

326

327 def __init__(self, rhumb, lat1, lon1, azi12, caps=Caps.STANDARD, name=NN):

328 '''New C{RhumbLine}.

329 '''

330 _xinstanceof(self._Rhumb, rhumb=rhumb)

331

332 self._lat1 = _Lat(lat1=_fix90(lat1))

333 self._lon1 = _Lon(lon1= lon1)

334 self._lon12 = _norm180(self._lon1)

335 if azi12: # non-zero, non-None

336 self.azi12 = _norm180(azi12)

337

338 n = name or rhumb.name

339 if n:

340 self.name=n

341

342 self._caps = caps

343 self._debug |= (caps | rhumb._debug) & Caps._DEBUG_DIRECT_LINE

344 if (caps & Caps.LINE_OFF): # copy to avoid updates

345 self._rhumb = rhumb.copy(deep=False, name=_under(rhumb.name))

346 else:

347 self._rhumb = rhumb

348 _rls.append(self)

349

350 def __del__(self): # XXX use weakref?

351 if _rls: # may be empty or None

352 try: # PYCHOK no cover

353 _rls.remove(self)

354 except (TypeError, ValueError):

355 pass

356 self._rhumb = None

357 # _update_all(self) # throws TypeError during Python 2 cleanup

358

359 @Property

360 def azi12(self):

361 '''Get this rhumb line's I{azimuth} (compass C{degrees}).

362 '''

363 return self._azi12

364

365 @azi12.setter # PYCHOK setter!

366 def azi12(self, azi12):

367 '''Set this rhumb line's I{azimuth} (compass C{degrees}).

368 '''

369 z = _norm180(azi12)

370 if self._azi12 != z:

371 if self._rhumb:

372 _update_all(self)

373 self._azi12 = z

374 self._salp, self._calp = sincos2d(z) # no NEG0

375

376 @property_RO

377 def azi12_sincos2(self): # PYCHOK no cover

378 '''Get this rhumb line's I{azimuth} sine and cosine (2-tuple C{(sin, cos)}).

379 '''

380 return self._scalp, self._calp

381

382 def distance2(self, lat, lon):

383 '''Return the distance from and (initial) bearing at the given

384 point to this rhumb line's start point.

385

386 @arg lat: Latitude of the point (C{degrees}).

387 @arg lon: Longitude of the points (C{degrees}).

388

389 @return: A L{Distance2Tuple}C{(distance, initial)} with the C{distance}

390 in C{meter} and C{initial} bearing in C{degrees}.

391

392 @see: Methods C{intersection2} and C{nearestOn4} of L{RhumbLine} and

393 L{RhumbLineAux}.

394 '''

395 r = self.rhumb.Inverse(self.lat1, self.lon1, lat, lon)

396# outmask=Caps.AZIMUTH_DISTANCE)

397 return Distance2Tuple(r.s12, r.azi12)

398

399 @property_RO

400 def ellipsoid(self):

401 '''Get this rhumb line's ellipsoid (L{Ellipsoid}).

402 '''

403 return self.rhumb.ellipsoid

404

405 @property_RO

406 def exact(self):

407 '''Get this rhumb line's I{exact} option (C{bool}).

408 '''

409 return self.rhumb.exact

410

411 def intersection2(self, other, tol=_TOL, **eps):

412 '''I{Iteratively} find the intersection of this and an other rhumb line.

413

414 @arg other: The other rhumb line (C{RhumbLine}).

415 @kwarg tol: Tolerance for longitudinal convergence (C{degrees}).

416 @kwarg eps: Tolerance for L{pygeodesy.intersection3d3} (C{EPS}).

417

418 @return: A L{LatLon2Tuple}{(lat, lon)} with the C{lat}- and

419 C{lon}gitude of the intersection point.

420

421 @raise IntersectionError: No convergence for this B{C{tol}} or

422 no intersection for an other reason.

423

424 @see: Methods C{distance2} and C{nearestOn4} and function

425 L{pygeodesy.intersection3d3}.

426

427 @note: Each iteration involves a round trip to this rhumb line's

428 L{ExactTransverseMercator} or L{KTransverseMercator}

429 projection and invoking function L{pygeodesy.intersection3d3}

430 in that domain.

431 '''

432 _xinstanceof(RhumbLineBase, other=other)

433 _xdatum(self.rhumb, other.rhumb, Error=RhumbError)

434 try:

435 if other is self:

436 raise ValueError(_coincident_)

437 # make globals and invariants locals

438 _diff = euclid # approximate length

439 _i3d3 = _intersect3d3 # NOT .vector3d.intersection3d3

440 _LL2T = LatLon2Tuple

441 _xTMr = self.xTM.reverse # ellipsoidal or spherical

442 _s_3d, s_az = self._xTM3d, self.azi12

443 _o_3d, o_az = other._xTM3d, other.azi12

444 t = fabs(s_az - o_az)

445 if t < EPS or fabs(t - _180_0) < EPS:

446 raise ValueError(_parallel_)

447 # use halfway point as initial estimate

448 p = _LL2T(favg(self.lat1, other.lat1),

449 favg(self.lon1, other.lon1))

450 for i in range(1, _TRIPS):

451 v = _i3d3(_s_3d(p), s_az, # point + bearing

452 _o_3d(p), o_az, useZ=False, **eps)[0]

453 t = _xTMr(v.x, v.y, lon0=p.lon) # PYCHOK Reverse4Tuple

454 d = _diff(t.lon - p.lon, t.lat) # PYCHOK t.lat + p.lat - p.lat

455 p = _LL2T(t.lat + p.lat, t.lon) # PYCHOK t.lon + p.lon = lon0

456 if d < tol:

457 return _LL2T(p.lat, p.lon, iteration=i, # PYCHOK p...

458 name=self.intersection2.__name__)

459 except Exception as x:

460 raise IntersectionError(_no_(_intersection_), cause=x)

461 t = unstr(self.intersection2, tol=tol, **eps)

462 raise IntersectionError(Fmt.no_convergence(d), txt=t)

463

464 @Property_RO

465 def isLoxodrome(self):

466 '''Is this rhumb line a loxodrome (C{True} if non-meridional and

467 non-parallel, C{False} if parallel or C{None} if meridional)?

468

469 @see: I{Osborne's} U{2.5 Rumb lines and loxodromes

470 <https://Zenodo.org/record/35392>}, page 37.

471 '''

472 return bool(self._salp) if self._calp else None

473

474 @Property_RO

475 def lat1(self):

476 '''Get this rhumb line's latitude (C{degrees90}).

477 '''

478 return self._lat1

479

480 @Property_RO

481 def lon1(self):

482 '''Get this rhumb line's longitude (C{degrees180}).

483 '''

484 return self._lon1

485

486 @Property_RO

487 def latlon1(self):

488 '''Get this rhumb line's lat- and longitude (L{LatLon2Tuple}C{(lat, lon)}).

489 '''

490 return LatLon2Tuple(self.lat1, self.lon1)

491

492 def _mu22(self, mu12, mu1):

493 mu2 = mu12 + mu1

494 x90 = fabs(mu2) > 90

495 if x90: # reduce to [-180, 180)

496 mu2 = _norm180(mu2)

497 if fabs(mu2) > 90: # point on anti-meridian

498 mu2 = _norm180(_180_0 - mu2)

499 return mu2, x90

500

501 def nearestOn4(self, lat, lon, tol=_TOL, exact=None, eps=EPS, est=None):

502 '''I{Iteratively} locate the point on this rhumb line nearest to the

503 given point, in part transcoded from I{Karney}'s C++ U{rhumb-intercept

504 <https://SourceForge.net/p/geographiclib/discussion/1026620/thread/2ddc295e/>}.

505

506 @arg lat: Latitude of the point (C{degrees}).

507 @arg lon: Longitude of the point (C{degrees}).

508 @kwarg tol: Longitudinal convergence tolerance (C{degrees}) or the

509 distance tolerance (C(meter)) when C{B{exact} is None},

510 respectively C{B{exact} is not None}.

511 @kwarg exact: If C{None}, use a rhumb line perpendicular to this rhumb

512 line, otherwise use an I{exact} C{Geodesic...} from the

513 given point perpendicular to this rhumb line (C{bool} or

514 C{Geodesic...}), see method L{Ellipsoid.geodesic_}.

515 @kwarg eps: Optional tolerance for L{pygeodesy.intersection3d3}

516 (C{EPS}), used only if C{B{exact} is None}.

517 @kwarg est: Optional, initial estimate for the distance C{s13} of

518 the intersection I{along} this rhumb line (C{meter}),

519 used only if C{B{exact} is not None}.

520

521 @return: A L{NearestOn4Tuple}C{(lat, lon, distance, normal)} with

522 the C{lat}- and C{lon}gitude of the nearest point on and

523 the C{distance} in C{meter} to this rhumb line and the

524 C{normal} azimuth at the intersection.

525

526 @raise ImportError: I{Karney}'s U{geographiclib

527 <https://PyPI.org/project/geographiclib>}

528 package not found or not installed.

529

530 @raise IntersectionError: No convergence for this B{C{eps}} or

531 no intersection for an other reason.

532

533 @see: Methods C{distance2} and C{intersection2} and function

534 L{pygeodesy.intersection3d3}.

535 '''

536 if exact is None:

537 z = _norm180(self.azi12 + _90_0) # perpendicular azimuth

538 rl = RhumbLineBase(self.rhumb, lat, lon, z, caps=Caps.LINE_OFF)

539 p = self.intersection2(rl, tol=tol, eps=eps)

540 t = rl.distance2(p.lat, p.lon)

541 r = NearestOn4Tuple(p.lat, p.lon, t.distance, z,

542 iteration=p.iteration)

543 else: # C{rhumb-intercept}

544 azi = self.azi12

545 szi = self._salp

546 E = self.ellipsoid

547 gX = E.geodesic_(exact=exact)

548 Cs = Caps

549 gm = Cs.AZIMUTH | Cs.LATITUDE_LONGITUDE | Cs.REDUCEDLENGTH | Cs.GEODESICSCALE

550 if est is None: # get an estimate from the perpendicular

551 r = gX.Inverse(self.lat1, self.lon1, lat, lon, outmask=Cs.AZIMUTH_DISTANCE)

552 d, _ = _diff182(r.azi2, azi, K_2_0=True)

553 _, c = sincos2d(d)

554 s12 = c * r.s12 # signed

555 else:

556 s12 = Meter(est=est)

557 try:

558 tol = Float_(tol=tol, low=EPS, high=None)

559 # def _over(p, q): # see @note at RhumbLine[Aux].Position

560 # return (p / (q or _copysign(tol, q))) if isfinite(q) else NAN

561

562 _s12 = _MODS.fsums.Fsum(s12).fsum2_

563 for i in range(1, _TRIPS): # suffix 1 == C++ 2, 2 == C++ 3

564 p = self.Position(s12) # outmask=Cs.LATITUDE_LONGITUDE

565 r = gX.Inverse(lat, lon, p.lat2, p.lon2, outmask=gm)

566 d, _ = _diff182(azi, r.azi2, K_2_0=True)

567 s, c, s2, c2 = sincos2d_(d, r.lat2)

568 c2 *= E.rocPrimeVertical(r.lat2) # aka rocTransverse

569 s *= (s2 * szi / c2) - (s * r.M21 / r.m12) # XXX _over?

570 s12, t = _s12(c / s) # XXX _over?

571 if fabs(t) < tol: # or fabs(c) < EPS

572 break

573 r = NearestOn4Tuple(r.lat2, r.lon2, s12, r.azi2,

574 iteration=i)

575 except Exception as x: # Fsum(NAN) Value-, ZeroDivisionError

576 raise IntersectionError(_no_(_intersection_), cause=x)

577 return r

578

579 def Position(self, s12, outmask=0): # PYCHOK no cover

580 '''I{Must be overloaded}, see function C{notOverloaded}.

581 '''

582 _MODS.named.notOverloaded(self, s12, outmask=outmask)

583

584 @Property_RO

585 def rhumb(self):

586 '''Get this rhumb line's rhumb (L{RhumbAux} or L{Rhumb}.

587 '''

588 return self._rhumb

589

590 def toStr(self, prec=6, sep=_COMMASPACE_, **unused): # PYCHOK signature

591 '''Return this C{RhumbLine} as string.

592

593 @kwarg prec: The C{float} precision, number of decimal digits (0..9).

594 Trailing zero decimals are stripped for B{C{prec}} values

595 of 1 and above, but kept for negative B{C{prec}} values.

596 @kwarg sep: Separator to join (C{str}).

597

598 @return: C{RhumbLine} (C{str}).

599 '''

600 d = dict(rhumb=self.rhumb, lat1=self.lat1, lon1=self.lon1,

601 azi12=self.azi12, exact=self.exact,

602 TMorder=self.TMorder, xTM=self.xTM)

603 return sep.join(pairs(itemsorted(d, asorted=False), prec=prec))

604

605 @property_RO

606 def TMorder(self):

607 '''Get this rhumb line's I{Transverse Mercator} order (C{int}, 4, 5, 6, 7 or 8).

608 '''

609 return self.rhumb.TMorder

610

611 @Property_RO

612 def xTM(self):

613 '''Get this rhumb line's I{Transverse Mercator} projection (L{ExactTransverseMercator}

614 if I{exact} and I{ellipsoidal}, otherwise L{KTransverseMercator} for C{TMorder}).

615 '''

616 E = self.ellipsoid

617 # ExactTransverseMercator doesn't handle spherical earth models

618 return _MODS.etm.ExactTransverseMercator(E) if self.exact and E.isEllipsoidal else \

619 _MODS.ktm.KTransverseMercator(E, TMorder=self.TMorder)

620

621 def _xTM3d(self, latlon0, z=INT0, V3d=Vector3d):

622 '''(INTERNAL) C{xTM.forward} this C{latlon1} to C{V3d} with B{C{latlon0}}

623 as current intersection estimate and central meridian.

624 '''

625 t = self.xTM.forward(self.lat1 - latlon0.lat, self.lon1, lon0=latlon0.lon)

626 return V3d(t.easting, t.northing, z)

627

628

629__all__ += _ALL_DOCS(RhumbBase, RhumbLineBase)

630

631

632 if __name__ == '__main__':

633

634 from pygeodesy import printf, RhumbAux as A, Rhumb as R

635

636 A = A(_EWGS84).Line(30, 0, 45)

637 R = R(_EWGS84).Line(30, 0, 45)

638

639 n = 1

640 for i in range(1, 10):

641 s = .5e6 + 1e6 / i

642 a = A.Position(s).lon2

643 r = R.Position(s).lon2

644 e = (fabs(a - r) * 100.0 / a) if a else 0

645 printf('Positions %s vs %s, diff %.2f%%', r, a, e, nl=n)

646 n = 0

647

648 for exact in (None, False, True, None):

649 for est in (None, 1e6):

650 a = A.nearestOn4(60, 0, exact=exact, est=est)

651 r = R.nearestOn4(60, 0, exact=exact, est=est)

652 printf('%s, iteration=%s, exact=%s, est=%s\n%s, iteration=%s',

653 a.toRepr(), a.iteration, exact, est, r.toRepr(), r.iteration, nl=1)

654

655# % python3 -m pygeodesy.rhumbBase

656

657# Positions 11.614558469016366 vs 11.61455846901637, diff 0.00%

658# Positions 7.589823028268422 vs 7.589823028268423, diff 0.00%

659# Positions 6.285260674163688 vs 6.285260674163687, diff 0.00%

660# Positions 5.639389953251457 vs 5.6393899532514595, diff 0.00%

661# Positions 5.253855274357075 vs 5.253855274357073, diff 0.00%

662# Positions 4.9976460429038 vs 4.9976460429038045, diff 0.00%

663# Positions 4.815033637404729 vs 4.81503363740473, diff 0.00%

664# Positions 4.678288217488354 vs 4.678288217488353, diff 0.00%

665# Positions 4.572056679062825 vs 4.572056679062826, diff 0.00%

666

667# NearestOn4Tuple(lat=45.0, lon=15.830286, distance=1977981.142985, normal=135.0), iteration=9, exact=None, est=None

668# NearestOn4Tuple(lat=45.0, lon=15.830286, distance=1977981.142985, normal=135.0), iteration=9

669

670# NearestOn4Tuple(lat=45.0, lon=15.830286, distance=1977981.142985, normal=135.0), iteration=9, exact=None, est=1000000.0

671# NearestOn4Tuple(lat=45.0, lon=15.830286, distance=1977981.142985, normal=135.0), iteration=9

672

673# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=5, exact=False, est=None

674# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=5

675

676# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=7, exact=False, est=1000000.0

677# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=7

678

679# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=5, exact=True, est=None

680# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=5

681

682# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=7, exact=True, est=1000000.0

683# NearestOn4Tuple(lat=49.634582, lon=25.767876, distance=3083112.636236, normal=135.0), iteration=7

684

685# **) MIT License

686#

687# Copyright (C) 2022-2023 -- mrJean1 at Gmail -- All Rights Reserved.

688#

689# Permission is hereby granted, free of charge, to any person obtaining a

690# copy of this software and associated documentation files (the "Software"),

691# to deal in the Software without restriction, including without limitation

692# the rights to use, copy, modify, merge, publish, distribute, sublicense,

693# and/or sell copies of the Software, and to permit persons to whom the

694# Software is furnished to do so, subject to the following conditions:

695#

696# The above copyright notice and this permission notice shall be included

697# in all copies or substantial portions of the Software.

698#

699# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

700# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

701# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

702# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

703# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

704# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

705# OTHER DEALINGS IN THE SOFTWARE.