1

2# -*- coding: utf-8 -*-

3

4 u'''Wrapper to invoke I{Karney}'s U{RhumbSolve

5<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>} utility

6 as an (exact) rhumb or rhumb line from I{either GeographicLib 2.0 or 2.2+}.

7

8@note: Set env variable C{PYGEODESY_RHUMBSOLVE} to the (fully qualified)

9 path of the C{RhumbSolve} executable.

10'''

11# from pygeodesy.basics import _xinstanceof # from .karney

12 from pygeodesy.constants import _0_0, _180_0, _N_180_0, _90_0 # PYCHOK used!

13 from pygeodesy.errors import RhumbError # PYCHOK used!

14 from pygeodesy.interns import NN, _a12_, _azi12_, _lat2_, _lon2_, _s12_, _S12_, _UNDER_

15 from pygeodesy.karney import Caps, GDict, _norm180, Rhumb8Tuple, _sincos2d, _xinstanceof

16 from pygeodesy.lazily import _ALL_DOCS, _ALL_LAZY, _ALL_MODS as _MODS, _getenv

17 from pygeodesy.namedTuples import Destination3Tuple, Distance3Tuple

18 from pygeodesy.props import deprecated_method, Property, Property_RO

19 from pygeodesy.solveBase import _SolveBase, _SolveLineBase

20 from pygeodesy.utily import _unrollon, _Wrap, wrap360

21

22__all__ = _ALL_LAZY.rhumbsolve

23__version__ = '23.08.22'

24

25_PYGEODESY_RHUMBSOLVE_ = 'PYGEODESY_RHUMBSOLVE' # PYCHOK used!

26

27

28 class _RhumbSolveBase(_SolveBase):

29 '''(INTERNAL) Base class for L{RhumbSolve} and L{RhumbLineSolve}.

30 '''

31 _Error = RhumbError

32 _Names_Direct = _lat2_, _lon2_, _S12_

33 _Names_Inverse = _azi12_, _s12_, _S12_

34 _Solve_name = 'RhumbSolve'

35 _Solve_path = _getenv(_PYGEODESY_RHUMBSOLVE_, _PYGEODESY_RHUMBSOLVE_)

36

37 @Property_RO

38 def _cmdBasic(self):

39 '''(INTERNAL) Get the basic C{RhumbSolve} cmd (C{tuple}).

40 '''

41 return (self.RhumbSolve,) + self._e_option \

42 + self._p_option \

43 + self._s_option

44

45 @Property

46 def RhumbSolve(self):

47 '''Get the U{RhumbSolve<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>}

48 executable (C{filename}).

49 '''

50 return self._Solve_path

51

52 @RhumbSolve.setter # PYCHOK setter!

53 def RhumbSolve(self, path):

54 '''Set the U{RhumbSolve<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>}

55 executable (C{filename}), the (fully qualified) path to the C{RhumbSolve} executable.

56

57 @raise RhumbError: Invalid B{C{path}}, B{C{path}} doesn't exist or isn't

58 the C{RhumbSolve} executable.

59 '''

60 self._setSolve(path)

61

62 @Property_RO

63 def _s_option(self): # == not -E for GeodSolve

64 return () if self.Exact else ('-s',)

65

66 def toStr(self, **prec_sep): # PYCHOK signature

67 '''Return this C{RhumbSolve} as string.

68

69 @kwarg prec_sep: Keyword argumens C{B{prec}=6} and C{B{sep}=', '}

70 for the C{float} C{prec}ision, number of decimal digits

71 (0..9) and the C{sep}arator string to join. Trailing

72 zero decimals are stripped for B{C{prec}} values of

73 1 and above, but kept for negative B{C{prec}} values.

74

75 @return: RhumbSolve items (C{str}).

76 '''

77 return self._toStr(RhumbSolve=self.RhumbSolve, **prec_sep)

78

79# @Property_RO

80# def _u_option(self):

81# return '-u' if self.unroll else ()

82

83

84 class RhumbSolve(_RhumbSolveBase):

85 '''Wrapper to invoke I{Karney}'s U{RhumbSolve<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>}

86 like a class, similar to L{pygeodesy.Rhumb} and L{pygeodesy.RhumbAux}.

87

88 @note: Use property C{RhumbSolve} or env variable C{PYGEODESY_RHUMBSOLVE} to specify the (fully

89 qualified) path to the C{RhumbSolve} executable.

90

91 @note: This C{rhumb} is intended I{for testing purposes only}, it invokes the C{RhumbSolve}

92 executable for I{every} method call.

93 '''

94# def Area(self, polyline=False, name=NN):

95# '''Set up a L{RhumbArea} to compute area and

96# perimeter of a polygon.

97#

98# @kwarg polyline: If C{True} perimeter only, otherwise

99# area and perimeter (C{bool}).

100# @kwarg name: Optional name (C{str}).

101#

102# @return: A L{RhumbArea} instance.

103#

104# @note: The B{C{debug}} setting is passed as C{verbose}

105# to the returned L{RhumbAreaExact} instance.

106# '''

107# rA = _MODS.rhumb*.RhumbArea(self, polyline=polyline,

108# name=name or self.name)

109# if self.verbose or self.debug: # PYCHOK no cover

110# rA.verbose = True

111# return rA

112

113# Polygon = Area # for C{geographiclib} compatibility

114

115 def _azimuth_reverse(self, azimuth):

116 '''(INTERNAL) Reverse final azimuth C{azimuth}.

117 '''

118 z = _norm180(float(azimuth))

119 if self.reverse2: # like .utils.atan2d

120 z += _180_0 if z < 0 else _N_180_0

121 return z

122

123 def _Direct(self, ll1, azi12, s12, **outmask):

124 '''(INTERNAL) Short-cut version, see .latlonBase.

125 '''

126 return self.Direct(ll1.lat, ll1.lon, azi12, s12, **outmask)

127

128 def Direct3(self, lat1, lon1, azi1, s12): # PYCHOK outmask

129 '''Return the destination lat, lon and reverse azimuth

130 (final bearing) in C{degrees}.

131

132 @return: L{Destination3Tuple}C{(lat, lon, final)}.

133 '''

134 r = self._GDictDirect(lat1, lon1, azi1, False, s12, floats=False)

135 z = self._azimuth_reverse(r.azi12)

136 return Destination3Tuple(float(r.lat2), float(r.lon2), wrap360(z),

137 iteration=r._iteration)

138

139 def _DirectLine(self, ll1, azi12, **name_caps):

140 '''(INTERNAL) Short-cut version, see .latlonBase.

141 '''

142 return self.DirectLine(ll1.lat, ll1.lon, azi12, **name_caps)

143

144 def DirectLine(self, lat1, lon1, azi1, caps=Caps.STANDARD, name=NN):

145 '''Set up a L{RhumbLineSolve} in terms of the I{direct} rhumb

146 problem to compute several points on a single rhumb line.

147

148 @arg lat1: Latitude of the first point (C{degrees}).

149 @arg lon1: Longitude of the first point (C{degrees}).

150 @arg azi1: Azimuth at the first point (compass C{degrees}).

151 @kwarg caps: Bit-or'ed combination of L{Caps} values specifying

152 the capabilities the L{RhumbLineSolve} instance

153 should possess, always C{Caps.ALL}.

154

155 @return: A L{RhumbLineSolve} instance.

156

157 @note: If the point is at a pole, the azimuth is defined by keeping

158 B{C{lon1}} fixed, writing C{B{lat1} = ±(90 − ε)}, and taking

159 the limit C{ε → 0+}.

160

161 @see: C++ U{RhumbExact.Line

162 <https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1RhumbExact.html>}

163 and Python U{Rhumb.Line<https://GeographicLib.SourceForge.io/Python/doc/code.html>}.

164 '''

165 return RhumbLineSolve(self, lat1, lon1, azi1, caps=caps, name=name or self.name)

166

167 def _GDictDirect(self, lat, lon, azi1, arcmode, s12_a12, *unused, **floats): # PYCHOK signature

168 '''(INTERNAL) Get C{_GenDirect}-like result as an 8-item C{GDict}.

169 '''

170 d = _RhumbSolveBase._GDictDirect(self, lat, lon, azi1, arcmode, s12_a12, **floats)

171 r = GDict(lat1=lat, lon1=lon, azi12=azi1, s12=s12_a12) # a12=s12_a12 / self.ellipsoid._L_90

172 r.update(d)

173 return r

174

175 def _GDictInverse(self, lat1, lon1, lat2, lon2, *unused, **floats): # PYCHOK signature

176 '''(INTERNAL) Get C{_GenInverse}-like result as an 8-item C{GDict}, but

177 I{without} C{_SALPs_CALPs_}.

178 '''

179 i = _RhumbSolveBase._GDictInverse(self, lat1, lon1, lat2, lon2, **floats)

180 a = float(i.s12) / self.ellipsoid._L_90 # for .Inverse1

181 r = GDict(lat1=lat1, lon1=lon1, lat2=lat2, lon2=lon2, a12=a)

182 r.update(i)

183 return r

184

185 def _Inverse(self, ll1, ll2, wrap, **unused):

186 '''(INTERNAL) Short-cut version, see .latlonBase.

187 '''

188 if wrap:

189 ll2 = _unrollon(ll1, _Wrap.point(ll2))

190 return self._GDictInverse(ll1.lat, ll1.lon, ll2.lat, ll2.lon)

191

192 def Inverse3(self, lat1, lon1, lat2, lon2): # PYCHOK outmask

193 '''Return the distance in C{meter} and the forward and

194 reverse azimuths (initial and final bearing) in C{degrees}.

195

196 @return: L{Distance3Tuple}C{(distance, initial, final)}.

197 '''

198 r = self._GDictInverse(lat1, lon1, lat2, lon2, floats=False)

199 z = self._azimuth_reverse(r.azi12)

200 return Distance3Tuple(float(r.s12), wrap360(r.azi12), wrap360(z),

201 iteration=r._iteration)

202

203 def _InverseLine(self, ll1, ll2, wrap, **name_caps):

204 '''(INTERNAL) Short-cut version, see .latlonBase.

205 '''

206 if wrap:

207 ll2 = _unrollon(ll1, _Wrap.point(ll2))

208 return self.InverseLine(ll1.lat, ll1.lon, ll2.lat, ll2.lon, **name_caps)

209

210 def InverseLine(self, lat1, lon1, lat2, lon2, caps=Caps.STANDARD, name=NN):

211 '''Define a L{RhumbLineSolve} in terms of the I{inverse}

212 rhumb problem.

213

214 @arg lat1: Latitude of the first point (C{degrees90}).

215 @arg lon1: Longitude of the first point (C{degrees180}).

216 @arg lat2: Latitude of the second point (C{degrees90}).

217 @arg lon2: Longitude of the second point (C{degrees180}).

218 @kwarg caps: Optional C{caps}, see L{RhumbLine} C{B{caps}}.

219

220 @return: A L{RhumbLineSolve} instance and invoke its method

221 L{RhumbLine.Position} to compute each point.

222

223 @note: Updates to this rhumb are reflected in the returned

224 rhumb line.

225 '''

226 r = self.Inverse(lat1, lon1, lat2, lon2) # outmask=Caps.AZIMUTH

227 return RhumbLineSolve(self, lat1, lon1, r.azi12, caps=caps,

228 name=name or self.name)

229

230 Line = DirectLine

231

232

233 class RhumbLineSolve(_RhumbSolveBase, _SolveLineBase):

234 '''Wrapper to invoke I{Karney}'s U{RhumbSolve<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>},

235 the C{Exact} version of class L{pygeodesy.RhumbLine}.

236

237 @note: Use property C{RhumbSolve} or env variable C{PYGEODESY_RHUMBSOLVE} to specify the (fully

238 qualified) path to the C{RhumbSolve} executable.

239

240 @note: This C{rhumb line} is intended I{for testing purposes only}, it invokes the C{RhumbSolve}

241 executable for I{every} method call.

242 '''

243 def __init__(self, rhumb, lat1, lon1, azi12, caps=Caps.STANDARD, name=NN):

244 '''New L{RhumbLineSolve} instance, allowing points to be found along

245 a rhumb starting at C{(B{lat1}, B{lon1})} with azimuth B{C{azi12}}.

246

247 @arg rhumb: The rhumb to use (L{RhumbSolve}).

248 @arg lat1: Latitude of the first point (C{degrees90}).

249 @arg lon1: Longitude of the first point (C{degrees180}).

250 @arg azi12: Azimuth of the rhumb line (compass C{degrees180}).

251 @kwarg caps: Bit-or'ed combination of L{Caps} values specifying

252 the capabilities the L{RhumbLineSolve} instance should

253 possess, always C{Caps.ALL}. Use C{Caps.LINE_OFF}

254 if updates to the B{C{rhumb}} should I{not} be

255 reflected in this L{RhumbLineSolve} instance.

256

257 @kwarg name: Optional name (C{str}).

258

259 @raise RhumbError: Invalid path for C{RhumbSolve} executable or

260 isn't the C{RhumbSolve} executable, see

261 property C{B{rhumb}.RhumbSolve}.

262

263 @raise TypeError: Invalid B{C{rhumb}}.

264 '''

265 _xinstanceof(RhumbSolve, rhumb=rhumb)

266 if (caps & Caps.LINE_OFF): # copy to avoid updates

267 rhumb = rhumb.copy(deep=False, name=NN(_UNDER_, rhumb.name))

268 _SolveLineBase.__init__(self, rhumb, lat1, lon1, caps, name, azi12=azi12)

269 try:

270 self.RhumbSolve = rhumb.RhumbSolve # rhumb or copy of rhumb

271 except RhumbError:

272 pass

273

274# def ArcPosition(self, a12, *unused):

275# '''Find the position on the line given B{C{a12}}.

276#

277# @arg a12: Spherical arc length from the first point to the

278# second point (C{degrees}).

279#

280# @return: A C{dict} with 8 items C{lat1, lon1, lat2, lon2,

281# azi12, a12, s12, S12}.

282# '''

283# s = a12 * self.ellipsoid._L_90

284# a = self._GDictInvoke(self._cmdArc, True, self._Names_Direct, s)

285# r = GDict(a12=a12, s12=s, **self._lla1)

286# r.updated(a)

287# return r

288

289 @Property_RO

290 def azi12(self):

291 '''Get this rhumb line's azimuth (compass C{degrees}).

292 '''

293 return self._lla1.azi12

294

295 azi1 = azi12 # like GeodesicLineSolve

296

297 @Property_RO

298 def azi12_sincos2(self): # PYCHOK no cover

299 '''Get the sine and cosine of this rhumb line's azimuth (2-tuple C{(sin, cos)}).

300 '''

301 return _sincos2d(self.azi12)

302

303 azi1_sincos2 = azi12_sincos2

304

305# @Property_RO

306# def _cmdArc(self):

307# '''(INTERNAL) Get the C{RhumbSolve} I{-a -L} cmd (C{tuple}).

308# '''

309# return self._cmdDistance + ('-a',)

310

311 def Position(self, s12, **unused):

312 '''Find the position on the line given B{C{s12}}.

313

314 @arg s12: Distance from the first point to the second (C{meter}).

315

316 @return: A L{GDict} with 7 items C{lat1, lon1, lat2, lon2,

317 azi12, s12, S12}.

318 '''

319 d = self._GDictInvoke(self._cmdDistance, True, self._Names_Direct, s12)

320 r = GDict(s12=s12, **self._lla1) # a12=s12 / self.ellipsoid._L_90

321 r.update(d)

322 return r

323

324 def toStr(self, **prec_sep): # PYCHOK signature

325 '''Return this C{RhumbLineSolve} as string.

326

327 @kwarg prec_sep: Keyword argumens C{B{prec}=6} and C{B{sep}=', '}

328 for the C{float} C{prec}ision, number of decimal digits

329 (0..9) and the C{sep}arator string to join. Trailing

330 zero decimals are stripped for B{C{prec}} values of

331 1 and above, but kept for negative B{C{prec}} values.

332

333 @return: RhumbLineSolve items (C{str}).

334 '''

335 return _SolveLineBase._toStr(self, azi12=self.azi12, rhumb=self._solve,

336 RhumbSolve=self.RhumbSolve, **prec_sep)

337

338

339 class RhumbSolve7Tuple(Rhumb8Tuple):

340 '''7-Tuple C{(lat1, lon1, lat2, lon2, azi12, s12, S12)} with lat- C{lat1},

341 C{lat2} and longitudes C{lon1}, C{lon2} of both points, the azimuth of

342 the rhumb line C{azi12}, the distance C{s12} and the area C{S12} under

343 the rhumb line between both points.

344 '''

345 assert Rhumb8Tuple._Names_.index(_a12_) == 7

346 _Names_ = Rhumb8Tuple._Names_[:7] # drop a12

347 _Units_ = Rhumb8Tuple._Units_[:7]

348

349 @deprecated_method

350 def _to7Tuple(self): # PYCHOK no cover

351 '''DEPRECATED, I{don't use!}

352 '''

353 return _MODS.deprecated.Rhumb7Tuple(self[:7])

354

355

356__all__ += _ALL_DOCS(_RhumbSolveBase)

357

358 if __name__ == '__main__':

359

360 from pygeodesy.lazily import printf

361 from sys import argv

362

363 def rhumb_intercept(rS, lat1, lon1, lat2, lon2, azi2, s23):

364 # using RhumbSolve and GeodesicExact for I{Karney}'s C++ U{rhumb-intercept.cpp

365 # <https://SourceForge.net/p/geographiclib/discussion/1026620/thread/2ddc295e/>

366 from pygeodesy.constants import EPS4 as _TOL

367 from pygeodesy.karney import _diff182

368

369 E = rS.ellipsoid

370 gX = E.geodesicx # == GeodesicExact(E)

371 m = gX.STANDARD | gX.REDUCEDLENGTH | gX.GEODESICSCALE

372

373 rlS = rS.Line(lat2, lon2, azi2)

374 sa, _ = rlS.azi12_sincos2 # aka _salp, _calp

375 for i in range(1, 16):

376 p = rlS.Position(s23) # outmask=gX.LATITUDE_LONGITUDE

377 r = gX.Inverse(lat1, lon1, p.lat2, p.lon2, outmask=m)

378 d, _ = _diff182(azi2, r.azi2, K_2_0=True)

379 s, c = _sincos2d(d)

380 printf('%2d %.3f %.8f, %.8f, %.8e',

381 i, s23, r.lat2, r.lon2, c)

382 s2, c2 = _sincos2d(r.lat2)

383 c2 *= E.rocTransverse(r.lat2)

384 if c2 and r.m12:

385 s *= (s2 * sa) / c2 - s * r.M21 / r.m12

386 t = (c / s) if s else _0_0

387 if abs(t) < _TOL:

388 break

389 s23 += t

390 else:

391 break

392

393 rS = RhumbSolve(name='Test')

394 rS.verbose = '--verbose' in argv # or '-v' in argv

395

396 if rS.RhumbSolve in (_PYGEODESY_RHUMBSOLVE_, None): # not set

397 rS.RhumbSolve = '/opt/local/bin/RhumbSolve' # '/opt/local/Cellar/geographiclib/2.2/bin/RhumbSolve' # HomeBrew

398 printf('version: %s', rS.version)

399

400 if len(argv) > 6: # 60 0 30 0 45 1e6

401 t = (14, 's23'), (7, 'lat3'), (11, 'lon3'), (13, 'cos()')

402 printf(' '.join('%*s' % _ for _ in t))

403 rhumb_intercept(rS, *map(float, argv[-6:]))

404 exit()

405

406 r = rS.Direct(40.6, -73.8, 51, 5.5e6)

407 printf('Direct: %r', r, nl=1)

408 printf('Direct3: %r', rS.Direct3(40.6, -73.8, 51, 5.5e6))

409

410 printf('Inverse: %r', rS.Inverse( 40.6, -73.8, 51.6, -0.5), nl=1)

411 printf('Inverse1: %r', rS.Inverse1(40.6, -73.8, 51.6, -0.5))

412 printf('Inverse3: %r', rS.Inverse3(40.6, -73.8, 51.6, -0.5))

413

414 printf('Inverse: %r', rS.Inverse( 40.6, -73.8, 35.8, 140.3), nl=1)

415 printf('Inverse1: %r', rS.Inverse1(40.6, -73.8, 35.8, 140.3))

416 printf('Inverse3: %r', rS.Inverse3(40.6, -73.8, 35.8, 140.3))

417

418 rlS = RhumbLineSolve(rS, 40.6, -73.8, 51, name='LineTest')

419 p = rlS.Position(5.5e6)

420 printf('Position: %s %r', p == r, p, nl=1)

421# p = rlS.ArcPosition(49.475527)

422# printf('ArcPosition: %s %r', p == r, p)

423

424# % python3 -m pygeodesy.rhumbsolve

425

426# version: /opt/local/bin/RhumbSolve: GeographicLib version 1.51

427#

428# Direct: GDict(S12=44095641862956.148438, azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0)

429# Direct3: Destination3Tuple(lat=71.6889, lon=0.25552, final=51.0)

430#

431# Inverse: GDict(S12=37395209100030.367188, a12=51.929543, azi12=77.76839, lat1=40.6, lat2=51.6, lon1=-73.8, lon2=-0.5, s12=5771083.383328)

432# Inverse1: 51.92954250756195

433# Inverse3: Distance3Tuple(distance=5771083.383328, initial=77.76839, final=77.76839)

434#

435# Inverse: GDict(S12=-63760642939072.492188, a12=115.02062, azi12=-92.388888, lat1=40.6, lat2=35.8, lon1=-73.8, lon2=140.3, s12=12782581.067684)

436# Inverse1: 115.02061966879258

437# Inverse3: Distance3Tuple(distance=12782581.067684, initial=267.611112, final=267.611112)

438#

439# Position: True GDict(S12=44095641862956.148438, azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0)

440

441

442# % python3 -m pygeodesy.rhumbsolve --verbose

443

444# RhumbSolve 'Test' 1: /opt/local/bin/RhumbSolve --version (invoke)

445# RhumbSolve 'Test' 1: /opt/local/bin/RhumbSolve: GeographicLib version 1.51 (0)

446# version: /opt/local/bin/RhumbSolve: GeographicLib version 1.51

447# RhumbSolve 'Test' 2: /opt/local/bin/RhumbSolve -p 10 \ 40.600000000000001 -73.799999999999997 51.0 5500000.0 (Direct)

448# RhumbSolve 'Test' 2: lat2=71.688899882813047, lon2=0.255519824423445, S12=44095641862956.148 (0)

449

450# Direct: GDict(S12=44095641862956.148438, azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0)

451# RhumbSolve 'Test' 3: /opt/local/bin/RhumbSolve -p 10 \ 40.600000000000001 -73.799999999999997 51.0 5500000.0 (Direct3)

452# RhumbSolve 'Test' 3: lat2=71.688899882813047, lon2=0.255519824423445, S12=44095641862956.148 (0)

453# Direct3: Destination3Tuple(lat=71.6889, lon=0.25552, final=51.0)

454# RhumbSolve 'Test' 4: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse)

455# RhumbSolve 'Test' 4: azi12=77.768389710255661, s12=5771083.3833280317, S12=37395209100030.367 (0)

456

457# Inverse: GDict(S12=37395209100030.367188, a12=51.929543, azi12=77.76839, lat1=40.6, lat2=51.6, lon1=-73.8, lon2=-0.5, s12=5771083.383328)

458# RhumbSolve 'Test' 5: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse1)

459# RhumbSolve 'Test' 5: azi12=77.768389710255661, s12=5771083.3833280317, S12=37395209100030.367 (0)

460# Inverse1: 51.92954250756195

461# RhumbSolve 'Test' 6: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse3)

462# RhumbSolve 'Test' 6: azi12=77.768389710255661, s12=5771083.3833280317, S12=37395209100030.367 (0)

463# Inverse3: Distance3Tuple(distance=5771083.383328, initial=77.76839, final=77.76839)

464# RhumbSolve 'Test' 7: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 35.799999999999997 140.300000000000011 (Inverse)

465# RhumbSolve 'Test' 7: azi12=-92.388887981699639, s12=12782581.0676841792, S12=-63760642939072.492 (0)

466

467# Inverse: GDict(S12=-63760642939072.492188, a12=115.02062, azi12=-92.388888, lat1=40.6, lat2=35.8, lon1=-73.8, lon2=140.3, s12=12782581.067684)

468# RhumbSolve 'Test' 8: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 35.799999999999997 140.300000000000011 (Inverse1)

469# RhumbSolve 'Test' 8: azi12=-92.388887981699639, s12=12782581.0676841792, S12=-63760642939072.492 (0)

470# Inverse1: 115.02061966879258

471# RhumbSolve 'Test' 9: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 35.799999999999997 140.300000000000011 (Inverse3)

472# RhumbSolve 'Test' 9: azi12=-92.388887981699639, s12=12782581.0676841792, S12=-63760642939072.492 (0)

473# Inverse3: Distance3Tuple(distance=12782581.067684, initial=267.611112, final=267.611112)

474

475# Position: True GDict(S12=44095641862956.148438, azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0)

476

477

478# % python3 -m pygeodesy.rhumbsolve

479

480# version: /opt/local/bin/RhumbSolve: GeographicLib version 2.2

481

482# Direct: GDict(azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0, S12=44095641862956.109375)

483# Direct3: Destination3Tuple(lat=71.6889, lon=0.25552, final=51.0)

484

485# Inverse: GDict(a12=51.929543, azi12=77.76839, lat1=40.6, lat2=51.6, lon1=-73.8, lon2=-0.5, s12=5771083.383328, S12=37395209100030.390625)

486# Inverse1: 51.92954250756191

487# Inverse3: Distance3Tuple(distance=5771083.383328, initial=77.76839, final=77.76839)

488

489# Inverse: GDict(a12=115.02062, azi12=-92.388888, lat1=40.6, lat2=35.8, lon1=-73.8, lon2=140.3, s12=12782581.067684, S12=-63760642939072.5)

490# Inverse1: 115.02061966879249

491# Inverse3: Distance3Tuple(distance=12782581.067684, initial=267.611112, final=267.611112)

492

493# Position: True GDict(azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0, S12=44095641862956.109375)

494

495

496# % python3 -m pygeodesy.rhumbsolve --verbose

497

498# RhumbSolve 'Test' 1: /opt/local/bin/RhumbSolve --version (invoke)

499# RhumbSolve 'Test' 1: /opt/local/bin/RhumbSolve: GeographicLib version 2.2 (0)

500# version: /opt/local/bin/RhumbSolve: GeographicLib version 2.2

501# RhumbSolve 'Test' 2: /opt/local/bin/RhumbSolve -p 10 \ 40.600000000000001 -73.799999999999997 51.0 5500000.0 (Direct)

502# RhumbSolve 'Test' 2: lat2=71.688899882813018, lon2=0.255519824423402, S12=44095641862956.109 (0)

503

504# Direct: GDict(azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0, S12=44095641862956.109375)

505# RhumbSolve 'Test' 3: /opt/local/bin/RhumbSolve -p 10 \ 40.600000000000001 -73.799999999999997 51.0 5500000.0 (Direct3)

506# RhumbSolve 'Test' 3: lat2=71.688899882813018, lon2=0.255519824423402, S12=44095641862956.109 (0)

507# Direct3: Destination3Tuple(lat=71.6889, lon=0.25552, final=51.0)

508# RhumbSolve 'Test' 4: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse)

509# RhumbSolve 'Test' 4: azi12=77.768389710255661, s12=5771083.383328028, S12=37395209100030.391 (0)

510

511# Inverse: GDict(a12=51.929543, azi12=77.76839, lat1=40.6, lat2=51.6, lon1=-73.8, lon2=-0.5, s12=5771083.383328, S12=37395209100030.390625)

512# RhumbSolve 'Test' 5: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse1)

513# RhumbSolve 'Test' 5: azi12=77.768389710255661, s12=5771083.383328028, S12=37395209100030.391 (0)

514# Inverse1: 51.92954250756191

515# RhumbSolve 'Test' 6: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 51.600000000000001 -0.5 (Inverse3)

516# RhumbSolve 'Test' 6: azi12=77.768389710255661, s12=5771083.383328028, S12=37395209100030.391 (0)

517# Inverse3: Distance3Tuple(distance=5771083.383328, initial=77.76839, final=77.76839)

518# RhumbSolve 'Test' 7: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 35.799999999999997 140.300000000000011 (Inverse)

519# RhumbSolve 'Test' 7: azi12=-92.388887981699654, s12=12782581.0676841699, S12=-63760642939072.5 (0)

520

521# Inverse: GDict(a12=115.02062, azi12=-92.388888, lat1=40.6, lat2=35.8, lon1=-73.8, lon2=140.3, s12=12782581.067684, S12=-63760642939072.5)

522# RhumbSolve 'Test' 8: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 35.799999999999997 140.300000000000011 (Inverse1)

523# RhumbSolve 'Test' 8: azi12=-92.388887981699654, s12=12782581.0676841699, S12=-63760642939072.5 (0)

524# Inverse1: 115.02061966879249

525# RhumbSolve 'Test' 9: /opt/local/bin/RhumbSolve -p 10 -i \ 40.600000000000001 -73.799999999999997 35.799999999999997 140.300000000000011 (Inverse3)

526# RhumbSolve 'Test' 9: azi12=-92.388887981699654, s12=12782581.0676841699, S12=-63760642939072.5 (0)

527# Inverse3: Distance3Tuple(distance=12782581.067684, initial=267.611112, final=267.611112)

528

529# Position: True GDict(azi12=51, lat1=40.6, lat2=71.6889, lon1=-73.8, lon2=0.25552, s12=5500000.0, S12=44095641862956.109375)

530

531

532# % python3 -m pygeodesy.rhumbsolve 60 0 30 0 45 1e6

533

534# version: /opt/local/bin/RhumbSolve: GeographicLib version 2.2

535# s23 lat3 lon3 cos()

536# 1 1000000.000 36.37559999, 7.58982303, -5.83098638e-01

537# 2 4532573.097 58.84251798, 41.57078946, 4.05349594e-01

538# 3 2233216.895 44.22871762, 17.86660260, -2.91432608e-01

539# 4 3168401.173 50.17678842, 26.60741388, 3.00555188e-02

540# 5 3082690.347 49.63189746, 25.76374255, -1.49446251e-04

541# 6 3083112.629 49.63458216, 25.76787599, -2.59865190e-09

542# 7 3083112.636 49.63458221, 25.76787606, 4.96052409e-16

543# 8 3083112.636 49.63458221, 25.76787606, -4.96052409e-16

544# 9 3083112.636 49.63458221, 25.76787606, 4.96052409e-16

545# 10 3083112.636 49.63458221, 25.76787606, -4.96052409e-16

546# 11 3083112.636 49.63458221, 25.76787606, 4.96052409e-16

547# 12 3083112.636 49.63458221, 25.76787606, -4.96052409e-16

548# 13 3083112.636 49.63458221, 25.76787606, 4.96052409e-16

549# 14 3083112.636 49.63458221, 25.76787606, -4.96052409e-16

550# 15 3083112.636 49.63458221, 25.76787606, 4.96052409e-16

551

552# **) MIT License

553#

554# Copyright (C) 2022-2023 -- mrJean1 at Gmail -- All Rights Reserved.

555#

556# Permission is hereby granted, free of charge, to any person obtaining a

557# copy of this software and associated documentation files (the "Software"),

558# to deal in the Software without restriction, including without limitation

559# the rights to use, copy, modify, merge, publish, distribute, sublicense,

560# and/or sell copies of the Software, and to permit persons to whom the

561# Software is furnished to do so, subject to the following conditions:

562#

563# The above copyright notice and this permission notice shall be included

564# in all copies or substantial portions of the Software.

565#

566# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

567# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

568# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

569# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

570# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

571# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

572# OTHER DEALINGS IN THE SOFTWARE.