Package pygeodesy :: Module cartesianBase |
[frames] | no frames]

# Module cartesianBase

(INTERNAL) Private `CartesianBase` class for elliposiodal, spherical and N-/vectorial `Cartesian`s and public functions rtp2xyz, rtp2xyz_, xyz2rtp and xyz2rtp_.

After (C) Chris Veness 2011-2024 published under the same MIT Licence**, see https://www.Movable-Type.co.UK/scripts/latlong.html, https://www.Movable-Type.co.UK/scripts/latlong-vectors.html and https://www.Movable-Type.co.UK/scripts/geodesy/docs/latlon-ellipsoidal.js.html.

Version: 24.12.04

Classes
| CartesianBase (INTERNAL) Base class for ellipsoidal and spherical `Cartesian`.
| RadiusThetaPhi3Tuple 3-Tuple `(r, theta, phi)` with radial distance `r` in `meter`, inclination `theta` (with respect to the positive z-axis) and azimuthal angle `phi` in Degrees or Radians representing a spherical, polar position.

Functions
rtp2xyz(r_rtp, theta=0, phi=0, **name_Cartesian_and_kwds) Convert spherical, polar `(r, theta, phi)` to cartesian `(x, y, z)` coordinates. |
rtp2xyz_(r_rtp, theta=0, phi=0, **name_Cartesian_and_kwds) Convert spherical, polar `(r, theta, phi)` to cartesian `(x, y, z)` coordinates. |
xyz2rtp(x_xyz, y=0, z=0, **name) Convert cartesian `(x, y, z)` to spherical, polar `(r, theta, phi)` coordinates. |
xyz2rtp_(x_xyz, y=0, z=0, **name) Convert cartesian `(x, y, z)` to spherical, polar `(r, theta, phi)` coordinates. |

Variables
| __all__ = `_ALL_LAZY.cartesianBase`

Function Details

### rtp2xyz (r_rtp, theta=0, phi=0, **name_Cartesian_and_kwds) |
Convert spherical, polar `(r, theta, phi)` to cartesian `(x, y, z)` coordinates. Arguments: `theta` - Inclination `theta` (`degrees` with respect to the positive z-axis), required if `r_rtp` is `scalar`, ignored otherwise. `phi` - Azimuthal angle `phi` (`degrees`), like `theta`. See Also: Function rtp2xyz_ for further details.

### rtp2xyz_ (r_rtp, theta=0, phi=0, **name_Cartesian_and_kwds) |
Convert spherical, polar `(r, theta, phi)` to cartesian `(x, y, z)` coordinates. Arguments: `r_rtp` - Radial distance (`scalar`, conventially `meter`) or a previous RadiusThetaPhi3Tuple instance. `theta` - Inclination `theta` (`radians` with respect to the positive z-axis), required if `r_rtp` is `scalar`, ignored otherwise. `phi` - Azimuthal angle `phi` (`radians`), like `theta`. `name_Cartesian_and_kwds` - Optional `name=NN` (`str`), `Cartesian=None` class to return the coordinates and optionally, additional `Cartesian` keyword arguments. Returns: A `Cartesian(x, y, z)` instance or if no `Cartesian` keyword argument is given a Vector3Tuple`(x, y, z)`, with `x`, `y` and `z` in the same units as radius `r`, `meter` conventionally. Raises: `TypeError` - Invalid `r_rtp`, `theta`, `phi` or `name_Cartesian_and_kwds` item. See Also: Physics convention (ISO 80000-2:2019), class RadiusThetaPhi3Tuple and functions rtp2xyz and xyz2rtp.

### xyz2rtp (x_xyz, y=0, z=0, **name) |
Convert cartesian `(x, y, z)` to spherical, polar `(r, theta, phi)` coordinates. Returns: RadiusThetaPhi3Tuple`(r, theta, phi)` with `theta` and `phi`, both in Degrees. See Also: Function xyz2rtp_ for further details.

### xyz2rtp_ (x_xyz, y=0, z=0, **name) |
Convert cartesian `(x, y, z)` to spherical, polar `(r, theta, phi)` coordinates. Arguments: `x_xyz` - X component (`scalar`) or a cartesian (`Cartesian`, Ecef9Tuple, `Nvector`, Vector3d, Vector3Tuple, Vector4Tuple or a `tuple` or `list` of 3+ `scalar` items) if no `y_z` specified. `y` - Y component (`scalar`), required if `x_xyz` is `scalar`, ignored otherwise. `z` - Z component (`scalar`), like `y`. `name` - Optional `name=NN` (`str`). Returns: RadiusThetaPhi3Tuple`(r, theta, phi)` with radial distance `r` (`meter`, same units as `x`, `y` and `z`), inclination `theta` (with respect to the positive z-axis) and azimuthal angle `phi`, both in Radians. See Also: Physics convention (ISO 80000-2:2019), class RadiusThetaPhi3Tuple and function xyz2rtp.