1

2# -*- coding: utf-8 -*-

3

4 u'''(INTERNAL) Private elliposiodal and spherical C{Nvector} base classes

5 L{LatLonNvectorBase} and L{NvectorBase} and function L{sumOf}.

6

7 Pure Python implementation of C{n-vector}-based geodesy tools for ellipsoidal

8 earth models, transcoded from JavaScript originals by I{(C) Chris Veness 2005-2016}

9 and published under the same MIT Licence**, see U{Vector-based geodesy

10<https://www.Movable-Type.co.UK/scripts/latlong-vectors.html>}.

11'''

12

13# from pygeodesy.basics import map1 # from .namedTuples

14 from pygeodesy.constants import EPS, EPS1, EPS_2, R_M, _2_0, _N_2_0

15# from pygeodesy.datums import _spherical_datum # from .formy

16 from pygeodesy.errors import IntersectionError, _ValueError, VectorError, \

17 _xkwds, _xkwds_pop2

18 from pygeodesy.fmath import fdot, fidw, hypot_ # PYCHOK fdot shared

19 from pygeodesy.fsums import Fsum, fsumf_

20 from pygeodesy.formy import _isequalTo, n_xyz2latlon, n_xyz2philam, \

21 _spherical_datum

22# from pygeodesy.internals import _under # from .named

23 from pygeodesy.interns import NN, _1_, _2_, _3_, _bearing_, _coincident_, \

24 _COMMASPACE_, _distance_, _h_, _insufficient_, \

25 _intersection_, _no_, _NorthPole_, _point_, \

26 _pole_, _SPACE_, _SouthPole_

27 from pygeodesy.latlonBase import LatLonBase, _ALL_DOCS, _ALL_LAZY, _MODS

28# from pygeodesy.lazily import _ALL_DOCS, _ALL_LAZY, _ALL_MODS as _MODS # from .latlonBase

29 from pygeodesy.named import _xother3, _under

30 from pygeodesy.namedTuples import Trilaterate5Tuple, Vector3Tuple, \

31 Vector4Tuple, map1

32 from pygeodesy.props import deprecated_method, Property_RO, property_doc_, \

33 property_RO, _update_all

34 from pygeodesy.streprs import Fmt, hstr, unstr, _xattrs

35 from pygeodesy.units import Bearing, Height, Radius_, Scalar

36 from pygeodesy.utily import sincos2d, _unrollon, _unrollon3

37 from pygeodesy.vector3d import Vector3d, _xyzhdn3

38

39 from math import fabs, sqrt

40

41__all__ = _ALL_LAZY.nvectorBase

42__version__ = '24.05.31'

43

44

45 class NvectorBase(Vector3d): # XXX kept private

46 '''Base class for ellipsoidal and spherical C{Nvector}s.

47 '''

48 _datum = None # L{Datum}, overriden

49 _h = Height(h=0) # height (C{meter})

50 _H = NN # height prefix (C{str}), '↑' in JS version

51

52 def __init__(self, x_xyz, y=None, z=None, h=0, ll=None, datum=None, **name):

53 '''New n-vector normal to the earth's surface.

54

55 @arg x_xyz: X component of vector (C{scalar}) or (3-D) vector

56 (C{Nvector}, L{Vector3d}, L{Vector3Tuple} or

57 L{Vector4Tuple}).

58 @kwarg y: Y component of vector (C{scalar}), ignored if B{C{x_xyz}}

59 is not C{scalar}, otherwise same units as B{C{x_xyz}}.

60 @kwarg z: Z component of vector (C{scalar}), ignored if B{C{x_xyz}}

61 is not C{scalar}, otherwise same units as B{C{x_xyz}}.

62 @kwarg h: Optional height above surface (C{meter}).

63 @kwarg ll: Optional, original latlon (C{LatLon}).

64 @kwarg datum: Optional, I{pass-thru} datum (L{Datum}).

65 @kwarg name: Optional C{B{name}=NN} (C{str}).

66

67 @raise TypeError: Non-scalar B{C{x}}, B{C{y}} or B{C{z}}

68 coordinate or B{C{x}} not an C{Nvector},

69 L{Vector3Tuple} or L{Vector4Tuple} or

70 invalid B{C{datum}}.

71 '''

72 h, d, n = _xyzhdn3(x_xyz, h, datum, ll, **name)

73 Vector3d.__init__(self, x_xyz, y=y, z=z, ll=ll, name=n)

74 if h:

75 self.h = h

76 if d is not None:

77 self._datum = _spherical_datum(d, name=self.name) # pass-thru

78

79 @Property_RO

80 def datum(self):

81 '''Get the I{pass-thru} datum (C{Datum}) or C{None}.

82 '''

83 return self._datum

84

85 @property_RO

86 def Ecef(self):

87 '''Get the ECEF I{class} (L{EcefKarney}), I{once}.

88 '''

89 NvectorBase.Ecef = E = _MODS.ecef.EcefKarney # overwrite property_RO

90 return E

91

92 @property_RO

93 def ellipsoidalNvector(self):

94 '''Get the C{Nvector type} iff ellipsoidal, overloaded in L{pygeodesy.ellipsoidalNvector.Nvector}.

95 '''

96 return False

97

98 @property_doc_(''' the height above surface (C{meter}).''')

99 def h(self):

100 '''Get the height above surface (C{meter}).

101 '''

102 return self._h

103

104 @h.setter # PYCHOK setter!

105 def h(self, h):

106 '''Set the height above surface (C{meter}).

107

108 @raise TypeError: If B{C{h}} invalid.

109

110 @raise VectorError: If B{C{h}} invalid.

111 '''

112 h = Height(h=h, Error=VectorError)

113 if self._h != h:

114 _update_all(self)

115 self._h = h

116

117 @property_doc_(''' the height prefix (C{str}).''')

118 def H(self):

119 '''Get the height prefix (C{str}).

120 '''

121 return self._H

122

123 @H.setter # PYCHOK setter!

124 def H(self, H):

125 '''Set the height prefix (C{str}).

126 '''

127 self._H = str(H) if H else NN

128

129 def hStr(self, prec=-2, m=NN):

130 '''Return a string for the height B{C{h}}.

131

132 @kwarg prec: Number of (decimal) digits, unstripped (C{int}).

133 @kwarg m: Optional unit of the height (C{str}).

134

135 @see: Function L{pygeodesy.hstr}.

136 '''

137 return NN(self.H, hstr(self.h, prec=prec, m=m))

138

139 @Property_RO

140 def isEllipsoidal(self):

141 '''Check whether this n-vector is ellipsoidal (C{bool} or C{None} if unknown).

142 '''

143 return self.datum.isEllipsoidal if self.datum else None

144

145 @Property_RO

146 def isSpherical(self):

147 '''Check whether this n-vector is spherical (C{bool} or C{None} if unknown).

148 '''

149 return self.datum.isSpherical if self.datum else None

150

151 @Property_RO

152 def lam(self):

153 '''Get the (geodetic) longitude in C{radians} (C{float}).

154 '''

155 return self.philam.lam

156

157 @Property_RO

158 def lat(self):

159 '''Get the (geodetic) latitude in C{degrees} (C{float}).

160 '''

161 return self.latlon.lat

162

163 @Property_RO

164 def latlon(self):

165 '''Get the (geodetic) lat-, longitude in C{degrees} (L{LatLon2Tuple}C{(lat, lon)}).

166 '''

167 return n_xyz2latlon(self.x, self.y, self.z, name=self.name)

168

169 @Property_RO

170 def latlonheight(self):

171 '''Get the (geodetic) lat-, longitude in C{degrees} and height (L{LatLon3Tuple}C{(lat, lon, height)}).

172 '''

173 return self.latlon.to3Tuple(self.h)

174

175 @Property_RO

176 def latlonheightdatum(self):

177 '''Get the lat-, longitude in C{degrees} with height and datum (L{LatLon4Tuple}C{(lat, lon, height, datum)}).

178 '''

179 return self.latlonheight.to4Tuple(self.datum)

180

181 @Property_RO

182 def lon(self):

183 '''Get the (geodetic) longitude in C{degrees} (C{float}).

184 '''

185 return self.latlon.lon

186

187 @Property_RO

188 def phi(self):

189 '''Get the (geodetic) latitude in C{radians} (C{float}).

190 '''

191 return self.philam.phi

192

193 @Property_RO

194 def philam(self):

195 '''Get the (geodetic) lat-, longitude in C{radians} (L{PhiLam2Tuple}C{(phi, lam)}).

196 '''

197 return n_xyz2philam(self.x, self.y, self.z, name=self.name)

198

199 @Property_RO

200 def philamheight(self):

201 '''Get the (geodetic) lat-, longitude in C{radians} and height (L{PhiLam3Tuple}C{(phi, lam, height)}).

202 '''

203 return self.philam.to3Tuple(self.h)

204

205 @Property_RO

206 def philamheightdatum(self):

207 '''Get the lat-, longitude in C{radians} with height and datum (L{PhiLam4Tuple}C{(phi, lam, height, datum)}).

208 '''

209 return self.philamheight.to4Tuple(self.datum)

210

211 @property_RO

212 def sphericalNvector(self):

213 '''Get the C{Nvector type} iff spherical, overloaded in L{pygeodesy.sphericalNvector.Nvector}.

214 '''

215 return False

216

217 @deprecated_method

218 def to2ab(self): # PYCHOK no cover

219 '''DEPRECATED, use property L{philam}.

220

221 @return: A L{PhiLam2Tuple}C{(phi, lam)}.

222 '''

223 return self.philam

224

225 @deprecated_method

226 def to3abh(self, height=None): # PYCHOK no cover

227 '''DEPRECATED, use property L{philamheight} or C{philam.to3Tuple(B{height})}.

228

229 @kwarg height: Optional height, overriding this

230 n-vector's height (C{meter}).

231

232 @return: A L{PhiLam3Tuple}C{(phi, lam, height)}.

233

234 @raise ValueError: Invalid B{C{height}}.

235 '''

236 return self.philamheight if height in (None, self.h) else \

237 self.philam.to3Tuple(height)

238

239 def toCartesian(self, h=None, Cartesian=None, datum=None, **Cartesian_kwds):

240 '''Convert this n-vector to C{Nvector}-based cartesian (ECEF) coordinates.

241

242 @kwarg h: Optional height, overriding this n-vector's height (C{meter}).

243 @kwarg Cartesian: Optional class to return the (ECEF) coordinates

244 (C{Cartesian}).

245 @kwarg datum: Optional datum (C{Datum}), overriding this datum.

246 @kwarg Cartesian_kwds: Optional, additional B{C{Cartesian}} keyword

247 arguments, ignored if C{B{Cartesian} is None}.

248

249 @return: The cartesian (ECEF) coordinates (B{C{Cartesian}}) or

250 if C{B{Cartesian} is None}, an L{Ecef9Tuple}C{(x, y, z,

251 lat, lon, height, C, M, datum)} with C{C} and C{M} if

252 available.

253

254 @raise TypeError: Invalid B{C{Cartesian}} or B{C{Cartesian_kwds}}

255 argument.

256

257 @raise ValueError: Invalid B{C{h}}.

258 '''

259 D = _spherical_datum(datum or self.datum, name=self.name)

260 E = D.ellipsoid

261 h = self.h if h is None else Height(h)

262

263 x, y, z = self.x, self.y, self.z

264 # Kenneth Gade eqn 22

265 n = E.b / hypot_(x * E.a_b, y * E.a_b, z)

266 r = h + n * E.a2_b2

267

268 x *= r

269 y *= r

270 z *= h + n

271

272 if Cartesian is None:

273 r = self.Ecef(D).reverse(x, y, z, M=True)

274 else:

275 kwds = _xkwds(Cartesian_kwds, datum=D) # h=0

276 r = Cartesian(x, y, z, **kwds)

277 return self._xnamed(r)

278

279 @deprecated_method

280 def to2ll(self): # PYCHOK no cover

281 '''DEPRECATED, use property L{latlon}.

282

283 @return: A L{LatLon2Tuple}C{(lat, lon)}.

284 '''

285 return self.latlon

286

287 @deprecated_method

288 def to3llh(self, height=None): # PYCHOK no cover

289 '''DEPRECATED, use property C{latlonheight} or C{latlon.to3Tuple(B{height})}.

290

291 @kwarg height: Optional height, overriding this

292 n-vector's height (C{meter}).

293

294 @return: A L{LatLon3Tuple}C{(lat, lon, height)}.

295

296 @raise ValueError: Invalid B{C{height}}.

297 '''

298 return self.latlonheight if height in (None, self.h) else \

299 self.latlon.to3Tuple(height)

300

301 def toLatLon(self, height=None, LatLon=None, datum=None, **LatLon_kwds):

302 '''Convert this n-vector to an C{Nvector}-based geodetic point.

303

304 @kwarg height: Optional height, overriding this n-vector's

305 height (C{meter}).

306 @kwarg LatLon: Optional class to return the geodetic point

307 (C{LatLon}) or C{None}.

308 @kwarg datum: Optional, spherical datum (C{Datum}).

309 @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword

310 arguments, ignored if C{B{LatLon} is None}.

311

312 @return: The geodetic point (C{LatLon}) or if C{B{LatLon} is None},

313 an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M,

314 datum)} with C{C} and C{M} if available.

315

316 @raise TypeError: Invalid B{C{LatLon}} or B{C{LatLon_kwds}}

317 argument.

318

319 @raise ValueError: Invalid B{C{height}}.

320 '''

321 d = _spherical_datum(datum or self.datum, name=self.name)

322 h = self.h if height is None else Height(height)

323 # use self.Cartesian(Cartesian=None) for better accuracy of the height

324 # than self.Ecef(d).forward(self.lat, self.lon, height=h, M=True)

325 if LatLon is None:

326 r = self.toCartesian(h=h, Cartesian=None, datum=d)

327 else:

328 kwds = _xkwds(LatLon_kwds, height=h, datum=d)

329 r = self._xnamed(LatLon(self.lat, self.lon, **kwds))

330 return r

331

332 def toStr(self, prec=5, fmt=Fmt.PAREN, sep=_COMMASPACE_): # PYCHOK expected

333 '''Return a string representation of this n-vector.

334

335 Height component is only included if non-zero.

336

337 @kwarg prec: Number of (decimal) digits, unstripped (C{int}).

338 @kwarg fmt: Enclosing backets format (C{str}).

339 @kwarg sep: Optional separator between components (C{str}).

340

341 @return: Comma-separated C{"(x, y, z [, h])"} enclosed in

342 B{C{fmt}} brackets (C{str}).

343 '''

344 t = Vector3d.toStr(self, prec=prec, fmt=NN, sep=sep)

345 if self.h:

346 t = sep.join((t, self.hStr()))

347 return (fmt % (t,)) if fmt else t

348

349 def toVector3d(self, norm=True):

350 '''Convert this n-vector to a 3-D vector, I{ignoring height}.

351

352 @kwarg norm: Normalize the 3-D vector (C{bool}).

353

354 @return: The (normalized) vector (L{Vector3d}).

355 '''

356 v = Vector3d.unit(self) if norm else self

357 return Vector3d(v.x, v.y, v.z, name=self.name)

358

359 @deprecated_method

360 def to4xyzh(self, h=None): # PYCHOK no cover

361 '''DEPRECATED, use property L{xyzh} or C{xyz.to4Tuple(B{h})}.'''

362 return self.xyzh if h in (None, self.h) else Vector4Tuple(

363 self.x, self.y, self.z, h, name=self.name)

364

365 def unit(self, ll=None):

366 '''Normalize this n-vector to unit length.

367

368 @kwarg ll: Optional, original latlon (C{LatLon}).

369

370 @return: Normalized vector (C{Nvector}).

371 '''

372 return _xattrs(Vector3d.unit(self, ll=ll), _under(_h_))

373

374 @Property_RO

375 def xyzh(self):

376 '''Get this n-vector's components (L{Vector4Tuple}C{(x, y, z, h)})

377 '''

378 return self.xyz.to4Tuple(self.h)

379

380

381 NorthPole = NvectorBase(0, 0, +1, name=_NorthPole_) # North pole (C{Nvector})

382 SouthPole = NvectorBase(0, 0, -1, name=_SouthPole_) # South pole (C{Nvector})

383

384

385 class _N_vector_(NvectorBase):

386 '''(INTERNAL) Minimal, low-overhead C{n-vector}.

387 '''

388 def __init__(self, x, y, z, h=0, **name):

389 self._x, self._y, self._z = x, y, z

390 if h:

391 self._h = h

392 if name:

393 self.name = name

394

395

396 class LatLonNvectorBase(LatLonBase):

397 '''(INTERNAL) Base class for n-vector-based ellipsoidal and

398 spherical C{LatLon} classes.

399 '''

400

401 def _update(self, updated, *attrs, **setters): # PYCHOK _Nv=None

402 '''(INTERNAL) Zap cached attributes if updated.

403

404 @see: C{ellipsoidalNvector.LatLon} and C{sphericalNvector.LatLon}

405 for the special case of B{C{_Nv}}.

406 '''

407 if updated:

408 _Nv, setters = _xkwds_pop2(setters, _Nv=None)

409 if _Nv is not None:

410 if _Nv._fromll is not None:

411 _Nv._fromll = None

412 self._Nv = None

413 LatLonBase._update(self, updated, *attrs, **setters)

414

415# def distanceTo(self, other, **kwds): # PYCHOK no cover

416# '''I{Must be overloaded}.'''

417# self._notOverloaded(other, **kwds)

418

419 def intersections2(self, radius1, other, radius2, **kwds): # PYCHOK expected

420 '''B{Not implemented}, throws a C{NotImplementedError} always.'''

421 self._notImplemented(radius1, other, radius2, **kwds)

422

423 def others(self, *other, **name_other_up):

424 '''Refined class comparison.

425

426 @arg other: The other instance (C{LatLonNvectorBase}).

427 @kwarg name_other_up: Overriding C{name=other} and C{up=1}

428 keyword arguments.

429

430 @return: The B{C{other}} if compatible.

431

432 @raise TypeError: Incompatible B{C{other}} C{type}.

433 '''

434 if other:

435 other0 = other[0]

436 if isinstance(other0, (self.__class__, LatLonNvectorBase)): # XXX NvectorBase?

437 return other0

438

439 other, name, up = _xother3(self, other, **name_other_up)

440 if not isinstance(other, (self.__class__, LatLonNvectorBase)): # XXX NvectorBase?

441 LatLonBase.others(self, other, name=name, up=up + 1)

442 return other

443

444 def toNvector(self, **Nvector_and_kwds): # PYCHOK signature

445 '''Convert this point to C{Nvector} components, I{including height}.

446

447 @kwarg Nvector_and_kwds: Optional C{Nvector} class and C{Nvector} keyword arguments,

448 Specify C{B{Nvector}=...} to override this C{Nvector} class

449 or use C{B{Nvector}=None}.

450

451 @return: An C{Nvector} or if C{Nvector is None}, a L{Vector4Tuple}C{(x, y, z, h)}.

452

453 @raise TypeError: Invalid C{Nvector} or other B{C{Nvector_and_kwds}} item.

454 '''

455 return LatLonBase.toNvector(self, **_xkwds(Nvector_and_kwds, Nvector=NvectorBase))

456

457 def triangulate(self, bearing1, other, bearing2, height=None, wrap=False): # PYCHOK signature

458 '''Locate a point given this, an other point and the (initial) bearing

459 from this and the other point.

460

461 @arg bearing1: Bearing at this point (compass C{degrees360}).

462 @arg other: The other point (C{LatLon}).

463 @arg bearing2: Bearing at the other point (compass C{degrees360}).

464 @kwarg height: Optional height at the triangulated point, overriding

465 the mean height (C{meter}).

466 @kwarg wrap: If C{True}, use this and the B{C{other}} point

467 I{normalized} (C{bool}).

468

469 @return: Triangulated point (C{LatLon}).

470

471 @raise TypeError: Invalid B{C{other}} point.

472

473 @raise Valuerror: Points coincide.

474 '''

475 return _triangulate(self, bearing1, self.others(other), bearing2,

476 height=height, wrap=wrap, LatLon=self.classof)

477

478 def trilaterate(self, distance1, point2, distance2, point3, distance3,

479 radius=R_M, height=None, useZ=False, wrap=False):

480 '''Locate a point at given distances from this and two other points.

481

482 @arg distance1: Distance to this point (C{meter}, same units

483 as B{C{radius}}).

484 @arg point2: Second reference point (C{LatLon}).

485 @arg distance2: Distance to point2 (C{meter}, same units as

486 B{C{radius}}).

487 @arg point3: Third reference point (C{LatLon}).

488 @arg distance3: Distance to point3 (C{meter}, same units as

489 B{C{radius}}).

490 @kwarg radius: Mean earth radius (C{meter}).

491 @kwarg height: Optional height at trilaterated point, overriding

492 the mean height (C{meter}, same units as B{C{radius}}).

493 @kwarg useZ: Include Z component iff non-NaN, non-zero (C{bool}).

494 @kwarg wrap: If C{True}, use this, B{C{point2}} and B{C{point3}}

495 I{normalized} (C{bool}).

496

497 @return: Trilaterated point (C{LatLon}).

498

499 @raise IntersectionError: No intersection, trilateration failed.

500

501 @raise TypeError: Invalid B{C{point2}} or B{C{point3}}.

502

503 @raise ValueError: Some B{C{points}} coincide or invalid B{C{distance1}},

504 B{C{distance2}}, B{C{distance3}} or B{C{radius}}.

505

506 @see: U{Trilateration<https://WikiPedia.org/wiki/Trilateration>},

507 Veness' JavaScript U{Trilateration<https://www.Movable-Type.co.UK/

508 scripts/latlong-vectors.html>} and method C{LatLon.trilaterate5}

509 of other, non-C{Nvector LatLon} classes.

510 '''

511 return _trilaterate(self, distance1, self.others(point2=point2), distance2,

512 self.others(point3=point3), distance3,

513 radius=radius, height=height, useZ=useZ,

514 wrap=wrap, LatLon=self.classof)

515

516 def trilaterate5(self, distance1, point2, distance2, point3, distance3, # PYCHOK signature

517 area=False, eps=EPS1, radius=R_M, wrap=False):

518 '''B{Not implemented} for C{B{area}=True} and falls back to method

519 C{trilaterate} otherwise.

520

521 @return: A L{Trilaterate5Tuple}C{(min, minPoint, max, maxPoint, n)}

522 with a single trilaterated intersection C{minPoint I{is}

523 maxPoint}, C{min I{is} max} the nearest intersection

524 margin and count C{n = 1}.

525

526 @raise NotImplementedError: Keyword argument C{B{area}=True} not

527 (yet) supported.

528

529 @see: Method L{trilaterate} for other and more details.

530 '''

531 if area:

532 self._notImplemented(area=area)

533

534 t = _trilaterate(self, distance1, self.others(point2=point2), distance2,

535 self.others(point3=point3), distance3,

536 radius=radius, useZ=True, wrap=wrap,

537 LatLon=self.classof)

538 # ... and handle B{C{eps}} and C{IntersectionError}

539 # like function C{.latlonBase._trilaterate5}

540 d = self.distanceTo(t, radius=radius, wrap=wrap) # PYCHOK distanceTo

541 d = min(fabs(distance1 - d), fabs(distance2 - d), fabs(distance3 - d))

542 if d < eps: # min is max, minPoint is maxPoint

543 return Trilaterate5Tuple(d, t, d, t, 1) # n = 1

544 t = _SPACE_(_no_(_intersection_), Fmt.PAREN(min.__name__, Fmt.f(d, prec=3)))

545 raise IntersectionError(area=area, eps=eps, radius=radius, wrap=wrap, txt=t)

546

547

548 def _nsumOf(nvs, h_None, Vector, Vector_kwds): # .sphericalNvector, .vector3d

549 '''(INTERNAL) Separated to allow callers to embellish exceptions.

550 '''

551 X, Y, Z, n = Fsum(), Fsum(), Fsum(), 0

552 H = Fsum() if h_None is None else n

553 for n, v in enumerate(nvs or ()): # one pass

554 X += v.x

555 Y += v.y

556 Z += v.z

557 H += v.h

558 if n < 1:

559 raise ValueError(_SPACE_(Fmt.PARENSPACED(len=n), _insufficient_))

560

561 x, y, z = map1(float, X, Y, Z)

562 h = H.fover(n) if h_None is None else h_None

563 return Vector3Tuple(x, y, z).to4Tuple(h) if Vector is None else \

564 Vector(x, y, z, **_xkwds(Vector_kwds, h=h))

565

566

567 def sumOf(nvectors, Vector=None, h=None, **Vector_kwds):

568 '''Return the I{vectorial} sum of two or more n-vectors.

569

570 @arg nvectors: Vectors to be added (C{Nvector}[]).

571 @kwarg Vector: Optional class for the vectorial sum (C{Nvector})

572 or C{None}.

573 @kwarg h: Optional height, overriding the mean height (C{meter}).

574 @kwarg Vector_kwds: Optional, additional B{C{Vector}} keyword

575 arguments, ignored if C{B{Vector} is None}.

576

577 @return: Vectorial sum (B{C{Vector}}) or a L{Vector4Tuple}C{(x, y,

578 z, h)} if B{C{Vector}} is C{None}.

579

580 @raise VectorError: No B{C{nvectors}}.

581 '''

582 try:

583 return _nsumOf(nvectors, h, Vector, Vector_kwds)

584 except (TypeError, ValueError) as x:

585 raise VectorError(nvectors=nvectors, Vector=Vector, cause=x)

586

587

588 def _triangulate(point1, bearing1, point2, bearing2, height=None,

589 wrap=False, **LatLon_and_kwds):

590 # (INTERNAL) Locate a point given two known points and initial

591 # bearings from those points, see C{LatLon.triangulate} above

592

593 def _gc(p, b, _i_):

594 n = p.toNvector()

595 de = NorthPole.cross(n, raiser=_pole_).unit() # east vector @ n

596 dn = n.cross(de) # north vector @ n

597 s, c = sincos2d(Bearing(b, name=_bearing_ + _i_))

598 dest = de.times(s)

599 dnct = dn.times(c)

600 d = dnct.plus(dest) # direction vector @ n

601 return n.cross(d) # great circle point + bearing

602

603 if wrap:

604 point2 = _unrollon(point1, point2, wrap=wrap)

605 if _isequalTo(point1, point2, eps=EPS):

606 raise _ValueError(points=point2, wrap=wrap, txt=_coincident_)

607

608 gc1 = _gc(point1, bearing1, _1_) # great circle p1 + b1

609 gc2 = _gc(point2, bearing2, _2_) # great circle p2 + b2

610

611 n = gc1.cross(gc2, raiser=_point_) # n-vector of intersection point

612 h = point1._havg(point2, h=height)

613 kwds = _xkwds(LatLon_and_kwds, height=h)

614 return n.toLatLon(**kwds) # Nvector(n.x, n.y, n.z).toLatLon(...)

615

616

617 def _trilaterate(point1, distance1, point2, distance2, point3, distance3,

618 radius=R_M, height=None, useZ=False,

619 wrap=False, **LatLon_and_kwds):

620 # (INTERNAL) Locate a point at given distances from

621 # three other points, see LatLon.triangulate above

622

623 def _nr2(p, d, r, _i_, *qs): # .toNvector and angular distance squared

624 for q in qs:

625 if _isequalTo(p, q, eps=EPS):

626 raise _ValueError(points=p, txt=_coincident_)

627 return p.toNvector(), (Scalar(d, name=_distance_ + _i_) / r)**2

628

629 p1, r = point1, Radius_(radius)

630 p2, p3, _ = _unrollon3(p1, point2, point3, wrap)

631

632 n1, r12 = _nr2(p1, distance1, r, _1_)

633 n2, r22 = _nr2(p2, distance2, r, _2_, p1)

634 n3, r32 = _nr2(p3, distance3, r, _3_, p1, p2)

635

636 # the following uses x,y coordinate system with origin at n1, x axis n1->n2

637 y = n3.minus(n1)

638 x = n2.minus(n1)

639 z = None

640

641 d = x.length # distance n1->n2

642 if d > EPS_2: # and y.length > EPS_2:

643 X = x.unit() # unit vector in x direction n1->n2

644 i = X.dot(y) # signed magnitude of x component of n1->n3

645 Y = y.minus(X.times(i)).unit() # unit vector in y direction

646 j = Y.dot(y) # signed magnitude of y component of n1->n3

647 if fabs(j) > EPS_2:

648 # courtesy of U{Carlos Freitas<https://GitHub.com/mrJean1/PyGeodesy/issues/33>}

649 x = fsumf_(r12, -r22, d**2) / (d * _2_0) # n1->intersection x- and ...

650 y = fsumf_(r12, -r32, i**2, j**2, x * i * _N_2_0) / (j * _2_0) # ... y-component

651 # courtesy of U{AleixDev<https://GitHub.com/mrJean1/PyGeodesy/issues/43>}

652 z = fsumf_(max(r12, r22, r32), -(x**2), -(y**2)) # XXX not just r12!

653 if z > EPS:

654 n = n1.plus(X.times(x)).plus(Y.times(y))

655 if useZ: # include Z component

656 Z = X.cross(Y) # unit vector perpendicular to plane

657 n = n.plus(Z.times(sqrt(z)))

658 if height is None:

659 h = fidw((point1.height, point2.height, point3.height),

660 map1(fabs, distance1, distance2, distance3))

661 else:

662 h = Height(height)

663 kwds = _xkwds(LatLon_and_kwds, height=h)

664 return n.toLatLon(**kwds) # Nvector(n.x, n.y, n.z).toLatLon(...)

665

666 # no intersection, d < EPS_2 or fabs(j) < EPS_2 or z < EPS

667 t = _SPACE_(_no_, _intersection_, NN)

668 raise IntersectionError(point1=point1, distance1=distance1,

669 point2=point2, distance2=distance2,

670 point3=point3, distance3=distance3,

671 txt=unstr(t, z=z, useZ=useZ, wrap=wrap))

672

673

674__all__ += _ALL_DOCS(LatLonNvectorBase, NvectorBase, sumOf) # classes

675

676# **) MIT License

677#

678# Copyright (C) 2016-2024 -- mrJean1 at Gmail -- All Rights Reserved.

679#

680# Permission is hereby granted, free of charge, to any person obtaining a

681# copy of this software and associated documentation files (the "Software"),

682# to deal in the Software without restriction, including without limitation

683# the rights to use, copy, modify, merge, publish, distribute, sublicense,

684# and/or sell copies of the Software, and to permit persons to whom the

685# Software is furnished to do so, subject to the following conditions:

686#

687# The above copyright notice and this permission notice shall be included

688# in all copies or substantial portions of the Software.

689#

690# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

691# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

692# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

693# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

694# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

695# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

696# OTHER DEALINGS IN THE SOFTWARE.